(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SLB9673AU20FW2610XTMA1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.8 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SLB9673AU20FW2610XTMA1"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SLB9673AU20FW2610XTMA1"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/196/Infineon_OPTIGA_TPM_SLB_9673_FW26_DataSheet_v01_30-3363760.pdf"
				(at 50.8 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Security ICs / Authentication ICs"
				(at 50.8 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SLB9673AU20FW2610XTMA1"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Infineon"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SLB9673AU20FW2610XTMA1_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "1")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "GPIO_00")
					(number "3")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "GPIO_01")
					(number "4")
				)
				(pin no_connect line
					(at 33.02 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "NCI")
					(number "5")
				)
				(pin no_connect line
					(at 33.02 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "GPIO_02")
					(number "7")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "NCI/VDD")
					(number "8")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "9")
				)
				(pin no_connect line
					(at 33.02 -27.94 180)
					(length 2.54)
					(hide yes)
					(name "NCI")
					(number "10")
				)
				(pin no_connect line
					(at 33.02 -30.48 180)
					(length 2.54)
					(hide yes)
					(name "NCI")
					(number "11")
				)
				(pin no_connect line
					(at 33.02 -35.56 180)
					(length 2.54)
					(hide yes)
					(name "NCI")
					(number "12")
				)
				(pin no_connect line
					(at 33.02 -38.1 180)
					(length 2.54)
					(hide yes)
					(name "NCI")
					(number "13")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "14")
				)
				(pin no_connect line
					(at 33.02 -40.64 180)
					(length 2.54)
					(hide yes)
					(name "NCI")
					(number "15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "NCI/GND")
					(number "16")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "RST#")
					(number "17")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "I2C_PIRQ#")
					(number "18")
				)
				(pin no_connect line
					(at 33.02 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "19")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "TEST#")
					(number "20")
				)
				(pin no_connect line
					(at 33.02 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "21")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "22")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "23")
				)
				(pin no_connect line
					(at 33.02 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "24")
				)
				(pin no_connect line
					(at 33.02 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "NCI")
					(number "25")
				)
				(pin no_connect line
					(at 33.02 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "NCI")
					(number "26")
				)
				(pin no_connect line
					(at 33.02 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "NCI")
					(number "27")
				)
				(pin no_connect line
					(at 33.02 -7.62 180)
					(length 2.54)
					(hide yes)
					(name "NCI")
					(number "28")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SDA")
					(number "29")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SCL")
					(number "30")
				)
				(pin no_connect line
					(at 33.02 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "NCI")
					(number "31")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "32")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "EP")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
