(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SM51625EL"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SM51625EL"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SM51625EL"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/54/sm51625el-934089.pdf"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Interface driver/receiver/transceiver"
				(at 50.8 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SM51625EL"
				(at 50.8 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Bourns"
				(at 48.26 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SM51625EL_1_1"
				(text ""
					(at 8.89 0.254 0)
				)
				(text ""
					(at 8.89 -9.906 0)
				)
				(text ""
					(at 8.89 -20.066 0)
				)
				(text ""
					(at 8.89 -30.48 0)
				)
				(text ""
					(at 10.16 -3.81 0)
				)
				(text ""
					(at 10.16 -5.08 0)
				)
				(text ""
					(at 10.16 -6.35 0)
				)
				(text ""
					(at 10.16 -8.89 0)
				)
				(text ""
					(at 10.16 -10.16 0)
				)
				(text ""
					(at 10.16 -11.43 0)
				)
				(text ""
					(at 10.16 -13.97 0)
				)
				(text ""
					(at 10.16 -15.24 0)
				)
				(text ""
					(at 10.16 -16.51 0)
				)
				(text ""
					(at 10.16 -20.32 0)
				)
				(text ""
					(at 10.16 -21.59 0)
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "TCT1")
					(number "1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "TD1+")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "TD1-")
					(number "3")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "TCT2")
					(number "4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "TD2+")
					(number "5")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TD2-")
					(number "6")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "TCT3")
					(number "7")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "TD3+")
					(number "8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "TD3-")
					(number "9")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "TCT4")
					(number "10")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "TD4+")
					(number "11")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "TD4-")
					(number "12")
				)
				(pin passive line
					(at 30.48 -35.56 180)
					(length 2.54)
					(name "MX4-")
					(number "13")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "MX4+")
					(number "14")
				)
				(pin passive line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "MCT4")
					(number "15")
				)
				(pin passive line
					(at 30.48 -25.4 180)
					(length 2.54)
					(name "MX3-")
					(number "16")
				)
				(pin passive line
					(at 30.48 -20.32 180)
					(length 2.54)
					(name "MX3+")
					(number "17")
				)
				(pin passive line
					(at 30.48 -22.86 180)
					(length 2.54)
					(name "MCT3")
					(number "18")
				)
				(pin passive line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "MX2-")
					(number "19")
				)
				(pin passive line
					(at 30.48 -10.16 180)
					(length 2.54)
					(name "MX2+")
					(number "20")
				)
				(pin passive line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "MCT2")
					(number "21")
				)
				(pin passive line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "MX1-")
					(number "22")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(name "MX1+")
					(number "23")
				)
				(pin passive line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "MCT1")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
)
