(footprint "MP_Terminal_M4_SMD_Horizontal_SMTRAM4-9-7ET"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Mounting Hardware, SMD M4")
	(property "Reference" "REF**"
		(at 0 -4.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "MP_Terminal_M4_SMD_Horizontal_SMTRAM4-9-7ET"
		(at -5.72 4.91 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_paste_margin_ratio -1)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -5.77 6.1 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.77 7.3 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5.77 8.5 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -3.95 0)
		(size 1.35 1.35)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.95 0)
		(size 1.35 1.35)
		(drill 1.35)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at 0 0)
		(size 10.65 6.57)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.025)
	)
	(embedded_fonts no)
	(model "antmicro_smtram4_9_7et.glb"
		(offset
			(xyz 0 -3.5 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
