(footprint "Spacer_Drill2.5mm_H1mm_SMTSO-M1.4-1ET"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Mounting Hardware, inside through hole M3, height 14mm")
	(property "Reference" "REF**"
		(at 0 -3.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Spacer_Drill2.5mm_H1mm_SMTSO-M1.4-1ET"
		(at 0 4.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_paste_margin_ratio -1)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -2.7 6.7 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -2.7 7.9 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.7 9.1 0)
		(layer "F.Fab")
	)
	(pad "1" smd oval
		(at -1.675 0)
		(size 0.8 1)
		(layers "F.Cu" "F.Paste")
	)
	(pad "1" smd oval
		(at -1.175 -1.175 135)
		(size 0.8 1)
		(layers "F.Cu" "F.Paste")
	)
	(pad "1" smd oval
		(at -1.175 1.175 45)
		(size 0.8 1)
		(layers "F.Cu" "F.Paste")
	)
	(pad "1" smd oval
		(at 0 -1.675 270)
		(size 0.8 1)
		(layers "F.Cu" "F.Paste")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 4.19 4.19)
		(drill 2.5)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "1" smd oval
		(at 0 1.675 90)
		(size 0.8 1)
		(layers "F.Cu" "F.Paste")
	)
	(pad "1" smd oval
		(at 1.175 -1.175 225)
		(size 0.8 1)
		(layers "F.Cu" "F.Paste")
	)
	(pad "1" smd oval
		(at 1.175 1.175 135)
		(size 0.8 1)
		(layers "F.Cu" "F.Paste")
	)
	(pad "1" smd oval
		(at 1.675 0)
		(size 0.8 1)
		(layers "F.Cu" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_smtso_m1_4_1et.glb"
		(offset
			(xyz 0 0 -0.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 -90 0)
		)
	)
)
