(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN55HVD233-SEP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN55HVD233-SEP"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN55HVD233-SEP"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn55hvd233-sep.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "3.3-V Radiation Hardened CAN Transceiver, 1 Mbps, SOIC-8"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN55HVD233MDPSEP"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, TRANSCEIVER, CAN, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN55HVD233-SEP_1_1"
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "D")
					(number "1")
				)
				(pin power_in line
					(at 17.78 -12.7 180)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "3")
				)
				(pin output line
					(at 0 -6.35 0)
					(length 2.54)
					(name "R")
					(number "4")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "LBK")
					(number "5")
				)
				(pin bidirectional line
					(at 17.78 -6.35 180)
					(length 2.54)
					(name "CAN_L")
					(number "6")
				)
				(pin bidirectional line
					(at 17.78 -3.81 180)
					(length 2.54)
					(name "CAN_H")
					(number "7")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "RS")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
