(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN55LVTA4-SEP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN55LVTA4-SEP"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN55LVTA4-SEP"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn55lvta4-sep.pdf?ts=1757905579930&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FSN55LVTA4-SEP"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Radiation Tolerant Quad Channel LVDS High-Speed Differential Line Driver"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN55LVTA4MDTSEP"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, TRANSCEIVER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN55LVTA4-SEP_1_1"
				(pin passive line
					(at 0 -6.35 0)
					(length 2.54)
					(name "1A")
					(number "1")
				)
				(pin passive line
					(at 20.32 -6.35 180)
					(length 2.54)
					(name "1Y")
					(number "2")
				)
				(pin passive line
					(at 20.32 -8.89 180)
					(length 2.54)
					(name "1Z")
					(number "3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "G")
					(number "4")
				)
				(pin passive line
					(at 20.32 -16.51 180)
					(length 2.54)
					(name "2Z")
					(number "5")
				)
				(pin passive line
					(at 20.32 -13.97 180)
					(length 2.54)
					(name "2Y")
					(number "6")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 2.54)
					(name "2A")
					(number "7")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 2.54)
					(name "3A")
					(number "9")
				)
				(pin passive line
					(at 20.32 -21.59 180)
					(length 2.54)
					(name "3Y")
					(number "10")
				)
				(pin passive line
					(at 20.32 -24.13 180)
					(length 2.54)
					(name "3Z")
					(number "11")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "~{G}")
					(number "12")
				)
				(pin passive line
					(at 20.32 -31.75 180)
					(length 2.54)
					(name "4Z")
					(number "13")
				)
				(pin passive line
					(at 20.32 -29.21 180)
					(length 2.54)
					(name "4Y")
					(number "14")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 2.54)
					(name "4A")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
