(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN65DP159RGZR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.8 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN65DP159RGZR"
				(at 50.8 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN65DP159RGZR"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn75dp159.pdf?ts=1728245191743&ref_url=https%253A%252F%252Fwww.mouser.de%252F"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Display Interface, Level Shifter Retimer, DVI, HDMI, I2C, 6 Gbps"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN65DP159RGZR "
				(at 50.8 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, IC, HDMI"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN65DP159RGZR_1_1"
				(pin input line
					(at 0 -49.53 0)
					(length 2.54)
					(name "SWAP/POL")
					(number "1")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "IN_D2_P")
					(number "2")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "IN_D2_N")
					(number "3")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 2.54)
					(name "HPD_SRC")
					(number "4")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "IN_D1_P")
					(number "5")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "IN_D1_N")
					(number "6")
				)
				(pin power_in line
					(at 0 -74.93 0)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "IN_D0_P")
					(number "8")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "IN_D0_N")
					(number "9")
				)
				(pin input line
					(at 0 -52.07 0)
					(length 2.54)
					(name "I2C_EN/PIN")
					(number "10")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "IN_CLK_P")
					(number "11")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "IN_CLK_N")
					(number "12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "13")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 2.54)
					(name "SDA_CTL")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 2.54)
					(name "SCL_CTL")
					(number "16")
				)
				(pin no_connect line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "NC")
					(number "17")
				)
				(pin output line
					(at 27.94 -36.83 180)
					(length 2.54)
					(name "CEC_EN")
					(number "18")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 2.54)
					(name "GND")
					(number "19")
				)
				(pin input line
					(at 0 -54.61 0)
					(length 2.54)
					(name "PRE_SEL")
					(number "20")
				)
				(pin input line
					(at 0 -57.15 0)
					(length 2.54)
					(name "EQ_SEL/A0")
					(number "21")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 2.54)
					(name "VSADJ")
					(number "22")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "23")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "24")
				)
				(pin output line
					(at 27.94 -24.13 180)
					(length 2.54)
					(name "OUT_CLK_N")
					(number "25")
				)
				(pin output line
					(at 27.94 -21.59 180)
					(length 2.54)
					(name "OUT_CLK_P")
					(number "26")
				)
				(pin input line
					(at 0 -59.69 0)
					(length 2.54)
					(name "~{HDMI_SEL}/A1")
					(number "27")
				)
				(pin output line
					(at 27.94 -8.89 180)
					(length 2.54)
					(name "OUT_D0_N")
					(number "28")
				)
				(pin output line
					(at 27.94 -6.35 180)
					(length 2.54)
					(name "OUT_D0_P")
					(number "29")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 2.54)
					(name "GND")
					(number "30")
				)
				(pin output line
					(at 27.94 -13.97 180)
					(length 2.54)
					(name "OUT_D1_N")
					(number "31")
				)
				(pin output line
					(at 27.94 -11.43 180)
					(length 2.54)
					(name "OUT_D1_P")
					(number "32")
				)
				(pin input line
					(at 27.94 -27.94 180)
					(length 2.54)
					(name "HPD_SNK")
					(number "33")
				)
				(pin output line
					(at 27.94 -19.05 180)
					(length 2.54)
					(name "OUT_D2_N")
					(number "34")
				)
				(pin output line
					(at 27.94 -16.51 180)
					(length 2.54)
					(name "OUT_D2_P")
					(number "35")
				)
				(pin input line
					(at 0 -62.23 0)
					(length 2.54)
					(name "TX_TERM_CTL")
					(number "36")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "37")
				)
				(pin bidirectional line
					(at 27.94 -33.02 180)
					(length 2.54)
					(name "SCL_SNK")
					(number "38")
				)
				(pin bidirectional line
					(at 27.94 -30.48 180)
					(length 2.54)
					(name "SDA_SNK")
					(number "39")
				)
				(pin input line
					(at 0 -64.77 0)
					(length 2.54)
					(name "SLEW_CTL")
					(number "40")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 2.54)
					(name "GND")
					(number "41")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 2.54)
					(name "OE")
					(number "42")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "43")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "AUX_SRC_N")
					(number "44")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "AUX_SRC_P")
					(number "45")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "SCL_SRC")
					(number "46")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "SDA_SRC")
					(number "47")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "48")
				)
				(pin passive line
					(at 0 -74.93 0)
					(length 2.54)
					(name "GND")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
