(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN65DSI84"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN65DSI84"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN65DSI84"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn65dsi84-q1.pdf?ts=1705413548625&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FSN65DSI84-Q1"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Automotive Single-Channel MIPI® DSI to Dual-Link LVDS Bridge"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN65DSI84TPAPRQ1"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, CONTROLLER, DSI, LVDS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "NFBGA64_ZXH_TEX NFBGA64_ZXH_TEX-M NFBGA64_ZXH_TEX-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN65DSI84_1_1"
				(pin no_connect line
					(at 2.54 -58.42 0)
					(length 2.54)
					(hide yes)
					(name "RSVD2")
					(number "1")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 2.54)
					(name "EN")
					(number "2")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "3")
				)
				(pin no_connect line
					(at 2.54 -59.69 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin no_connect line
					(at 2.54 -60.96 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin no_connect line
					(at 2.54 -62.23 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin no_connect line
					(at 2.54 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin no_connect line
					(at 2.54 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "8")
				)
				(pin no_connect line
					(at 2.54 -6.35 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "9")
				)
				(pin no_connect line
					(at 2.54 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "10")
				)
				(pin no_connect line
					(at 2.54 -53.34 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "11")
				)
				(pin no_connect line
					(at 2.54 -54.61 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "12")
				)
				(pin no_connect line
					(at 2.54 -55.88 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "14")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "SCL")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "SDA")
					(number "16")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 2.54)
					(name "REFCLK")
					(number "17")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "18")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "DA0P")
					(number "19")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "DA0N")
					(number "20")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "DA1P")
					(number "21")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "DA1N")
					(number "22")
				)
				(pin power_out line
					(at 0 -71.12 0)
					(length 2.54)
					(name "GND")
					(number "23")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "DACP")
					(number "24")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "DACN")
					(number "25")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "26")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 2.54)
					(name "DA2P")
					(number "27")
				)
				(pin input line
					(at 0 -29.21 0)
					(length 2.54)
					(name "DA2N")
					(number "28")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 2.54)
					(name "DA3P")
					(number "29")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 2.54)
					(name "DA3N")
					(number "30")
				)
				(pin power_out line
					(at 0 -64.77 0)
					(length 2.54)
					(name "VCORE")
					(number "31")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "32")
				)
				(pin output line
					(at 0 -48.26 0)
					(length 2.54)
					(name "IRQ")
					(number "33")
				)
				(pin no_connect line
					(at 2.54 -57.15 0)
					(length 2.54)
					(hide yes)
					(name "RSVD1")
					(number "34")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "35")
				)
				(pin output line
					(at 30.48 -22.86 180)
					(length 2.54)
					(name "A_Y3P")
					(number "36")
				)
				(pin output line
					(at 30.48 -25.4 180)
					(length 2.54)
					(name "A_Y3N")
					(number "37")
				)
				(pin output line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "A_CLKP")
					(number "38")
				)
				(pin output line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "A_CLKN")
					(number "39")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "40")
				)
				(pin output line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "A_Y2P")
					(number "41")
				)
				(pin output line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "A_Y2N")
					(number "42")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "43")
				)
				(pin output line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "A_Y1P")
					(number "44")
				)
				(pin output line
					(at 30.48 -10.16 180)
					(length 2.54)
					(name "A_Y1N")
					(number "45")
				)
				(pin output line
					(at 30.48 0 180)
					(length 2.54)
					(name "A_Y0P")
					(number "46")
				)
				(pin output line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "A_Y0N")
					(number "47")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "48")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "49")
				)
				(pin output line
					(at 30.48 -63.5 180)
					(length 2.54)
					(name "B_Y3P")
					(number "50")
				)
				(pin output line
					(at 30.48 -60.96 180)
					(length 2.54)
					(name "B_Y3N")
					(number "51")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "52")
				)
				(pin output line
					(at 30.48 -71.12 180)
					(length 2.54)
					(name "B_CLKP")
					(number "53")
				)
				(pin output line
					(at 30.48 -68.58 180)
					(length 2.54)
					(name "B_CLKN")
					(number "54")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "55")
				)
				(pin output line
					(at 30.48 -53.34 180)
					(length 2.54)
					(name "B_Y2P")
					(number "56")
				)
				(pin output line
					(at 30.48 -55.88 180)
					(length 2.54)
					(name "B_Y2N")
					(number "57")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "58")
				)
				(pin output line
					(at 30.48 -45.72 180)
					(length 2.54)
					(name "B_Y1P")
					(number "59")
				)
				(pin output line
					(at 30.48 -48.26 180)
					(length 2.54)
					(name "B_Y1N")
					(number "60")
				)
				(pin output line
					(at 30.48 -38.1 180)
					(length 2.54)
					(name "B_Y0P")
					(number "61")
				)
				(pin output line
					(at 30.48 -40.64 180)
					(length 2.54)
					(name "B_Y0N")
					(number "62")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "63")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "ADDR")
					(number "64")
				)
				(pin power_in line
					(at 0 -68.58 0)
					(length 2.54)
					(name "PAD")
					(number "65")
				)
			)
			(embedded_fonts no)
		)
)
