(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN74AC7541_VQFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN74AC7541_VQFN"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN74AC7541_VQFN"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74ac7541.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Octal buffer with open-drain outputs"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN74AC7541RKSR"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, BUFFER, TRANSCEIVER, DRIVER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN74AC7541_VQFN_1_1"
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "~{OE1}")
					(number "1")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "A1")
					(number "2")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "A2")
					(number "3")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "A3")
					(number "4")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "A4")
					(number "5")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "A5")
					(number "6")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "A6")
					(number "7")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "A7")
					(number "8")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "A8")
					(number "9")
				)
				(pin power_in line
					(at 17.78 -27.94 180)
					(length 2.54)
					(name "GND")
					(number "10")
				)
				(pin open_collector line
					(at 17.78 -21.59 180)
					(length 2.54)
					(name "Y8")
					(number "11")
				)
				(pin open_collector line
					(at 17.78 -19.05 180)
					(length 2.54)
					(name "Y7")
					(number "12")
				)
				(pin open_collector line
					(at 17.78 -16.51 180)
					(length 2.54)
					(name "Y6")
					(number "13")
				)
				(pin open_collector line
					(at 17.78 -13.97 180)
					(length 2.54)
					(name "Y5")
					(number "14")
				)
				(pin open_collector line
					(at 17.78 -11.43 180)
					(length 2.54)
					(name "Y4")
					(number "15")
				)
				(pin open_collector line
					(at 17.78 -8.89 180)
					(length 2.54)
					(name "Y3")
					(number "16")
				)
				(pin open_collector line
					(at 17.78 -6.35 180)
					(length 2.54)
					(name "Y2")
					(number "17")
				)
				(pin open_collector line
					(at 17.78 -3.81 180)
					(length 2.54)
					(name "Y1")
					(number "18")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "~{OE2}")
					(number "19")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{CC}")
					(number "20")
				)
				(pin passive line
					(at 17.78 -27.94 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
