(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN74AHC14Q"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN74AHC14Q"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN74AHC14Q"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74ahc14q-q1.pdf?ts=1717720237884"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Automotive 6-ch, 2-V to 5.5-V inverters with Schmitt-Trigger inputs"
				(at 27.94 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN74AHC14Q-Q1"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, INVERTER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN74AHC14Q_0_1")
			(symbol "SN74AHC14Q_1_1"
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "1A")
					(number "1")
				)
				(pin output line
					(at 19.05 -2.54 180)
					(length 2.54)
					(name "1Y")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "2A")
					(number "3")
				)
				(pin output line
					(at 19.05 -5.08 180)
					(length 2.54)
					(name "2Y")
					(number "4")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "3A")
					(number "5")
				)
				(pin output line
					(at 19.05 -7.62 180)
					(length 2.54)
					(name "3Y")
					(number "6")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin output line
					(at 19.05 -10.16 180)
					(length 2.54)
					(name "4Y")
					(number "8")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "4A")
					(number "9")
				)
				(pin output line
					(at 19.05 -12.7 180)
					(length 2.54)
					(name "5Y")
					(number "10")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "5A")
					(number "11")
				)
				(pin output line
					(at 19.05 -15.24 180)
					(length 2.54)
					(name "6Y")
					(number "12")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "6A")
					(number "13")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{CC}")
					(number "14")
				)
			)
			(embedded_fonts no)
		)
)
