(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN74AVC2T245_UQFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN74AVC2T245_UQFN"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN74AVC2T245_UQFN"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74avc2t245.pdf?ts=1678888074783&ref_url=https%253A%252F%252Fwww.google.com%252F"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Transceiver Non Inverting, AVC Family, 2 Input, 12 mA, 2.4 ns, 1.2 V to 3.6 V, LFCSP-10"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN74AVC2T245RSWR"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, LEVEL-SHIFTER, VOLTAGE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN74AVC2T245_UQFN_1_1"
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "DIR_{2}")
					(number "1")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "~{OE}")
					(number "2")
				)
				(pin power_in line
					(at 17.78 -13.97 180)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin bidirectional line
					(at 17.78 -6.35 180)
					(length 2.54)
					(name "B_{2}")
					(number "4")
				)
				(pin bidirectional line
					(at 17.78 -3.81 180)
					(length 2.54)
					(name "B_{1}")
					(number "5")
				)
				(pin power_in line
					(at 17.78 0 180)
					(length 2.54)
					(name "V_{CCB}")
					(number "6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{CCA}")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 2.54)
					(name "A_{1}")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "A_{2}")
					(number "9")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "DIR_{1}")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
)
