(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN74AXC4T245_UQFN"
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.894 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN74AXC4T245_UQFN"
				(at 41.148 -5.334 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN74AXC4T245_UQFN"
				(at 41.148 -7.874 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/gpn/sn74axc4t245"
				(at 41.148 -13.462 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Four-Bit Bus Transceiver, 0.65V to 3.6V voltage translation, direction and output enable control, 16 pin UQFN"
				(at 41.148 -23.876 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN74AXC4T245RSVR"
				(at 41.148 -10.922 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 41.148 -18.796 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 41.148 -21.336 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 41.148 -16.002 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, LEVEL-SHIFTER, VOLTAGE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "RSV16_TEX"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN74AXC4T245_UQFN_1_1"
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "1~{OE}")
					(number "1")
				)
				(pin power_in line
					(at 21.59 0 180)
					(length 2.54)
					(name "V_{CCB}")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{CCA}")
					(number "3")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "1DIR")
					(number "4")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "2DIR")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 2.54)
					(name "1A1")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "1A2")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 2.54)
					(name "2A1")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 2.54)
					(name "2A2")
					(number "9")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 2.54)
					(name "GND")
					(number "10")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "11")
				)
				(pin bidirectional line
					(at 21.59 -13.97 180)
					(length 2.54)
					(name "2B2")
					(number "12")
				)
				(pin bidirectional line
					(at 21.59 -11.43 180)
					(length 2.54)
					(name "2B1")
					(number "13")
				)
				(pin bidirectional line
					(at 21.59 -6.35 180)
					(length 2.54)
					(name "1B2")
					(number "14")
				)
				(pin bidirectional line
					(at 21.59 -3.81 180)
					(length 2.54)
					(name "1B1")
					(number "15")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 2.54)
					(name "2~{OE}")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
