(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN74AXC8T245_UQFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.8 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN74AXC8T245_UQFN"
				(at 50.8 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN74AXC8T245_UQFN"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74axc8t245.pdf?ts=1702327536011"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "8-bit dual-supply bus transceiver"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN74AXC8T245RJWR"
				(at 50.8 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "LEVEL-SHIFTER , DIGITAL"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN74AXC8T245_UQFN_0_1")
			(symbol "SN74AXC8T245_UQFN_1_1"
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "DIR1")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "A1")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "A2")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "A3")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "A4")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "A5")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "A6")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "A7")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "A8")
					(number "9")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "DIR2")
					(number "10")
				)
				(pin power_in line
					(at 20.32 -35.56 180)
					(length 2.54)
					(name "GND")
					(number "11")
				)
				(pin passive line
					(at 20.32 -35.56 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "12")
				)
				(pin bidirectional line
					(at 20.32 -22.86 180)
					(length 2.54)
					(name "B8")
					(number "13")
				)
				(pin bidirectional line
					(at 20.32 -20.32 180)
					(length 2.54)
					(name "B7")
					(number "14")
				)
				(pin bidirectional line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "B6")
					(number "15")
				)
				(pin bidirectional line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "B5")
					(number "16")
				)
				(pin bidirectional line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "B4")
					(number "17")
				)
				(pin bidirectional line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "B3")
					(number "18")
				)
				(pin bidirectional line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "B2")
					(number "19")
				)
				(pin bidirectional line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "B1")
					(number "20")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "OE_N")
					(number "21")
				)
				(pin power_in line
					(at 20.32 0 180)
					(length 2.54)
					(name "VCCB")
					(number "22")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(hide yes)
					(name "VCCB")
					(number "23")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCCA")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
)
