(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN74HC595B"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN74HC595B"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN74HC595B"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/general/docs/suppproductinfo.tsp?distId=26&gotoUrl=https://www.ti.com/lit/gpn/sn74hc595b"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Shift Register, 74HC595, Serial to Parallel, 1 Element, 8 bit, X1QFN, 16 Pins"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN74HC595BRWNR"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, LEVEL-SHIFTER, VOLTAGE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN74HC595B_1_1"
				(pin output line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "QB")
					(number "1")
				)
				(pin output line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "QC")
					(number "2")
				)
				(pin output line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "QD")
					(number "3")
				)
				(pin output line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "QE")
					(number "4")
				)
				(pin output line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "QF")
					(number "5")
				)
				(pin output line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "QG")
					(number "6")
				)
				(pin output line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "QH")
					(number "7")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin output line
					(at 20.32 -20.32 180)
					(length 2.54)
					(name "QH'")
					(number "9")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "~{SRCLR}")
					(number "10")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SRCLK")
					(number "11")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "RCLK")
					(number "12")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{OE}")
					(number "13")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SER")
					(number "14")
				)
				(pin output line
					(at 20.32 0 180)
					(length 2.54)
					(name "QA")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "16")
				)
				(pin no_connect line
					(at 2.54 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "EP")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
)
