(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN74LV1T125DBVR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN74LV1T125DBVR"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN74LV1T125DBVR"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lv1t125.pdf?HQS=dis-mous-null-mousermode-dsf-pf-null-wwe&ts=1627648952184&ref_url=https%253A%252F%252Fmouser.com%252F"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Buffer, 74LV1T125, 1.6 V to 5.5 V, SOT-23-5"
				(at 27.94 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN74LV1T125DBVR"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 27.94 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, BUFFER, TRANSCEIVER, LEVEL-SHIFTER, GATE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN74LV1T125DBVR_1_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "~{OE}")
					(number "1")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "A")
					(number "2")
				)
				(pin power_in line
					(at 13.97 -7.62 180)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin output line
					(at 13.97 -3.81 180)
					(length 2.54)
					(name "Y")
					(number "4")
				)
				(pin power_in line
					(at 13.97 0 180)
					(length 2.54)
					(name "VCC")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
)
