(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN74LVC1T45YZPR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 39.37 1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN74LVC1T45YZPR"
				(at 39.37 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN74LVC1T45YZPR"
				(at 39.37 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1t45.pdf"
				(at 39.37 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Single-Bit Dual-Supply Bus Transceiver with Configurable Voltage-Level Shifting and 3-State Outputs"
				(at 39.37 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN74LVC1T45YZPR"
				(at 39.37 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 39.37 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 39.37 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 39.37 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, LEVEL-SHIFTER, VOLTAGE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN74LVC1T45YZPR_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCCA")
					(number "A1")
				)
				(pin power_in line
					(at 16.51 0 180)
					(length 2.54)
					(name "VCCB")
					(number "A2")
				)
				(pin power_in line
					(at 16.51 -5.08 180)
					(length 2.54)
					(name "GND")
					(number "B1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DIR")
					(number "B2")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "A")
					(number "C1")
				)
				(pin bidirectional line
					(at 16.51 -2.54 180)
					(length 2.54)
					(name "B")
					(number "C2")
				)
			)
			(embedded_fonts no)
		)
)
