(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN74LXC1T45DBVR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 30.48 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN74LXC1T45DBVR"
				(at 30.48 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN74LXC1T45DBVR"
				(at 30.48 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lxc1t45.pdf?ts=1641200283005&ref_url=https%253A%252F%252Fwww.ti.com%252Fstore%252Fti%252Fen%252Fp%252Fproduct%252F%253Fp%253DSN74LXC1T45DBVR%2526keyMatch%253DSN74LXC1T45DBVR%2526tisearch%253Dsearch-everything%2526usecase%253DOPN"
				(at 30.48 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Logic translator/level shifter"
				(at 30.48 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN74LXC1T45DBVR"
				(at 30.48 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 30.48 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 30.48 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 30.48 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, LEVEL-SHIFTER, VOLTAGE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN74LXC1T45DBVR_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCCA")
					(number "1")
				)
				(pin power_in line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "A")
					(number "3")
				)
				(pin bidirectional line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "B")
					(number "4")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DIR")
					(number "5")
				)
				(pin power_in line
					(at 17.78 0 180)
					(length 2.54)
					(name "VCCB")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
