(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SPV1040TTR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SPV1040TTR"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SPV1040TTR"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/0d/30/c2/1a/92/03/48/cb/CD00287506.pdf/files/CD00287506.pdf/jcr:content/translations/en.CD00287506.pdf"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Battery Charger for 1 Cell, 5.5V Input, 5.2V Charge, TSSOP-8"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 43.18 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SPV1040TTR"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SPV1040TTR_1_1"
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "MPP-SET")
					(number "1")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "LX")
					(number "3")
				)
				(pin power_out line
					(at 24.13 0 180)
					(length 2.54)
					(name "VOUT")
					(number "4")
				)
				(pin input line
					(at 24.13 -7.62 180)
					(length 2.54)
					(name "VCTRL")
					(number "5")
				)
				(pin input line
					(at 24.13 -5.08 180)
					(length 2.54)
					(name "ICTRL_M")
					(number "6")
				)
				(pin input line
					(at 24.13 -2.54 180)
					(length 2.54)
					(name "ICTRL_P")
					(number "7")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "XSHUT")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
