(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SST26VF064B"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SST26VF064B"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SST26VF064B"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/3/282/1/SST26VF064B-SST26VF064BA-2-5V-3-0V-64-Mbit-Serial-Quad-IO--SQI--Flash-Memory-20005119K.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "64-Mbit 2.3V-3.6V, SQI Flash Memory, -40°C to +85°C"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SST26VF064B-104I/SM"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, FLASH, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SST26VF064B_0_0"
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SCK")
					(number "6")
				)
			)
			(symbol "SST26VF064B_1_0"
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "CE#")
					(number "1")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 2.54)
					(name "SO")
					(number "2")
					(alternate "SIO1" bidirectional line)
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "WP#")
					(number "3")
					(alternate "SIO2" bidirectional line)
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 2.54)
					(name "V_{SS}")
					(number "4")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SI")
					(number "5")
					(alternate "SIO0" bidirectional line)
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "HOLD#")
					(number "7")
					(alternate "SIO3" bidirectional line)
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{DD}")
					(number "8")
				)
			)
			(symbol "SST26VF064B_1_1")
			(embedded_fonts no)
		)
)
