(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "STM32F103C8T6"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.8 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "STM32F103C8T6"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "STM32F103C8T6"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103c8.pdf"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM MCU, Motor Control, STM32 Family STM32F1 Series Microcontrollers, ARM Cortex-M3, 32 bit, 72 MHz"
				(at 50.8 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "STM32F103C8T6"
				(at 50.8 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MICROCONTROLLER, IC, ARM, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "STM32F103C8T6_1_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "VBAT")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 2.54)
					(name "PC13-TAMPER-RTC")
					(number "2")
					(alternate "RTC_OUT" output line)
					(alternate "RTC_TAMPER" input line)
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 2.54)
					(name "PC14-OSC32_IN")
					(number "3")
					(alternate "RCC_OSC32_IN " input line)
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 2.54)
					(name "PC15-OSC32_OUT")
					(number "4")
					(alternate "ADC1_EXTI15" input line)
					(alternate "ADC2_EXTI15" input line)
					(alternate "RCC_OSC32_OUT" output line)
				)
				(pin bidirectional line
					(at 33.02 -43.18 180)
					(length 2.54)
					(name "PD0_OSC_IN")
					(number "5")
					(alternate "RCC_OSC_IN" input line)
				)
				(pin bidirectional line
					(at 33.02 -45.72 180)
					(length 2.54)
					(name "PD1_OSC_OUT")
					(number "6")
					(alternate "RCC_OSC_OUT" output line)
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "NRST")
					(number "7")
				)
				(pin power_in line
					(at 33.02 -59.69 180)
					(length 2.54)
					(name "VSSA")
					(number "8")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDA")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "PA0_WKUP")
					(number "10")
					(alternate "ADC1_IN0" input line)
					(alternate "ADC2_IN0" input line)
					(alternate "SYS_WKUP" output line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "USART2_CTS" output line)
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "PA1")
					(number "11")
					(alternate "ADC1_IN1" input line)
					(alternate "ADC2_IN1" input line)
					(alternate "TIM2_CH2" bidirectional line)
					(alternate "USART2_RTS" output line)
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "PA2")
					(number "12")
					(alternate "ADC1_IN2" input line)
					(alternate "ADC2_IN2" input line)
					(alternate "TIM2_CH3" bidirectional line)
					(alternate "USART2_TX" output line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "PA3")
					(number "13")
					(alternate "ADC1_IN3" input line)
					(alternate "ADC2_IN3" input line)
					(alternate "TIM2_CH4" bidirectional line)
					(alternate "USART2_RX" input line)
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "PA4")
					(number "14")
					(alternate "ADC1_IN4" input line)
					(alternate "ADC2_IN4" input line)
					(alternate "SPI1_NSS" output line)
					(alternate "USART2_CK" output line)
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "PA5")
					(number "15")
					(alternate "ADC1_IN5" input line)
					(alternate "ADC2_IN5" input line)
					(alternate "SPI1_SCK" output line)
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "PA6")
					(number "16")
					(alternate "ADC1_IN6" input line)
					(alternate "ADC2_IN6" input line)
					(alternate "SPI1_MISO" input line)
					(alternate "TIM1_BKIN" input line)
					(alternate "TIM3_CH1" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "PA7")
					(number "17")
					(alternate "ADC1_IN7" input line)
					(alternate "ADC2_IN7" input line)
					(alternate "SPI1_MOSI" output line)
					(alternate "TIM1_CH1N" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
				)
				(pin bidirectional line
					(at 33.02 0 180)
					(length 2.54)
					(name "PB0")
					(number "18")
					(alternate "ADC1_IN8" input line)
					(alternate "ADC2_IN8" input line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
				)
				(pin bidirectional line
					(at 33.02 -2.54 180)
					(length 2.54)
					(name "PB1")
					(number "19")
					(alternate "ADC1_IN9" input line)
					(alternate "ADC2_IN9" input line)
					(alternate "TIM1_CH3N" bidirectional line)
					(alternate "TIM3_CH4" bidirectional line)
				)
				(pin bidirectional line
					(at 33.02 -5.08 180)
					(length 2.54)
					(name "PB2")
					(number "20")
				)
				(pin bidirectional line
					(at 33.02 -25.4 180)
					(length 2.54)
					(name "PB10")
					(number "21")
					(alternate "TIM2_CH3" bidirectional line)
				)
				(pin bidirectional line
					(at 33.02 -27.94 180)
					(length 2.54)
					(name "PB11")
					(number "22")
					(alternate "ADC1_EXTI11" input line)
					(alternate "ADC2_EXTI11" input line)
					(alternate "TIM2_CH4" bidirectional line)
				)
				(pin passive line
					(at 33.02 -62.23 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "23")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDD")
					(number "24")
				)
				(pin bidirectional line
					(at 33.02 -30.48 180)
					(length 2.54)
					(name "PB12")
					(number "25")
					(alternate "TIM1_BKIN" input line)
				)
				(pin bidirectional line
					(at 33.02 -33.02 180)
					(length 2.54)
					(name "PB13")
					(number "26")
					(alternate "TIM1_CH1N" bidirectional line)
				)
				(pin bidirectional line
					(at 33.02 -35.56 180)
					(length 2.54)
					(name "PB14")
					(number "27")
					(alternate "TIM1_CH2N" bidirectional line)
				)
				(pin bidirectional line
					(at 33.02 -38.1 180)
					(length 2.54)
					(name "PB15")
					(number "28")
					(alternate "ADC1_EXTI15" input line)
					(alternate "ADC2_EXTI15" input line)
					(alternate "TIM1_CH3N" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "PA8")
					(number "29")
					(alternate "RCC_MCO" output line)
					(alternate "TIM1_CH1" bidirectional line)
					(alternate "USART1_CK" output line)
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "PA9")
					(number "30")
					(alternate "TIM1_CH2" bidirectional line)
					(alternate "USART1_TX" output line)
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "PA10")
					(number "31")
					(alternate "TIM1_CH3" bidirectional line)
					(alternate "USART1_RX" input line)
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "PA11")
					(number "32")
					(alternate "ADC1_EXTI11" input line)
					(alternate "ADC2_EXTI11" input line)
					(alternate "CAN_RX" input line)
					(alternate "TIM1_CH4" bidirectional line)
					(alternate "USART1_CTS" output line)
					(alternate "USB_DM" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "PA12")
					(number "33")
					(alternate "CAN_TX" output line)
					(alternate "TIM1_ETR" input line)
					(alternate "USART1_RTS" output line)
					(alternate "USB_DP" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "PA13")
					(number "34")
					(alternate "SYS_JTMS-SWDIO" bidirectional line)
				)
				(pin power_in line
					(at 33.02 -62.23 180)
					(length 2.54)
					(name "VSS")
					(number "35")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "36")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "PA14")
					(number "37")
					(alternate "SYS_JTCK-SWCLK" output line)
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "PA15")
					(number "38")
					(alternate "ADC1_EXTI15" input line)
					(alternate "ADC2_EXTI15" input line)
					(alternate "SPI1_NSS" output line)
					(alternate "SYS_JTDI" input line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" input line)
				)
				(pin bidirectional line
					(at 33.02 -7.62 180)
					(length 2.54)
					(name "PB3")
					(number "39")
					(alternate "SPI1_SCK" output line)
					(alternate "SYS_JTDO-TRACESWO" output line)
					(alternate "TIM2_CH2" bidirectional line)
				)
				(pin bidirectional line
					(at 33.02 -10.16 180)
					(length 2.54)
					(name "PB4")
					(number "40")
					(alternate "SPI1_MISO" input line)
					(alternate "SYS_NJTRST" input line)
					(alternate "TIM3_CH1" bidirectional line)
				)
				(pin bidirectional line
					(at 33.02 -12.7 180)
					(length 2.54)
					(name "PB5")
					(number "41")
					(alternate "I2C1_SMBA" bidirectional line)
					(alternate "SPI1_MOSI" output line)
					(alternate "TIM3_CH2" bidirectional line)
				)
				(pin bidirectional line
					(at 33.02 -15.24 180)
					(length 2.54)
					(name "PB6")
					(number "42")
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "USART1_TX" output line)
				)
				(pin bidirectional line
					(at 33.02 -17.78 180)
					(length 2.54)
					(name "PB7")
					(number "43")
					(alternate "I2C1_SDA" bidirectional line)
					(alternate "USART1_RX" input line)
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "BOOT0")
					(number "44")
				)
				(pin bidirectional line
					(at 33.02 -20.32 180)
					(length 2.54)
					(name "PB8")
					(number "45")
					(alternate "CAN_RX" input line)
					(alternate "I2C1_SCL" bidirectional line)
				)
				(pin bidirectional line
					(at 33.02 -22.86 180)
					(length 2.54)
					(name "PB9")
					(number "46")
					(alternate "CAN_TX" output line)
					(alternate "I2C1_SDA" bidirectional line)
				)
				(pin passive line
					(at 33.02 -62.23 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "47")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "48")
				)
			)
			(embedded_fonts no)
		)
)
