(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "STM32F401RET6"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 60.96 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "STM32F401RET6"
				(at 60.96 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "STM32F401RET6"
				(at 60.96 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f401re.pdf"
				(at 60.96 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM MCU, Dynamic Efficiency Line, STM32 Family STM32F4 Series Microcontrollers, ARM Cortex-M4"
				(at 60.96 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 60.96 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "STM32F401RET6"
				(at 60.96 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 60.96 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 60.96 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MICROCONTROLLER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "STM32F401RET6_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VBAT")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 2.54)
					(name "PC13")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 2.54)
					(name "PC14-OSC32_IN")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 2.54)
					(name "PC15-OSC32_OUT")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "PH0-OSC_IN")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "PH1-OSC_OUT")
					(number "6")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "NRST")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "PC0")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "PC1")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "PC2")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "PC3")
					(number "11")
				)
				(pin power_in line
					(at 0 -81.28 0)
					(length 2.54)
					(name "VSSA")
					(number "12")
					(alternate "VREF-" passive line)
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDDA")
					(number "13")
					(alternate "VREF+" passive line)
				)
				(pin bidirectional line
					(at 38.1 0 180)
					(length 2.54)
					(name "PA0")
					(number "14")
				)
				(pin bidirectional line
					(at 38.1 -2.54 180)
					(length 2.54)
					(name "PA1")
					(number "15")
				)
				(pin bidirectional line
					(at 38.1 -5.08 180)
					(length 2.54)
					(name "PA2")
					(number "16")
				)
				(pin bidirectional line
					(at 38.1 -7.62 180)
					(length 2.54)
					(name "PA3")
					(number "17")
				)
				(pin power_in line
					(at 0 -78.74 0)
					(length 2.54)
					(name "VSS")
					(number "18")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "19")
				)
				(pin bidirectional line
					(at 38.1 -10.16 180)
					(length 2.54)
					(name "PA4")
					(number "20")
				)
				(pin bidirectional line
					(at 38.1 -12.7 180)
					(length 2.54)
					(name "PA5")
					(number "21")
				)
				(pin bidirectional line
					(at 38.1 -15.24 180)
					(length 2.54)
					(name "PA6")
					(number "22")
				)
				(pin bidirectional line
					(at 38.1 -17.78 180)
					(length 2.54)
					(name "PA7")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "PC4")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "PC5")
					(number "25")
				)
				(pin bidirectional line
					(at 38.1 -43.18 180)
					(length 2.54)
					(name "PB0")
					(number "26")
				)
				(pin bidirectional line
					(at 38.1 -45.72 180)
					(length 2.54)
					(name "PB1")
					(number "27")
				)
				(pin bidirectional line
					(at 38.1 -48.26 180)
					(length 2.54)
					(name "PB2")
					(number "28")
				)
				(pin bidirectional line
					(at 38.1 -68.58 180)
					(length 2.54)
					(name "PB10")
					(number "29")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VCAP1")
					(number "30")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "31")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "32")
				)
				(pin bidirectional line
					(at 38.1 -73.66 180)
					(length 2.54)
					(name "PB12")
					(number "33")
				)
				(pin bidirectional line
					(at 38.1 -76.2 180)
					(length 2.54)
					(name "PB13")
					(number "34")
				)
				(pin bidirectional line
					(at 38.1 -78.74 180)
					(length 2.54)
					(name "PB14")
					(number "35")
				)
				(pin bidirectional line
					(at 38.1 -81.28 180)
					(length 2.54)
					(name "PB15")
					(number "36")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "PC6")
					(number "37")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "PC7")
					(number "38")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "PC8")
					(number "39")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "PC9")
					(number "40")
				)
				(pin bidirectional line
					(at 38.1 -20.32 180)
					(length 2.54)
					(name "PA8")
					(number "41")
				)
				(pin bidirectional line
					(at 38.1 -22.86 180)
					(length 2.54)
					(name "PA9")
					(number "42")
				)
				(pin bidirectional line
					(at 38.1 -25.4 180)
					(length 2.54)
					(name "PA10")
					(number "43")
				)
				(pin bidirectional line
					(at 38.1 -27.94 180)
					(length 2.54)
					(name "PA11")
					(number "44")
				)
				(pin bidirectional line
					(at 38.1 -30.48 180)
					(length 2.54)
					(name "PA12")
					(number "45")
				)
				(pin bidirectional line
					(at 38.1 -33.02 180)
					(length 2.54)
					(name "PA13")
					(number "46")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "47")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "48")
				)
				(pin bidirectional line
					(at 38.1 -35.56 180)
					(length 2.54)
					(name "PA14")
					(number "49")
				)
				(pin bidirectional line
					(at 38.1 -38.1 180)
					(length 2.54)
					(name "PA15")
					(number "50")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "PC10")
					(number "51")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 2.54)
					(name "PC11")
					(number "52")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 2.54)
					(name "PC12")
					(number "53")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "PD2")
					(number "54")
				)
				(pin bidirectional line
					(at 38.1 -50.8 180)
					(length 2.54)
					(name "PB3")
					(number "55")
				)
				(pin bidirectional line
					(at 38.1 -53.34 180)
					(length 2.54)
					(name "PB4")
					(number "56")
				)
				(pin bidirectional line
					(at 38.1 -55.88 180)
					(length 2.54)
					(name "PB5")
					(number "57")
				)
				(pin bidirectional line
					(at 38.1 -58.42 180)
					(length 2.54)
					(name "PB6")
					(number "58")
				)
				(pin bidirectional line
					(at 38.1 -60.96 180)
					(length 2.54)
					(name "PB7")
					(number "59")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "BOOT0")
					(number "60")
				)
				(pin bidirectional line
					(at 38.1 -63.5 180)
					(length 2.54)
					(name "PB8")
					(number "61")
				)
				(pin bidirectional line
					(at 38.1 -66.04 180)
					(length 2.54)
					(name "PB9")
					(number "62")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "63")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "64")
				)
			)
			(embedded_fonts no)
		)
)
