(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "STM32F407VET6"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 54.61 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "STM32F407VET6"
				(at 54.61 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "STM32F407VET6"
				(at 54.61 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f407ve.pdf"
				(at 54.61 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "High-performance foundation line, Arm Cortex-M4 core with DSP and FPU, 512 Kbytes of Flash memory, 168 MHz CPU, ART Accelerator, Ethernet, FSMC"
				(at 54.61 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "STM32F407VET6"
				(at 54.61 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 54.61 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 54.61 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 54.61 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, MCU, ADC, CLOCK, DAC, MICROCONTROLLER, SOC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "STM32F407VET6_1_1"
				(text "POWER"
					(at 12.7 -6.35 900)
				)
				(text "HSE"
					(at 12.7 -19.05 900)
				)
				(text "LSE"
					(at 12.7 -26.67 900)
				)
				(text "C_{ext}"
					(at 24.13 -1.27 900)
				)
				(text "Boot and Reset"
					(at 24.13 -13.97 900)
				)
				(text "POWER"
					(at 24.13 -26.67 900)
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 3.81)
					(name "VBAT")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PC14")
					(number "8")
					(alternate "RCC_OSC32_IN" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PC15")
					(number "9")
					(alternate "ADC1_EXTI15" bidirectional line)
					(alternate "ADC2_EXTI15" bidirectional line)
					(alternate "ADC3_EXTI15" bidirectional line)
					(alternate "RCC_OSC32_OUT" bidirectional line)
				)
				(pin power_in line
					(at 38.1 -27.94 180)
					(length 3.81)
					(name "VSS")
					(number "10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PH0")
					(number "12")
					(alternate "RCC_OSC_IN" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PH1")
					(number "13")
					(alternate "RCC_OSC_OUT" bidirectional line)
				)
				(pin input line
					(at 38.1 -12.7 180)
					(length 3.81)
					(name "NRST")
					(number "14")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "19")
				)
				(pin power_in line
					(at 38.1 -25.4 180)
					(length 3.81)
					(name "VSSA")
					(number "20")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VREF+")
					(number "21")
				)
				(pin power_in line
					(at 0 -3.81 0)
					(length 3.81)
					(name "VDDA")
					(number "22")
				)
				(pin passive line
					(at 38.1 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "27")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "28")
				)
				(pin power_out line
					(at 38.1 0 180)
					(length 3.81)
					(name "VCAP_1")
					(number "49")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "50")
				)
				(pin power_out line
					(at 38.1 -2.54 180)
					(length 3.81)
					(name "VCAP_2")
					(number "73")
				)
				(pin passive line
					(at 38.1 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "74")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "75")
				)
				(pin input line
					(at 38.1 -15.24 180)
					(length 3.81)
					(name "BOOT0")
					(number "94")
				)
				(pin passive line
					(at 38.1 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "99")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "100")
				)
			)
			(symbol "STM32F407VET6_2_1"
				(text "GPIOA"
					(at 13.97 -19.05 900)
				)
				(text "GPIOB"
					(at 13.97 -60.96 900)
				)
				(text "GPIOC"
					(at 19.05 -91.44 0)
				)
				(text "GPIOD"
					(at 24.13 -19.05 900)
				)
				(text "GPIOE"
					(at 24.13 -60.96 900)
				)
				(pin bidirectional line
					(at 38.1 -46.99 180)
					(length 3.81)
					(name "PE2")
					(number "1")
					(alternate "ETH_TXD3" bidirectional line)
					(alternate "FMC_A23" bidirectional line)
					(alternate "SAI1_MCLK_A" bidirectional line)
					(alternate "SPI4_SCK" bidirectional line)
					(alternate "SYS_TRACECLK" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -49.53 180)
					(length 3.81)
					(name "PE3")
					(number "2")
					(alternate "FMC_A19" bidirectional line)
					(alternate "SAI1_SD_B" bidirectional line)
					(alternate "SYS_TRACED0" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -52.07 180)
					(length 3.81)
					(name "PE4")
					(number "3")
					(alternate "DCMI_D4" bidirectional line)
					(alternate "FMC_A20" bidirectional line)
					(alternate "SAI1_FS_A" bidirectional line)
					(alternate "SPI4_NSS" bidirectional line)
					(alternate "SYS_TRACED1" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -54.61 180)
					(length 3.81)
					(name "PE5")
					(number "4")
					(alternate "DCMI_D6" bidirectional line)
					(alternate "FMC_A21" bidirectional line)
					(alternate "SAI1_SCK_A" bidirectional line)
					(alternate "SPI4_MISO" bidirectional line)
					(alternate "SYS_TRACED2" bidirectional line)
					(alternate "TIM9_CH1" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -57.15 180)
					(length 3.81)
					(name "PE6")
					(number "5")
					(alternate "DCMI_D7" bidirectional line)
					(alternate "FMC_A22" bidirectional line)
					(alternate "SAI1_SD_A" bidirectional line)
					(alternate "SPI4_MOSI" bidirectional line)
					(alternate "SYS_TRACED3" bidirectional line)
					(alternate "TIM9_CH2" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -99.06 180)
					(length 3.81)
					(name "PC13")
					(number "7")
					(alternate "RTC_AF1" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 3.81)
					(name "PC0")
					(number "15")
					(alternate "ADC1_IN10" bidirectional line)
					(alternate "ADC2_IN10" bidirectional line)
					(alternate "ADC3_IN10" bidirectional line)
					(alternate "FMC_SDNWE" bidirectional line)
					(alternate "USB_OTG_HS_ULPI_STP" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 3.81)
					(name "PC1")
					(number "16")
					(alternate "ADC1_IN11" bidirectional line)
					(alternate "ADC2_IN11" bidirectional line)
					(alternate "ADC3_IN11" bidirectional line)
					(alternate "ETH_MDC" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 3.81)
					(name "PC2")
					(number "17")
					(alternate "ADC1_IN12" bidirectional line)
					(alternate "ADC2_IN12" bidirectional line)
					(alternate "ADC3_IN12" bidirectional line)
					(alternate "ETH_TXD2" bidirectional line)
					(alternate "FMC_SDNE0" bidirectional line)
					(alternate "I2S2_ext_SD" bidirectional line)
					(alternate "SPI2_MISO" bidirectional line)
					(alternate "USB_OTG_HS_ULPI_DIR" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 3.81)
					(name "PC3")
					(number "18")
					(alternate "ADC1_IN13" bidirectional line)
					(alternate "ADC2_IN13" bidirectional line)
					(alternate "ADC3_IN13" bidirectional line)
					(alternate "ETH_TX_CLK" bidirectional line)
					(alternate "FMC_SDCKE0" bidirectional line)
					(alternate "I2S2_SD" bidirectional line)
					(alternate "SPI2_MOSI" bidirectional line)
					(alternate "USB_OTG_HS_ULPI_NXT" bidirectional line)
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PA0")
					(number "23")
					(alternate "ADC1_IN0" bidirectional line)
					(alternate "ADC2_IN0" bidirectional line)
					(alternate "ADC3_IN0" bidirectional line)
					(alternate "ETH_CRS" bidirectional line)
					(alternate "SYS_WKUP" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "TIM5_CH1" bidirectional line)
					(alternate "TIM8_ETR" bidirectional line)
					(alternate "UART4_TX" bidirectional line)
					(alternate "USART2_CTS" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PA1")
					(number "24")
					(alternate "ADC1_IN1" bidirectional line)
					(alternate "ADC2_IN1" bidirectional line)
					(alternate "ADC3_IN1" bidirectional line)
					(alternate "ETH_REF_CLK" bidirectional line)
					(alternate "ETH_RX_CLK" bidirectional line)
					(alternate "TIM2_CH2" bidirectional line)
					(alternate "TIM5_CH2" bidirectional line)
					(alternate "UART4_RX" bidirectional line)
					(alternate "USART2_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PA2")
					(number "25")
					(alternate "ADC1_IN2" bidirectional line)
					(alternate "ADC2_IN2" bidirectional line)
					(alternate "ADC3_IN2" bidirectional line)
					(alternate "ETH_MDIO" bidirectional line)
					(alternate "TIM2_CH3" bidirectional line)
					(alternate "TIM5_CH3" bidirectional line)
					(alternate "TIM9_CH1" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PA3")
					(number "26")
					(alternate "ADC1_IN3" bidirectional line)
					(alternate "ADC2_IN3" bidirectional line)
					(alternate "ADC3_IN3" bidirectional line)
					(alternate "ETH_COL" bidirectional line)
					(alternate "TIM2_CH4" bidirectional line)
					(alternate "TIM5_CH4" bidirectional line)
					(alternate "TIM9_CH2" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
					(alternate "USB_OTG_HS_ULPI_D0" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PA4")
					(number "29")
					(alternate "ADC1_IN4" bidirectional line)
					(alternate "ADC2_IN4" bidirectional line)
					(alternate "DAC_OUT1" bidirectional line)
					(alternate "DCMI_HSYNC" bidirectional line)
					(alternate "I2S3_WS" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "SPI3_NSS" bidirectional line)
					(alternate "USART2_CK" bidirectional line)
					(alternate "USB_OTG_HS_SOF" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PA5")
					(number "30")
					(alternate "ADC1_IN5" bidirectional line)
					(alternate "ADC2_IN5" bidirectional line)
					(alternate "DAC_OUT2" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "TIM8_CH1N" bidirectional line)
					(alternate "USB_OTG_HS_ULPI_CK" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PA6")
					(number "31")
					(alternate "ADC1_IN6" bidirectional line)
					(alternate "ADC2_IN6" bidirectional line)
					(alternate "DCMI_PIXCLK" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "TIM13_CH1" bidirectional line)
					(alternate "TIM1_BKIN" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
					(alternate "TIM8_BKIN" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PA7")
					(number "32")
					(alternate "ADC1_IN7" bidirectional line)
					(alternate "ADC2_IN7" bidirectional line)
					(alternate "ETH_CRS_DV" bidirectional line)
					(alternate "ETH_RX_DV" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
					(alternate "TIM1_CH1N" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "TIM8_CH1N" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 3.81)
					(name "PC4")
					(number "33")
					(alternate "ADC1_IN14" bidirectional line)
					(alternate "ADC2_IN14" bidirectional line)
					(alternate "ETH_RXD0" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 3.81)
					(name "PC5")
					(number "34")
					(alternate "ADC1_IN15" bidirectional line)
					(alternate "ADC2_IN15" bidirectional line)
					(alternate "ETH_RXD1" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 3.81)
					(name "PB0")
					(number "35")
					(alternate "ADC1_IN8" bidirectional line)
					(alternate "ADC2_IN8" bidirectional line)
					(alternate "ETH_RXD2" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
					(alternate "TIM8_CH2N" bidirectional line)
					(alternate "USB_OTG_HS_ULPI_D1" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 3.81)
					(name "PB1")
					(number "36")
					(alternate "ADC1_IN9" bidirectional line)
					(alternate "ADC2_IN9" bidirectional line)
					(alternate "ETH_RXD3" bidirectional line)
					(alternate "TIM1_CH3N" bidirectional line)
					(alternate "TIM3_CH4" bidirectional line)
					(alternate "TIM8_CH3N" bidirectional line)
					(alternate "USB_OTG_HS_ULPI_D2" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 3.81)
					(name "PB2")
					(number "37")
				)
				(pin bidirectional line
					(at 38.1 -59.69 180)
					(length 3.81)
					(name "PE7")
					(number "38")
					(alternate "FMC_D4" bidirectional line)
					(alternate "FMC_DA4" bidirectional line)
					(alternate "TIM1_ETR" bidirectional line)
					(alternate "UART7_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -62.23 180)
					(length 3.81)
					(name "PE8")
					(number "39")
					(alternate "FMC_D5" bidirectional line)
					(alternate "FMC_DA5" bidirectional line)
					(alternate "TIM1_CH1N" bidirectional line)
					(alternate "UART7_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -64.77 180)
					(length 3.81)
					(name "PE9")
					(number "40")
					(alternate "DAC_EXTI9" bidirectional line)
					(alternate "FMC_D6" bidirectional line)
					(alternate "FMC_DA6" bidirectional line)
					(alternate "TIM1_CH1" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -67.31 180)
					(length 3.81)
					(name "PE10")
					(number "41")
					(alternate "FMC_D7" bidirectional line)
					(alternate "FMC_DA7" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -69.85 180)
					(length 3.81)
					(name "PE11")
					(number "42")
					(alternate "ADC1_EXTI11" bidirectional line)
					(alternate "ADC2_EXTI11" bidirectional line)
					(alternate "ADC3_EXTI11" bidirectional line)
					(alternate "FMC_D8" bidirectional line)
					(alternate "FMC_DA8" bidirectional line)
					(alternate "SPI4_NSS" bidirectional line)
					(alternate "TIM1_CH2" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -72.39 180)
					(length 3.81)
					(name "PE12")
					(number "43")
					(alternate "FMC_D9" bidirectional line)
					(alternate "FMC_DA9" bidirectional line)
					(alternate "SPI4_SCK" bidirectional line)
					(alternate "TIM1_CH3N" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -74.93 180)
					(length 3.81)
					(name "PE13")
					(number "44")
					(alternate "FMC_D10" bidirectional line)
					(alternate "FMC_DA10" bidirectional line)
					(alternate "SPI4_MISO" bidirectional line)
					(alternate "TIM1_CH3" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -77.47 180)
					(length 3.81)
					(name "PE14")
					(number "45")
					(alternate "FMC_D11" bidirectional line)
					(alternate "FMC_DA11" bidirectional line)
					(alternate "SPI4_MOSI" bidirectional line)
					(alternate "TIM1_CH4" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -80.01 180)
					(length 3.81)
					(name "PE15")
					(number "46")
					(alternate "ADC1_EXTI15" bidirectional line)
					(alternate "ADC2_EXTI15" bidirectional line)
					(alternate "ADC3_EXTI15" bidirectional line)
					(alternate "FMC_D12" bidirectional line)
					(alternate "FMC_DA12" bidirectional line)
					(alternate "TIM1_BKIN" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 3.81)
					(name "PB10")
					(number "47")
					(alternate "ETH_RX_ER" bidirectional line)
					(alternate "I2C2_SCL" bidirectional line)
					(alternate "I2S2_CK" bidirectional line)
					(alternate "SPI2_SCK" bidirectional line)
					(alternate "TIM2_CH3" bidirectional line)
					(alternate "USART3_TX" bidirectional line)
					(alternate "USB_OTG_HS_ULPI_D3" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 3.81)
					(name "PB11")
					(number "48")
					(alternate "ADC1_EXTI11" bidirectional line)
					(alternate "ADC2_EXTI11" bidirectional line)
					(alternate "ADC3_EXTI11" bidirectional line)
					(alternate "ETH_TX_EN" bidirectional line)
					(alternate "I2C2_SDA" bidirectional line)
					(alternate "TIM2_CH4" bidirectional line)
					(alternate "USART3_RX" bidirectional line)
					(alternate "USB_OTG_HS_ULPI_D4" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 3.81)
					(name "PB12")
					(number "51")
					(alternate "CAN2_RX" bidirectional line)
					(alternate "ETH_TXD0" bidirectional line)
					(alternate "I2C2_SMBA" bidirectional line)
					(alternate "I2S2_WS" bidirectional line)
					(alternate "SPI2_NSS" bidirectional line)
					(alternate "TIM1_BKIN" bidirectional line)
					(alternate "USART3_CK" bidirectional line)
					(alternate "USB_OTG_HS_ID" bidirectional line)
					(alternate "USB_OTG_HS_ULPI_D5" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 3.81)
					(name "PB13")
					(number "52")
					(alternate "CAN2_TX" bidirectional line)
					(alternate "ETH_TXD1" bidirectional line)
					(alternate "I2S2_CK" bidirectional line)
					(alternate "SPI2_SCK" bidirectional line)
					(alternate "TIM1_CH1N" bidirectional line)
					(alternate "USART3_CTS" bidirectional line)
					(alternate "USB_OTG_HS_ULPI_D6" bidirectional line)
					(alternate "USB_OTG_HS_VBUS" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 3.81)
					(name "PB14")
					(number "53")
					(alternate "I2S2_ext_SD" bidirectional line)
					(alternate "SPI2_MISO" bidirectional line)
					(alternate "TIM12_CH1" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "TIM8_CH2N" bidirectional line)
					(alternate "USART3_RTS" bidirectional line)
					(alternate "USB_OTG_HS_DM" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 3.81)
					(name "PB15")
					(number "54")
					(alternate "ADC1_EXTI15" bidirectional line)
					(alternate "ADC2_EXTI15" bidirectional line)
					(alternate "ADC3_EXTI15" bidirectional line)
					(alternate "I2S2_SD" bidirectional line)
					(alternate "RTC_REFIN" bidirectional line)
					(alternate "SPI2_MOSI" bidirectional line)
					(alternate "TIM12_CH2" bidirectional line)
					(alternate "TIM1_CH3N" bidirectional line)
					(alternate "TIM8_CH3N" bidirectional line)
					(alternate "USB_OTG_HS_DP" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -20.32 180)
					(length 3.81)
					(name "PD8")
					(number "55")
					(alternate "FMC_D13" bidirectional line)
					(alternate "FMC_DA13" bidirectional line)
					(alternate "USART3_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -22.86 180)
					(length 3.81)
					(name "PD9")
					(number "56")
					(alternate "DAC_EXTI9" bidirectional line)
					(alternate "FMC_D14" bidirectional line)
					(alternate "FMC_DA14" bidirectional line)
					(alternate "USART3_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -25.4 180)
					(length 3.81)
					(name "PD10")
					(number "57")
					(alternate "FMC_D15" bidirectional line)
					(alternate "FMC_DA15" bidirectional line)
					(alternate "USART3_CK" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -27.94 180)
					(length 3.81)
					(name "PD11")
					(number "58")
					(alternate "ADC1_EXTI11" bidirectional line)
					(alternate "ADC2_EXTI11" bidirectional line)
					(alternate "ADC3_EXTI11" bidirectional line)
					(alternate "FMC_A16" bidirectional line)
					(alternate "FMC_CLE" bidirectional line)
					(alternate "USART3_CTS" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -30.48 180)
					(length 3.81)
					(name "PD12")
					(number "59")
					(alternate "FMC_A17" bidirectional line)
					(alternate "FMC_ALE" bidirectional line)
					(alternate "TIM4_CH1" bidirectional line)
					(alternate "USART3_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -33.02 180)
					(length 3.81)
					(name "PD13")
					(number "60")
					(alternate "FMC_A18" bidirectional line)
					(alternate "TIM4_CH2" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -35.56 180)
					(length 3.81)
					(name "PD14")
					(number "61")
					(alternate "FMC_D0" bidirectional line)
					(alternate "FMC_DA0" bidirectional line)
					(alternate "TIM4_CH3" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -38.1 180)
					(length 3.81)
					(name "PD15")
					(number "62")
					(alternate "ADC1_EXTI15" bidirectional line)
					(alternate "ADC2_EXTI15" bidirectional line)
					(alternate "ADC3_EXTI15" bidirectional line)
					(alternate "FMC_D1" bidirectional line)
					(alternate "FMC_DA1" bidirectional line)
					(alternate "TIM4_CH4" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 3.81)
					(name "PC6")
					(number "63")
					(alternate "DCMI_D0" bidirectional line)
					(alternate "I2S2_MCK" bidirectional line)
					(alternate "SDIO_D6" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
					(alternate "TIM8_CH1" bidirectional line)
					(alternate "USART6_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -83.82 180)
					(length 3.81)
					(name "PC7")
					(number "64")
					(alternate "DCMI_D1" bidirectional line)
					(alternate "I2S3_MCK" bidirectional line)
					(alternate "SDIO_D7" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "TIM8_CH2" bidirectional line)
					(alternate "USART6_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -86.36 180)
					(length 3.81)
					(name "PC8")
					(number "65")
					(alternate "DCMI_D2" bidirectional line)
					(alternate "SDIO_D0" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
					(alternate "TIM8_CH3" bidirectional line)
					(alternate "USART6_CK" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -88.9 180)
					(length 3.81)
					(name "PC9")
					(number "66")
					(alternate "DAC_EXTI9" bidirectional line)
					(alternate "DCMI_D3" bidirectional line)
					(alternate "I2C3_SDA" bidirectional line)
					(alternate "I2S_CKIN" bidirectional line)
					(alternate "RCC_MCO_2" bidirectional line)
					(alternate "SDIO_D1" bidirectional line)
					(alternate "TIM3_CH4" bidirectional line)
					(alternate "TIM8_CH4" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PA8")
					(number "67")
					(alternate "I2C3_SCL" bidirectional line)
					(alternate "RCC_MCO_1" bidirectional line)
					(alternate "TIM1_CH1" bidirectional line)
					(alternate "USART1_CK" bidirectional line)
					(alternate "USB_OTG_FS_SOF" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PA9")
					(number "68")
					(alternate "DAC_EXTI9" bidirectional line)
					(alternate "DCMI_D0" bidirectional line)
					(alternate "I2C3_SMBA" bidirectional line)
					(alternate "TIM1_CH2" bidirectional line)
					(alternate "USART1_TX" bidirectional line)
					(alternate "USB_OTG_FS_VBUS" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PA10")
					(number "69")
					(alternate "DCMI_D1" bidirectional line)
					(alternate "TIM1_CH3" bidirectional line)
					(alternate "USART1_RX" bidirectional line)
					(alternate "USB_OTG_FS_ID" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PA11")
					(number "70")
					(alternate "ADC1_EXTI11" bidirectional line)
					(alternate "ADC2_EXTI11" bidirectional line)
					(alternate "ADC3_EXTI11" bidirectional line)
					(alternate "CAN1_RX" bidirectional line)
					(alternate "TIM1_CH4" bidirectional line)
					(alternate "USART1_CTS" bidirectional line)
					(alternate "USB_OTG_FS_DM" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PA12")
					(number "71")
					(alternate "CAN1_TX" bidirectional line)
					(alternate "TIM1_ETR" bidirectional line)
					(alternate "USART1_RTS" bidirectional line)
					(alternate "USB_OTG_FS_DP" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PA13")
					(number "72")
					(alternate "SYS_JTMS-SWDIO" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PA14")
					(number "76")
					(alternate "SYS_JTCK-SWCLK" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PA15")
					(number "77")
					(alternate "ADC1_EXTI15" bidirectional line)
					(alternate "ADC2_EXTI15" bidirectional line)
					(alternate "ADC3_EXTI15" bidirectional line)
					(alternate "I2S3_WS" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "SPI3_NSS" bidirectional line)
					(alternate "SYS_JTDI" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -91.44 180)
					(length 3.81)
					(name "PC10")
					(number "78")
					(alternate "DCMI_D8" bidirectional line)
					(alternate "I2S3_CK" bidirectional line)
					(alternate "SDIO_D2" bidirectional line)
					(alternate "SPI3_SCK" bidirectional line)
					(alternate "UART4_TX" bidirectional line)
					(alternate "USART3_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -93.98 180)
					(length 3.81)
					(name "PC11")
					(number "79")
					(alternate "ADC1_EXTI11" bidirectional line)
					(alternate "ADC2_EXTI11" bidirectional line)
					(alternate "ADC3_EXTI11" bidirectional line)
					(alternate "DCMI_D4" bidirectional line)
					(alternate "I2S3_ext_SD" bidirectional line)
					(alternate "SDIO_D3" bidirectional line)
					(alternate "SPI3_MISO" bidirectional line)
					(alternate "UART4_RX" bidirectional line)
					(alternate "USART3_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -96.52 180)
					(length 3.81)
					(name "PC12")
					(number "80")
					(alternate "DCMI_D9" bidirectional line)
					(alternate "I2S3_SD" bidirectional line)
					(alternate "SDIO_CK" bidirectional line)
					(alternate "SPI3_MOSI" bidirectional line)
					(alternate "UART5_TX" bidirectional line)
					(alternate "USART3_CK" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 0 180)
					(length 3.81)
					(name "PD0")
					(number "81")
					(alternate "CAN1_RX" bidirectional line)
					(alternate "FMC_D2" bidirectional line)
					(alternate "FMC_DA2" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -2.54 180)
					(length 3.81)
					(name "PD1")
					(number "82")
					(alternate "CAN1_TX" bidirectional line)
					(alternate "FMC_D3" bidirectional line)
					(alternate "FMC_DA3" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -5.08 180)
					(length 3.81)
					(name "PD2")
					(number "83")
					(alternate "DCMI_D11" bidirectional line)
					(alternate "SDIO_CMD" bidirectional line)
					(alternate "TIM3_ETR" bidirectional line)
					(alternate "UART5_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -7.62 180)
					(length 3.81)
					(name "PD3")
					(number "84")
					(alternate "DCMI_D5" bidirectional line)
					(alternate "FMC_CLK" bidirectional line)
					(alternate "I2S2_CK" bidirectional line)
					(alternate "SPI2_SCK" bidirectional line)
					(alternate "USART2_CTS" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -10.16 180)
					(length 3.81)
					(name "PD4")
					(number "85")
					(alternate "FMC_NOE" bidirectional line)
					(alternate "USART2_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -12.7 180)
					(length 3.81)
					(name "PD5")
					(number "86")
					(alternate "FMC_NWE" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -15.24 180)
					(length 3.81)
					(name "PD6")
					(number "87")
					(alternate "DCMI_D10" bidirectional line)
					(alternate "FMC_NWAIT" bidirectional line)
					(alternate "I2S3_SD" bidirectional line)
					(alternate "SAI1_SD_A" bidirectional line)
					(alternate "SPI3_MOSI" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -17.78 180)
					(length 3.81)
					(name "PD7")
					(number "88")
					(alternate "FMC_NCE2" bidirectional line)
					(alternate "FMC_NE1" bidirectional line)
					(alternate "USART2_CK" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 3.81)
					(name "PB3")
					(number "89")
					(alternate "I2S3_CK" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "SPI3_SCK" bidirectional line)
					(alternate "SYS_JTDO-SWO" bidirectional line)
					(alternate "TIM2_CH2" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 3.81)
					(name "PB4")
					(number "90")
					(alternate "I2S3_ext_SD" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "SPI3_MISO" bidirectional line)
					(alternate "SYS_JTRST" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 3.81)
					(name "PB5")
					(number "91")
					(alternate "CAN2_RX" bidirectional line)
					(alternate "DCMI_D10" bidirectional line)
					(alternate "ETH_PPS_OUT" bidirectional line)
					(alternate "FMC_SDCKE1" bidirectional line)
					(alternate "I2C1_SMBA" bidirectional line)
					(alternate "I2S3_SD" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "SPI3_MOSI" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "USB_OTG_HS_ULPI_D7" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 3.81)
					(name "PB6")
					(number "92")
					(alternate "CAN2_TX" bidirectional line)
					(alternate "DCMI_D5" bidirectional line)
					(alternate "FMC_SDNE1" bidirectional line)
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "TIM4_CH1" bidirectional line)
					(alternate "USART1_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 3.81)
					(name "PB7")
					(number "93")
					(alternate "DCMI_VSYNC" bidirectional line)
					(alternate "FMC_NL" bidirectional line)
					(alternate "I2C1_SDA" bidirectional line)
					(alternate "TIM4_CH2" bidirectional line)
					(alternate "USART1_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 3.81)
					(name "PB8")
					(number "95")
					(alternate "CAN1_RX" bidirectional line)
					(alternate "DCMI_D6" bidirectional line)
					(alternate "ETH_TXD3" bidirectional line)
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "SDIO_D4" bidirectional line)
					(alternate "TIM10_CH1" bidirectional line)
					(alternate "TIM4_CH3" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 3.81)
					(name "PB9")
					(number "96")
					(alternate "CAN1_TX" bidirectional line)
					(alternate "DAC_EXTI9" bidirectional line)
					(alternate "DCMI_D7" bidirectional line)
					(alternate "I2C1_SDA" bidirectional line)
					(alternate "I2S2_WS" bidirectional line)
					(alternate "SDIO_D5" bidirectional line)
					(alternate "SPI2_NSS" bidirectional line)
					(alternate "TIM11_CH1" bidirectional line)
					(alternate "TIM4_CH4" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -41.91 180)
					(length 3.81)
					(name "PE0")
					(number "97")
					(alternate "DCMI_D2" bidirectional line)
					(alternate "FMC_NBL0" bidirectional line)
					(alternate "TIM4_ETR" bidirectional line)
					(alternate "UART8_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 38.1 -44.45 180)
					(length 3.81)
					(name "PE1")
					(number "98")
					(alternate "DCMI_D3" bidirectional line)
					(alternate "FMC_NBL1" bidirectional line)
					(alternate "UART8_TX" bidirectional line)
				)
			)
			(embedded_fonts no)
		)
)
