(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "STM32F412CGU6"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "STM32F412CGU6"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "STM32F412CGU6"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f412cg.pdf"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "MCU 32-bit STM32F4 ARM Cortex-M4 1024KB Flash"
				(at 55.88 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "STM32F412CGU6"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MICROCONTROLLER, IC, ARM, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "STM32F412CGU6_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VBAT")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "PC13")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "PC14-_OSC32_IN")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "PC15-_OSC32__OUT")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "PH0-OSC_IN")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "PH0-OSC_OUT")
					(number "6")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "NRST")
					(number "7")
				)
				(pin power_in line
					(at 0 -74.93 0)
					(length 2.54)
					(name "VSSA")
					(number "8")
					(alternate "VFEF-" passive line)
					(alternate "_VREF-" passive line)
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDDA")
					(number "9")
					(alternate "VREF+" passive line)
					(alternate "_VREF+" passive line)
				)
				(pin bidirectional line
					(at 34.29 0 180)
					(length 2.54)
					(name "PA0")
					(number "10")
				)
				(pin bidirectional line
					(at 34.29 -2.54 180)
					(length 2.54)
					(name "PA1")
					(number "11")
				)
				(pin bidirectional line
					(at 34.29 -5.08 180)
					(length 2.54)
					(name "PA2")
					(number "12")
				)
				(pin bidirectional line
					(at 34.29 -7.62 180)
					(length 2.54)
					(name "PA3")
					(number "13")
				)
				(pin bidirectional line
					(at 34.29 -10.16 180)
					(length 2.54)
					(name "PA4")
					(number "14")
				)
				(pin bidirectional line
					(at 34.29 -12.7 180)
					(length 2.54)
					(name "PA5")
					(number "15")
				)
				(pin bidirectional line
					(at 34.29 -15.24 180)
					(length 2.54)
					(name "PA6")
					(number "16")
				)
				(pin bidirectional line
					(at 34.29 -17.78 180)
					(length 2.54)
					(name "PA7")
					(number "17")
				)
				(pin bidirectional line
					(at 34.29 -41.91 180)
					(length 2.54)
					(name "PB0")
					(number "18")
				)
				(pin bidirectional line
					(at 34.29 -44.45 180)
					(length 2.54)
					(name "PB1")
					(number "19")
				)
				(pin bidirectional line
					(at 34.29 -46.99 180)
					(length 2.54)
					(name "PB2")
					(number "20")
				)
				(pin bidirectional line
					(at 34.29 -67.31 180)
					(length 2.54)
					(name "PB10")
					(number "21")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VCAP_1")
					(number "22")
				)
				(pin power_in line
					(at 0 -72.39 0)
					(length 2.54)
					(name "VSS")
					(number "23")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "24")
				)
				(pin bidirectional line
					(at 34.29 -69.85 180)
					(length 2.54)
					(name "PB12")
					(number "25")
				)
				(pin bidirectional line
					(at 34.29 -72.39 180)
					(length 2.54)
					(name "PB13")
					(number "26")
				)
				(pin bidirectional line
					(at 34.29 -74.93 180)
					(length 2.54)
					(name "PB14")
					(number "27")
				)
				(pin bidirectional line
					(at 34.29 -77.47 180)
					(length 2.54)
					(name "PB15")
					(number "28")
				)
				(pin bidirectional line
					(at 34.29 -20.32 180)
					(length 2.54)
					(name "PA8")
					(number "29")
				)
				(pin bidirectional line
					(at 34.29 -22.86 180)
					(length 2.54)
					(name "PA9")
					(number "30")
				)
				(pin bidirectional line
					(at 34.29 -25.4 180)
					(length 2.54)
					(name "PA10")
					(number "31")
				)
				(pin bidirectional line
					(at 34.29 -27.94 180)
					(length 2.54)
					(name "PA11")
					(number "32")
				)
				(pin bidirectional line
					(at 34.29 -30.48 180)
					(length 2.54)
					(name "PA12")
					(number "33")
				)
				(pin bidirectional line
					(at 34.29 -33.02 180)
					(length 2.54)
					(name "PA13")
					(number "34")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "35")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "36")
				)
				(pin bidirectional line
					(at 34.29 -35.56 180)
					(length 2.54)
					(name "PA14")
					(number "37")
				)
				(pin bidirectional line
					(at 34.29 -38.1 180)
					(length 2.54)
					(name "PA15")
					(number "38")
				)
				(pin bidirectional line
					(at 34.29 -49.53 180)
					(length 2.54)
					(name "PB3")
					(number "39")
				)
				(pin bidirectional line
					(at 34.29 -52.07 180)
					(length 2.54)
					(name "PB4")
					(number "40")
				)
				(pin bidirectional line
					(at 34.29 -54.61 180)
					(length 2.54)
					(name "PB5")
					(number "41")
				)
				(pin bidirectional line
					(at 34.29 -57.15 180)
					(length 2.54)
					(name "PB6")
					(number "42")
				)
				(pin bidirectional line
					(at 34.29 -59.69 180)
					(length 2.54)
					(name "PB7")
					(number "43")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "BOOT0")
					(number "44")
				)
				(pin bidirectional line
					(at 34.29 -62.23 180)
					(length 2.54)
					(name "PB8")
					(number "45")
				)
				(pin passive line
					(at 34.29 -64.77 180)
					(length 2.54)
					(name "PB9")
					(number "46")
				)
				(pin passive line
					(at 0 -72.39 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "47")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "48")
				)
				(pin power_in line
					(at 0 -77.47 0)
					(length 2.54)
					(name "EP")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
