(footprint "BGA-64_5x5mm_Layout8x8_P0.5mm_Ball0.255mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-64_5x5mm_Layout8x8_P0.5mm_Ball0.255mm"
		(at 0 3.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.7 7 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1 5.7 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at 0.2 4.6 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -1.75 -1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -1.25 -1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -0.75 -1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at -0.25 -1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at 0.25 -1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at 0.75 -1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at 1.25 -1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at 1.75 -1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -1.75 -1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -1.25 -1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -0.75 -1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -0.25 -1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at 0.25 -1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at 0.75 -1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at 1.25 -1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at 1.75 -1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -1.75 -0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -1.25 -0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -0.75 -0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at -0.25 -0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at 0.25 -0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C6" smd circle
		(at 0.75 -0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C7" smd circle
		(at 1.25 -0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd circle
		(at 1.75 -0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -1.75 -0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -1.25 -0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -0.75 -0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at -0.25 -0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at 0.25 -0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at 0.75 -0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D7" smd circle
		(at 1.25 -0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at 1.75 -0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -1.75 0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -1.25 0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -0.75 0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at -0.25 0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at 0.25 0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E6" smd circle
		(at 0.75 0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E7" smd circle
		(at 1.25 0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E8" smd circle
		(at 1.75 0.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -1.75 0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -1.25 0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -0.75 0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at -0.25 0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at 0.25 0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F6" smd circle
		(at 0.75 0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F7" smd circle
		(at 1.25 0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F8" smd circle
		(at 1.75 0.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -1.75 1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -1.25 1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at -0.75 1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at -0.25 1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G5" smd circle
		(at 0.25 1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G6" smd circle
		(at 0.75 1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G7" smd circle
		(at 1.25 1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G8" smd circle
		(at 1.75 1.25)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -1.75 1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -1.25 1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -0.75 1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -0.25 1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H5" smd circle
		(at 0.25 1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H6" smd circle
		(at 0.75 1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H7" smd circle
		(at 1.25 1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H8" smd circle
		(at 1.75 1.75)
		(size 0.255 0.255)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_stm32g491rei6.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
