(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "STM32H753IIT6"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "STM32H753IIT6"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "STM32H753IIT6"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h753ii.pdf"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM MCU, LQFP-176, STM32 Family STM32H7 Series Microcontrollers, ARM Cortex-M7, 32 bit, 480 MHz, 2 MB Flash"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "STM32H753IIT6"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MICROCONTROLLER, IC, ARM, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "STM32H753IIT6_1_1"
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "PA0")
					(number "40")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 5.08)
					(name "PA1")
					(number "41")
				)
				(pin bidirectional line
					(at 0 -5.08 180)
					(length 5.08)
					(name "PA2")
					(number "42")
				)
				(pin bidirectional line
					(at 0 -7.62 180)
					(length 5.08)
					(name "PA3")
					(number "47")
				)
				(pin bidirectional line
					(at 0 -10.16 180)
					(length 5.08)
					(name "PA4")
					(number "50")
				)
				(pin bidirectional line
					(at 0 -12.7 180)
					(length 5.08)
					(name "PA5")
					(number "51")
				)
				(pin bidirectional line
					(at 0 -15.24 180)
					(length 5.08)
					(name "PA6")
					(number "52")
				)
				(pin bidirectional line
					(at 0 -17.78 180)
					(length 5.08)
					(name "PA7")
					(number "53")
				)
				(pin bidirectional line
					(at 0 -20.32 180)
					(length 5.08)
					(name "PA8")
					(number "119")
				)
				(pin bidirectional line
					(at 0 -22.86 180)
					(length 5.08)
					(name "PA9")
					(number "120")
				)
				(pin bidirectional line
					(at 0 -25.4 180)
					(length 5.08)
					(name "PA10")
					(number "121")
				)
				(pin bidirectional line
					(at 0 -27.94 180)
					(length 5.08)
					(name "PA11")
					(number "122")
				)
				(pin bidirectional line
					(at 0 -30.48 180)
					(length 5.08)
					(name "PA12")
					(number "123")
				)
				(pin bidirectional line
					(at 0 -33.02 180)
					(length 5.08)
					(name "PA13")
					(number "124")
				)
				(pin bidirectional line
					(at 0 -35.56 180)
					(length 5.08)
					(name "PA14")
					(number "137")
				)
				(pin bidirectional line
					(at 0 -38.1 180)
					(length 5.08)
					(name "PA15")
					(number "138")
				)
			)
			(symbol "STM32H753IIT6_2_1"
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "PB0")
					(number "56")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 5.08)
					(name "PB1")
					(number "57")
				)
				(pin bidirectional line
					(at 0 -5.08 180)
					(length 5.08)
					(name "PB2")
					(number "58")
				)
				(pin bidirectional line
					(at 0 -25.4 180)
					(length 5.08)
					(name "PB10")
					(number "79")
				)
				(pin bidirectional line
					(at 0 -27.94 180)
					(length 5.08)
					(name "PB11")
					(number "80")
				)
				(pin bidirectional line
					(at 0 -30.48 180)
					(length 5.08)
					(name "PB12")
					(number "92")
				)
				(pin bidirectional line
					(at 0 -33.02 180)
					(length 5.08)
					(name "PB13")
					(number "93")
				)
				(pin bidirectional line
					(at 0 -35.56 180)
					(length 5.08)
					(name "PB14")
					(number "94")
				)
				(pin bidirectional line
					(at 0 -38.1 180)
					(length 5.08)
					(name "PB15")
					(number "95")
				)
				(pin bidirectional line
					(at 0 -7.62 180)
					(length 5.08)
					(name "PB3")
					(number "161")
				)
				(pin bidirectional line
					(at 0 -10.16 180)
					(length 5.08)
					(name "PB4")
					(number "162")
				)
				(pin bidirectional line
					(at 0 -12.7 180)
					(length 5.08)
					(name "PB5")
					(number "163")
				)
				(pin bidirectional line
					(at 0 -15.24 180)
					(length 5.08)
					(name "PB6")
					(number "164")
				)
				(pin bidirectional line
					(at 0 -17.78 180)
					(length 5.08)
					(name "PB7")
					(number "165")
				)
				(pin bidirectional line
					(at 0 -20.32 180)
					(length 5.08)
					(name "PB8")
					(number "167")
				)
				(pin bidirectional line
					(at 0 -22.86 180)
					(length 5.08)
					(name "PB9")
					(number "168")
				)
			)
			(symbol "STM32H753IIT6_3_1"
				(pin bidirectional line
					(at 0 -33.02 180)
					(length 5.08)
					(name "PC13")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -35.56 180)
					(length 5.08)
					(name "PC14-OSC32_IN")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -38.1 180)
					(length 5.08)
					(name "PC15-OSC32_OUT")
					(number "10")
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "PC0")
					(number "32")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 5.08)
					(name "PC1")
					(number "33")
				)
				(pin bidirectional line
					(at 0 -5.08 180)
					(length 5.08)
					(name "PC2_C")
					(number "34")
				)
				(pin bidirectional line
					(at 0 -7.62 180)
					(length 5.08)
					(name "PC3_C")
					(number "35")
				)
				(pin bidirectional line
					(at 0 -10.16 180)
					(length 5.08)
					(name "PC4")
					(number "54")
				)
				(pin bidirectional line
					(at 0 -12.7 180)
					(length 5.08)
					(name "PC5")
					(number "55")
				)
				(pin bidirectional line
					(at 0 -15.24 180)
					(length 5.08)
					(name "PC6")
					(number "115")
				)
				(pin bidirectional line
					(at 0 -17.78 180)
					(length 5.08)
					(name "PC7")
					(number "116")
				)
				(pin bidirectional line
					(at 0 -20.32 180)
					(length 5.08)
					(name "PC8")
					(number "117")
				)
				(pin bidirectional line
					(at 0 -22.86 180)
					(length 5.08)
					(name "PC9")
					(number "118")
				)
				(pin bidirectional line
					(at 0 -25.4 180)
					(length 5.08)
					(name "PC10")
					(number "139")
				)
				(pin bidirectional line
					(at 0 -27.94 180)
					(length 5.08)
					(name "PC11")
					(number "140")
				)
				(pin bidirectional line
					(at 0 -30.48 180)
					(length 5.08)
					(name "PC12")
					(number "141")
				)
			)
			(symbol "STM32H753IIT6_4_1"
				(pin bidirectional line
					(at 0 -20.32 180)
					(length 5.08)
					(name "PD8")
					(number "96")
				)
				(pin bidirectional line
					(at 0 -22.86 180)
					(length 5.08)
					(name "PD9")
					(number "97")
				)
				(pin bidirectional line
					(at 0 -25.4 180)
					(length 5.08)
					(name "PD10")
					(number "98")
				)
				(pin bidirectional line
					(at 0 -27.94 180)
					(length 5.08)
					(name "PD11")
					(number "99")
				)
				(pin bidirectional line
					(at 0 -30.48 180)
					(length 5.08)
					(name "PD12")
					(number "100")
				)
				(pin bidirectional line
					(at 0 -33.02 180)
					(length 5.08)
					(name "PD13")
					(number "101")
				)
				(pin bidirectional line
					(at 0 -35.56 180)
					(length 5.08)
					(name "PD14")
					(number "104")
				)
				(pin bidirectional line
					(at 0 -38.1 180)
					(length 5.08)
					(name "PD15")
					(number "105")
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "PD0")
					(number "142")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 5.08)
					(name "PD1")
					(number "143")
				)
				(pin bidirectional line
					(at 0 -5.08 180)
					(length 5.08)
					(name "PD2")
					(number "144")
				)
				(pin bidirectional line
					(at 0 -7.62 180)
					(length 5.08)
					(name "PD3")
					(number "145")
				)
				(pin bidirectional line
					(at 0 -10.16 180)
					(length 5.08)
					(name "PD4")
					(number "146")
				)
				(pin bidirectional line
					(at 0 -12.7 180)
					(length 5.08)
					(name "PD5")
					(number "147")
				)
				(pin bidirectional line
					(at 0 -15.24 180)
					(length 5.08)
					(name "PD6")
					(number "150")
				)
				(pin bidirectional line
					(at 0 -17.78 180)
					(length 5.08)
					(name "PD7")
					(number "151")
				)
			)
			(symbol "STM32H753IIT6_5_1"
				(pin bidirectional line
					(at 0 -5.08 180)
					(length 5.08)
					(name "PE2")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -7.62 180)
					(length 5.08)
					(name "PE3")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -10.16 180)
					(length 5.08)
					(name "PE4")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -12.7 180)
					(length 5.08)
					(name "PE5")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -15.24 180)
					(length 5.08)
					(name "PE6")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -17.78 180)
					(length 5.08)
					(name "PE7")
					(number "68")
				)
				(pin bidirectional line
					(at 0 -20.32 180)
					(length 5.08)
					(name "PE8")
					(number "69")
				)
				(pin bidirectional line
					(at 0 -22.86 180)
					(length 5.08)
					(name "PE9")
					(number "70")
				)
				(pin bidirectional line
					(at 0 -25.4 180)
					(length 5.08)
					(name "PE10")
					(number "73")
				)
				(pin bidirectional line
					(at 0 -27.94 180)
					(length 5.08)
					(name "PE11")
					(number "74")
				)
				(pin bidirectional line
					(at 0 -30.48 180)
					(length 5.08)
					(name "PE12")
					(number "75")
				)
				(pin bidirectional line
					(at 0 -33.02 180)
					(length 5.08)
					(name "PE13")
					(number "76")
				)
				(pin bidirectional line
					(at 0 -35.56 180)
					(length 5.08)
					(name "PE14")
					(number "77")
				)
				(pin bidirectional line
					(at 0 -38.1 180)
					(length 5.08)
					(name "PE15")
					(number "78")
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "PE0")
					(number "169")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 5.08)
					(name "PE1")
					(number "170")
				)
			)
			(symbol "STM32H753IIT6_6_1"
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "PF0")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 5.08)
					(name "PF1")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -5.08 180)
					(length 5.08)
					(name "PF2")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -7.62 180)
					(length 5.08)
					(name "PF3")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -10.16 180)
					(length 5.08)
					(name "PF4")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -12.7 180)
					(length 5.08)
					(name "PF5")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -15.24 180)
					(length 5.08)
					(name "PF6")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -17.78 180)
					(length 5.08)
					(name "PF7")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -20.32 180)
					(length 5.08)
					(name "PF8")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -22.86 180)
					(length 5.08)
					(name "PF9")
					(number "27")
				)
				(pin bidirectional line
					(at 0 -25.4 180)
					(length 5.08)
					(name "PF10")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -27.94 180)
					(length 5.08)
					(name "PF11")
					(number "59")
				)
				(pin bidirectional line
					(at 0 -30.48 180)
					(length 5.08)
					(name "PF12")
					(number "60")
				)
				(pin bidirectional line
					(at 0 -33.02 180)
					(length 5.08)
					(name "PF13")
					(number "63")
				)
				(pin bidirectional line
					(at 0 -35.56 180)
					(length 5.08)
					(name "PF14")
					(number "64")
				)
				(pin bidirectional line
					(at 0 -38.1 180)
					(length 5.08)
					(name "PF15")
					(number "65")
				)
			)
			(symbol "STM32H753IIT6_7_1"
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "PG0")
					(number "66")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 5.08)
					(name "PG1")
					(number "67")
				)
				(pin bidirectional line
					(at 0 -5.08 180)
					(length 5.08)
					(name "PG2")
					(number "106")
				)
				(pin bidirectional line
					(at 0 -7.62 180)
					(length 5.08)
					(name "PG3")
					(number "107")
				)
				(pin bidirectional line
					(at 0 -10.16 180)
					(length 5.08)
					(name "PG4")
					(number "108")
				)
				(pin bidirectional line
					(at 0 -12.7 180)
					(length 5.08)
					(name "PG5")
					(number "109")
				)
				(pin bidirectional line
					(at 0 -15.24 180)
					(length 5.08)
					(name "PG6")
					(number "110")
				)
				(pin bidirectional line
					(at 0 -17.78 180)
					(length 5.08)
					(name "PG7")
					(number "111")
				)
				(pin bidirectional line
					(at 0 -20.32 180)
					(length 5.08)
					(name "PG8")
					(number "112")
				)
				(pin bidirectional line
					(at 0 -22.86 180)
					(length 5.08)
					(name "PG9")
					(number "152")
				)
				(pin bidirectional line
					(at 0 -25.4 180)
					(length 5.08)
					(name "PG10")
					(number "153")
				)
				(pin bidirectional line
					(at 0 -27.94 180)
					(length 5.08)
					(name "PG11")
					(number "154")
				)
				(pin bidirectional line
					(at 0 -30.48 180)
					(length 5.08)
					(name "PG12")
					(number "155")
				)
				(pin bidirectional line
					(at 0 -33.02 180)
					(length 5.08)
					(name "PG13")
					(number "156")
				)
				(pin bidirectional line
					(at 0 -35.56 180)
					(length 5.08)
					(name "PG14")
					(number "157")
				)
				(pin bidirectional line
					(at 0 -38.1 180)
					(length 5.08)
					(name "PG15")
					(number "160")
				)
			)
			(symbol "STM32H753IIT6_8_1"
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "PH0-OSC_IN")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 5.08)
					(name "PH1-OSC_OUT")
					(number "30")
				)
				(pin bidirectional line
					(at 0 -5.08 180)
					(length 5.08)
					(name "PH2")
					(number "43")
				)
				(pin bidirectional line
					(at 0 -7.62 180)
					(length 5.08)
					(name "PH3")
					(number "44")
				)
				(pin bidirectional line
					(at 0 -10.16 180)
					(length 5.08)
					(name "PH4")
					(number "45")
				)
				(pin bidirectional line
					(at 0 -12.7 180)
					(length 5.08)
					(name "PH5")
					(number "46")
				)
				(pin bidirectional line
					(at 0 -15.24 180)
					(length 5.08)
					(name "PH6")
					(number "83")
				)
				(pin bidirectional line
					(at 0 -17.78 180)
					(length 5.08)
					(name "PH7")
					(number "84")
				)
				(pin bidirectional line
					(at 0 -20.32 180)
					(length 5.08)
					(name "PH8")
					(number "85")
				)
				(pin bidirectional line
					(at 0 -22.86 180)
					(length 5.08)
					(name "PH9")
					(number "86")
				)
				(pin bidirectional line
					(at 0 -25.4 180)
					(length 5.08)
					(name "PH10")
					(number "87")
				)
				(pin bidirectional line
					(at 0 -27.94 180)
					(length 5.08)
					(name "PH11")
					(number "88")
				)
				(pin bidirectional line
					(at 0 -30.48 180)
					(length 5.08)
					(name "PH12")
					(number "89")
				)
				(pin bidirectional line
					(at 0 -33.02 180)
					(length 5.08)
					(name "PH13")
					(number "128")
				)
				(pin bidirectional line
					(at 0 -35.56 180)
					(length 5.08)
					(name "PH14")
					(number "129")
				)
				(pin bidirectional line
					(at 0 -38.1 180)
					(length 5.08)
					(name "PH15")
					(number "130")
				)
			)
			(symbol "STM32H753IIT6_9_1"
				(pin bidirectional line
					(at 0 -20.32 180)
					(length 5.08)
					(name "PI8")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -22.86 180)
					(length 5.08)
					(name "PI9")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -25.4 180)
					(length 5.08)
					(name "PI10")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -27.94 180)
					(length 5.08)
					(name "PI11")
					(number "13")
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "PI0")
					(number "131")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 5.08)
					(name "PI1")
					(number "132")
				)
				(pin bidirectional line
					(at 0 -5.08 180)
					(length 5.08)
					(name "PI2")
					(number "133")
				)
				(pin bidirectional line
					(at 0 -7.62 180)
					(length 5.08)
					(name "PI3")
					(number "134")
				)
				(pin bidirectional line
					(at 0 -10.16 180)
					(length 5.08)
					(name "PI4")
					(number "173")
				)
				(pin bidirectional line
					(at 0 -12.7 180)
					(length 5.08)
					(name "PI5")
					(number "174")
				)
				(pin bidirectional line
					(at 0 -15.24 180)
					(length 5.08)
					(name "PI6")
					(number "175")
				)
				(pin bidirectional line
					(at 0 -17.78 180)
					(length 5.08)
					(name "PI7")
					(number "176")
				)
			)
			(symbol "STM32H753IIT6_10_1"
				(pin power_in line
					(at 30.48 0 180)
					(length 5.08)
					(name "VBAT")
					(number "6")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 5.08)
					(name "VSS")
					(number "14")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VDD")
					(number "15")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "22")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "23")
				)
				(pin input line
					(at 30.48 -35.56 180)
					(length 5.08)
					(name "NRST")
					(number "31")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "36")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "VSSA")
					(number "37")
				)
				(pin power_in line
					(at 30.48 -20.32 180)
					(length 5.08)
					(name "VREF+")
					(number "38")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "VDDA")
					(number "39")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "48")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "49")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "61")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "62")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "71")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "72")
				)
				(pin power_out line
					(at 30.48 -10.16 180)
					(length 5.08)
					(name "VCAP")
					(number "81")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "82")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "90")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "91")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "102")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "103")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "113")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 5.08)
					(name "VDD33USB")
					(number "114")
				)
				(pin passive line
					(at 30.48 -10.16 180)
					(length 5.08)
					(hide yes)
					(name "VCAP")
					(number "125")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "126")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "127")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "135")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "136")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "148")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "149")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "158")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "159")
				)
				(pin input line
					(at 30.48 -38.1 180)
					(length 5.08)
					(name "BOOT0")
					(number "166")
				)
				(pin input line
					(at 30.48 -33.02 180)
					(length 5.08)
					(name "PDR_ON")
					(number "171")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "172")
				)
			)
			(embedded_fonts no)
		)
)
