(footprint "LQFP-100_14x14mm_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -8.6 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "LQFP-100_14x14mm_P0.5mm"
		(at 0 9.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -9.1 10.4 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -9.1 11.6 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -9.1 12.8 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -7.75 -6)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "2" smd rect
		(at -7.75 -5.5)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "3" smd rect
		(at -7.75 -5)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "4" smd rect
		(at -7.75 -4.5)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "5" smd rect
		(at -7.75 -4)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "6" smd rect
		(at -7.75 -3.5)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "7" smd rect
		(at -7.75 -3)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "8" smd rect
		(at -7.75 -2.5)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "9" smd rect
		(at -7.75 -2)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "10" smd rect
		(at -7.75 -1.5)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "11" smd rect
		(at -7.75 -1)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "12" smd rect
		(at -7.75 -0.5)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "13" smd rect
		(at -7.75 0)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "14" smd rect
		(at -7.75 0.5)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "15" smd rect
		(at -7.75 1)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "16" smd rect
		(at -7.75 1.5)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "17" smd rect
		(at -7.75 2)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "18" smd rect
		(at -7.75 2.5)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "19" smd rect
		(at -7.75 3)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "20" smd rect
		(at -7.75 3.5)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "21" smd rect
		(at -7.75 4)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "22" smd rect
		(at -7.75 4.5)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "23" smd rect
		(at -7.75 5)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "24" smd rect
		(at -7.75 5.5)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "25" smd rect
		(at -7.75 6)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "26" smd rect
		(at -6 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "27" smd rect
		(at -5.5 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "28" smd rect
		(at -5 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "29" smd rect
		(at -4.5 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "30" smd rect
		(at -4 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "31" smd rect
		(at -3.5 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "32" smd rect
		(at -3 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "33" smd rect
		(at -2.5 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "34" smd rect
		(at -2 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "35" smd rect
		(at -1.5 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "36" smd rect
		(at -1 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "37" smd rect
		(at -0.5 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "38" smd rect
		(at 0 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "39" smd rect
		(at 0.5 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "40" smd rect
		(at 1 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "41" smd rect
		(at 1.5 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "42" smd rect
		(at 2 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "43" smd rect
		(at 2.5 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "44" smd rect
		(at 3 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "45" smd rect
		(at 3.5 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "46" smd rect
		(at 4 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "47" smd rect
		(at 4.5 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "48" smd rect
		(at 5 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "49" smd rect
		(at 5.5 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "50" smd rect
		(at 6 7.75 90)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "51" smd rect
		(at 7.75 6 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "52" smd rect
		(at 7.75 5.5 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "53" smd rect
		(at 7.75 5 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "54" smd rect
		(at 7.75 4.5 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "55" smd rect
		(at 7.75 4 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "56" smd rect
		(at 7.75 3.5 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "57" smd rect
		(at 7.75 3 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "58" smd rect
		(at 7.75 2.5 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "59" smd rect
		(at 7.75 2 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "60" smd rect
		(at 7.75 1.5 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "61" smd rect
		(at 7.75 1 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "62" smd rect
		(at 7.75 0.5 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "63" smd rect
		(at 7.75 0 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "64" smd rect
		(at 7.75 -0.5 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "65" smd rect
		(at 7.75 -1 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "66" smd rect
		(at 7.75 -1.5 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "67" smd rect
		(at 7.75 -2 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "68" smd rect
		(at 7.75 -2.5 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "69" smd rect
		(at 7.75 -3 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "70" smd rect
		(at 7.75 -3.5 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "71" smd rect
		(at 7.75 -4 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "72" smd rect
		(at 7.75 -4.5 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "73" smd rect
		(at 7.75 -5 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "74" smd rect
		(at 7.75 -5.5 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "75" smd rect
		(at 7.75 -6 180)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "76" smd rect
		(at 6 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "77" smd rect
		(at 5.5 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "78" smd rect
		(at 5 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "79" smd rect
		(at 4.5 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "80" smd rect
		(at 4 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "81" smd rect
		(at 3.5 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "82" smd rect
		(at 3 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "83" smd rect
		(at 2.5 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "84" smd rect
		(at 2 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "85" smd rect
		(at 1.5 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "86" smd rect
		(at 1 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "87" smd rect
		(at 0.5 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "88" smd rect
		(at 0 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "89" smd rect
		(at -0.5 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "90" smd rect
		(at -1 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "91" smd rect
		(at -1.5 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "92" smd rect
		(at -2 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "93" smd rect
		(at -2.5 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "94" smd rect
		(at -3 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "95" smd rect
		(at -3.5 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "96" smd rect
		(at -4 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "97" smd rect
		(at -4.5 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "98" smd rect
		(at -5 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "99" smd rect
		(at -5.5 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(pad "100" smd rect
		(at -6 -7.75 270)
		(size 1.1938 0.3048)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0508)
	)
	(embedded_fonts no)
	(model "antmicro_stm32l073v8t6.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
