(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "STM32L073V8T6"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "STM32L073V8T6"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "STM32L073V8T6"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.st.com/content/ccc/resource/technical/document/datasheet/d8/b3/7b/dc/18/22/44/f5/DM00141036.pdf/files/DM00141036.pdf/jcr:content/translations/en.DM00141036.pdf"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM® Cortex®-M0+ STM32L0 Microcontroller IC 32-Bit Single-Core 32MHz 64KB (64K x 8) FLASH 100-LQFP (14x14)"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "STM32L073V8T6"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, MICROCONTROLLER, IC, ARM, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "STM32L073V8T6_1_1"
				(pin bidirectional line
					(at 30.48 -33.02 180)
					(length 3.81)
					(name "PC13")
					(number "7")
				)
				(pin bidirectional line
					(at 30.48 0 180)
					(length 3.81)
					(name "PC0")
					(number "15")
				)
				(pin bidirectional line
					(at 30.48 -2.54 180)
					(length 3.81)
					(name "PC1")
					(number "16")
				)
				(pin bidirectional line
					(at 30.48 -5.08 180)
					(length 3.81)
					(name "PC2")
					(number "17")
				)
				(pin bidirectional line
					(at 30.48 -7.62 180)
					(length 3.81)
					(name "PC3")
					(number "18")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PA0")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PA1")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PA2")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PA3")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PA4")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PA5")
					(number "30")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PA6")
					(number "31")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PA7")
					(number "32")
				)
				(pin bidirectional line
					(at 30.48 -10.16 180)
					(length 3.81)
					(name "PC4")
					(number "33")
				)
				(pin bidirectional line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "PC5")
					(number "34")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PB0")
					(number "35")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PB1")
					(number "36")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PB2")
					(number "37")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 3.81)
					(name "PB10")
					(number "47")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "PB11")
					(number "48")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 3.81)
					(name "PB12")
					(number "51")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 3.81)
					(name "PB13")
					(number "52")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 3.81)
					(name "PB14")
					(number "53")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 3.81)
					(name "PB15")
					(number "54")
				)
				(pin bidirectional line
					(at 30.48 -63.5 180)
					(length 3.81)
					(name "PD8")
					(number "55")
				)
				(pin bidirectional line
					(at 30.48 -66.04 180)
					(length 3.81)
					(name "PD9")
					(number "56")
				)
				(pin bidirectional line
					(at 30.48 -68.58 180)
					(length 3.81)
					(name "PD10")
					(number "57")
				)
				(pin bidirectional line
					(at 30.48 -71.12 180)
					(length 3.81)
					(name "PD11")
					(number "58")
				)
				(pin bidirectional line
					(at 30.48 -73.66 180)
					(length 3.81)
					(name "PD12")
					(number "59")
				)
				(pin bidirectional line
					(at 30.48 -76.2 180)
					(length 3.81)
					(name "PD13")
					(number "60")
				)
				(pin bidirectional line
					(at 30.48 -78.74 180)
					(length 3.81)
					(name "PD14")
					(number "61")
				)
				(pin bidirectional line
					(at 30.48 -81.28 180)
					(length 3.81)
					(name "PD15")
					(number "62")
				)
				(pin bidirectional line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "PC6")
					(number "63")
				)
				(pin bidirectional line
					(at 30.48 -17.78 180)
					(length 3.81)
					(name "PC7")
					(number "64")
				)
				(pin bidirectional line
					(at 30.48 -20.32 180)
					(length 3.81)
					(name "PC8")
					(number "65")
				)
				(pin bidirectional line
					(at 30.48 -22.86 180)
					(length 3.81)
					(name "PC9")
					(number "66")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PA8")
					(number "67")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PA9")
					(number "68")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PA10")
					(number "69")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PA11")
					(number "70")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PA12")
					(number "71")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PA13")
					(number "72")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PA14")
					(number "76")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PA15")
					(number "77")
				)
				(pin bidirectional line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "PC10")
					(number "78")
				)
				(pin bidirectional line
					(at 30.48 -27.94 180)
					(length 3.81)
					(name "PC11")
					(number "79")
				)
				(pin bidirectional line
					(at 30.48 -30.48 180)
					(length 3.81)
					(name "PC12")
					(number "80")
				)
				(pin bidirectional line
					(at 30.48 -43.18 180)
					(length 3.81)
					(name "PD0")
					(number "81")
				)
				(pin bidirectional line
					(at 30.48 -45.72 180)
					(length 3.81)
					(name "PD1")
					(number "82")
				)
				(pin bidirectional line
					(at 30.48 -48.26 180)
					(length 3.81)
					(name "PD2")
					(number "83")
				)
				(pin bidirectional line
					(at 30.48 -50.8 180)
					(length 3.81)
					(name "PD3")
					(number "84")
				)
				(pin bidirectional line
					(at 30.48 -53.34 180)
					(length 3.81)
					(name "PD4")
					(number "85")
				)
				(pin bidirectional line
					(at 30.48 -55.88 180)
					(length 3.81)
					(name "PD5")
					(number "86")
				)
				(pin bidirectional line
					(at 30.48 -58.42 180)
					(length 3.81)
					(name "PD6")
					(number "87")
				)
				(pin bidirectional line
					(at 30.48 -60.96 180)
					(length 3.81)
					(name "PD7")
					(number "88")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PB3")
					(number "89")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PB4")
					(number "90")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PB5")
					(number "91")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "PB6")
					(number "92")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "PB7")
					(number "93")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 3.81)
					(name "PB8")
					(number "95")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 3.81)
					(name "PB9")
					(number "96")
				)
			)
			(symbol "STM32L073V8T6_2_1"
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PE2")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PE3")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PE4")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PE5")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PE6")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PE7")
					(number "38")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PE8")
					(number "39")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PE9")
					(number "40")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PE10")
					(number "41")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PE11")
					(number "42")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PE12")
					(number "43")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PE13")
					(number "44")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PE14")
					(number "45")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PE15")
					(number "46")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PE0")
					(number "97")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PE1")
					(number "98")
				)
			)
			(symbol "STM32L073V8T6_3_1"
				(pin power_in line
					(at 31.75 -8.89 180)
					(length 3.81)
					(name "VLCD")
					(number "6")
				)
				(pin bidirectional line
					(at 31.75 -21.59 180)
					(length 3.81)
					(name "PC14-OSC32_IN")
					(number "8")
				)
				(pin bidirectional line
					(at 31.75 -19.05 180)
					(length 3.81)
					(name "PC15-OSC32_OUT")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PH9")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PH10")
					(number "11")
				)
				(pin bidirectional line
					(at 31.75 -15.24 180)
					(length 3.81)
					(name "PH0-OSC_IN")
					(number "12")
				)
				(pin bidirectional line
					(at 31.75 -12.7 180)
					(length 3.81)
					(name "PH1-OSC_OUT")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "NRST")
					(number "14")
				)
				(pin power_in line
					(at 0 -19.05 0)
					(length 3.81)
					(name "VSSA")
					(number "19")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VREF-")
					(number "20")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VREF+")
					(number "21")
				)
				(pin power_in line
					(at 31.75 -2.54 180)
					(length 3.81)
					(name "VDDA")
					(number "22")
				)
				(pin power_in line
					(at 0 -21.59 0)
					(length 3.81)
					(name "VSS")
					(number "27")
				)
				(pin passive line
					(at 31.75 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "28")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "49")
				)
				(pin passive line
					(at 31.75 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "50")
				)
				(pin passive line
					(at 31.75 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "73")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "74")
				)
				(pin power_in line
					(at 31.75 -6.35 180)
					(length 3.81)
					(name "VDD_USB")
					(number "75")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "BOOT0")
					(number "94")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "99")
				)
				(pin power_in line
					(at 31.75 0 180)
					(length 3.81)
					(name "VDD")
					(number "100")
				)
			)
			(embedded_fonts no)
		)
)
