(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "STM32L100RBT6"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "STM32L100RBT6"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "STM32L100RBT6"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.st.com/en/microcontrollers-microprocessors/stm32l100rb.html"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM MCU, STM32 Family STM32L1 Series Microcontrollers, ARM Cortex-M3, 32 bit, 16 MHz, 128 KB"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "STM32L100RBT6"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MICROCONTROLLER, IC, ARM, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "STM32L100RBT6_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VLCD")
					(number "1")
				)
				(pin bidirectional line
					(at 38.1 -76.2 180)
					(length 2.54)
					(name "PC13-WKUP2")
					(number "2")
					(alternate "RTC_OUT" passive line)
					(alternate "RTC_TAMP1" passive line)
					(alternate "RTC_TS" passive line)
					(alternate "WKUP2" passive line)
				)
				(pin passive line
					(at 38.1 -78.74 180)
					(length 2.54)
					(name "PC14-OSC32_IN")
					(number "3")
					(alternate "OSC32_IN" passive line)
				)
				(pin passive line
					(at 38.1 -81.28 180)
					(length 2.54)
					(name "PC15-OSC32_OUT")
					(number "4")
					(alternate "OSC32_OUT" passive line)
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 2.54)
					(name "PH0-OSC_IN")
					(number "5")
					(alternate "OSC_IN" passive line)
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(name "PH1-OSC_OUT")
					(number "6")
					(alternate "OSC_OUT" passive line)
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "NRST")
					(number "7")
				)
				(pin bidirectional line
					(at 38.1 -43.18 180)
					(length 2.54)
					(name "PC0")
					(number "8")
					(alternate "ADC_IN10" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG18" passive line)
				)
				(pin bidirectional line
					(at 38.1 -45.72 180)
					(length 2.54)
					(name "PC1")
					(number "9")
					(alternate "ADC_IN11" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG19" passive line)
				)
				(pin bidirectional line
					(at 38.1 -48.26 180)
					(length 2.54)
					(name "PC2")
					(number "10")
					(alternate "ADC_IN12" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG20" passive line)
				)
				(pin bidirectional line
					(at 38.1 -50.8 180)
					(length 2.54)
					(name "PC3")
					(number "11")
					(alternate "ADC_IN13" passive line)
					(alternate "BOOT0" bidirectional line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG21" passive line)
				)
				(pin power_in line
					(at 0 -81.28 0)
					(length 2.54)
					(name "VSSA")
					(number "12")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDDA")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "PA0-WKUP1")
					(number "14")
					(alternate "ADC_IN0" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "TIM2_CH1_ETR" passive line)
					(alternate "USART2_CTS" passive line)
					(alternate "WKUP1" passive line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "PA1")
					(number "15")
					(alternate "ADC_IN1" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG0" passive line)
					(alternate "TIM2_CH2" passive line)
					(alternate "USART2_RTS" passive line)
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "PA2")
					(number "16")
					(alternate "ADC_IN2" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG1" passive line)
					(alternate "TIM2_CH3" passive line)
					(alternate "TIM9_CH1" passive line)
					(alternate "USART2_TX" passive line)
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "PA3")
					(number "17")
					(alternate "ADC_IN3" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG2" passive line)
					(alternate "OSC32_IN" input line)
					(alternate "TIM2_CH4" passive line)
					(alternate "TIM9_CH2" passive line)
					(alternate "USART2_RX" passive line)
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 2.54)
					(name "VSS")
					(number "18")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "PA4")
					(number "20")
					(alternate "ADC_IN4" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "DAC_OUT1" passive line)
					(alternate "SPI1_NSS" passive line)
					(alternate "USART2_CK" passive line)
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "PA5")
					(number "21")
					(alternate "ADC_IN5" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "DAC_OUT2" passive line)
					(alternate "SPI1_SCK" passive line)
					(alternate "TIM2_CH1_ETR" passive line)
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "PA6")
					(number "22")
					(alternate "ADC_IN6" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG3" passive line)
					(alternate "SPI1_MISO" passive line)
					(alternate "TIM10_CH1" passive line)
					(alternate "TIM3_CH1" passive line)
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "PA7")
					(number "23")
					(alternate "ADC_IN7" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG4" passive line)
					(alternate "SPI1_MOSI" passive line)
					(alternate "TIM11_CH1" passive line)
					(alternate "TIM3_CH2" passive line)
				)
				(pin bidirectional line
					(at 38.1 -53.34 180)
					(length 2.54)
					(name "PC4")
					(number "24")
					(alternate "ADC_IN14" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG22" passive line)
				)
				(pin bidirectional line
					(at 38.1 -55.88 180)
					(length 2.54)
					(name "PC5")
					(number "25")
					(alternate "ADC_IN15" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG23" passive line)
					(alternate "OSC32_OUT" output line)
				)
				(pin bidirectional line
					(at 38.1 0 180)
					(length 2.54)
					(name "PB0")
					(number "26")
					(alternate "ADC_IN8" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG5" passive line)
					(alternate "PG10" bidirectional line)
					(alternate "TIM3_CH3" passive line)
					(alternate "VREF_OUT" passive line)
				)
				(pin bidirectional line
					(at 38.1 -2.54 180)
					(length 2.54)
					(name "PB1")
					(number "27")
					(alternate "ADC_IN9" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG6" passive line)
					(alternate "TIM3_CH4" passive line)
					(alternate "VREF_OUT" passive line)
				)
				(pin bidirectional line
					(at 38.1 -5.08 180)
					(length 2.54)
					(name "PB2")
					(number "28")
					(alternate "BOOT1" passive line)
				)
				(pin bidirectional line
					(at 38.1 -25.4 180)
					(length 2.54)
					(name "PB10")
					(number "29")
					(alternate "I2C2_SCL" passive line)
					(alternate "LCD_SEG10" passive line)
					(alternate "TIM2_CH3" passive line)
					(alternate "USART3_TX" passive line)
				)
				(pin bidirectional line
					(at 38.1 -27.94 180)
					(length 2.54)
					(name "PB11")
					(number "30")
					(alternate "I2C2_SDA" passive line)
					(alternate "LCD_SEG11" passive line)
					(alternate "TIM2_CH4" passive line)
					(alternate "USART3_RX" passive line)
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "31")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "32")
				)
				(pin bidirectional line
					(at 38.1 -30.48 180)
					(length 2.54)
					(name "PB12")
					(number "33")
					(alternate "ADC_IN18" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "I2C2_SMBA" passive line)
					(alternate "LCD_SEG12" passive line)
					(alternate "OSC_IN" power_in line)
					(alternate "SPI2_NSS" passive line)
					(alternate "TIM10_CH1" passive line)
					(alternate "USART3_CK" passive line)
				)
				(pin bidirectional line
					(at 38.1 -33.02 180)
					(length 2.54)
					(name "PB13")
					(number "34")
					(alternate "ADC_IN19" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG13" passive line)
					(alternate "SPI2_SCK" passive line)
					(alternate "TIM9_CH1" passive line)
					(alternate "USART3_CTS" passive line)
				)
				(pin bidirectional line
					(at 38.1 -35.56 180)
					(length 2.54)
					(name "PB14")
					(number "35")
					(alternate "ADC_IN20" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG14" passive line)
					(alternate "SPI2_MISO" passive line)
					(alternate "TIM9_CH2" passive line)
					(alternate "USART3_RTS" passive line)
				)
				(pin bidirectional line
					(at 38.1 -38.1 180)
					(length 2.54)
					(name "PB15")
					(number "36")
					(alternate "ADC_IN21" passive line)
					(alternate "COMP1_INP" passive line)
					(alternate "LCD_SEG15" passive line)
					(alternate "RTC_REFIN" passive line)
					(alternate "SPI2_MOSI" passive line)
					(alternate "TIM11_CH1" passive line)
				)
				(pin bidirectional line
					(at 38.1 -58.42 180)
					(length 2.54)
					(name "PC6")
					(number "37")
					(alternate "LCD_SEG24" passive line)
					(alternate "TIM3_CH1" passive line)
				)
				(pin bidirectional line
					(at 38.1 -60.96 180)
					(length 2.54)
					(name "PC7")
					(number "38")
					(alternate "LCD_SEG25" passive line)
					(alternate "TIM3_CH2" passive line)
				)
				(pin bidirectional line
					(at 38.1 -63.5 180)
					(length 2.54)
					(name "PC8")
					(number "39")
					(alternate "LCD_SEG26" passive line)
					(alternate "TIM3_CH3" passive line)
				)
				(pin bidirectional line
					(at 38.1 -66.04 180)
					(length 2.54)
					(name "PC9")
					(number "40")
					(alternate "LCD_SEG27" passive line)
					(alternate "TIM3_CH4" passive line)
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "PA8")
					(number "41")
					(alternate "LCD_COM0" passive line)
					(alternate "MCO" passive line)
					(alternate "OSC_OUT" output line)
					(alternate "USART1_CK" passive line)
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "PA9")
					(number "42")
					(alternate "LCD_COM1" passive line)
					(alternate "USART1_TX" passive line)
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "PA10")
					(number "43")
					(alternate "LCD_COM2" passive line)
					(alternate "USART1_RX" passive line)
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "PA11")
					(number "44")
					(alternate "SPI1_MISO" passive line)
					(alternate "USART1_CTS" passive line)
					(alternate "USB_DM" passive line)
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "PA12")
					(number "45")
					(alternate "SPI1_MOSI" passive line)
					(alternate "USART1_RTS" passive line)
					(alternate "USB_DP" passive line)
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "PA13")
					(number "46")
					(alternate "JTMS-SWDIO" passive line)
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "47")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "48")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "PA14")
					(number "49")
					(alternate "JTCK-SWCLK" passive line)
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "PA15")
					(number "50")
					(alternate "JTDI" passive line)
					(alternate "LCD_SEG17" passive line)
					(alternate "PA15" passive line)
					(alternate "SPI1_NSS" passive line)
					(alternate "TIM2_CH1_ETR" passive line)
				)
				(pin bidirectional line
					(at 38.1 -68.58 180)
					(length 2.54)
					(name "PC10")
					(number "51")
					(alternate "LCD_COM4" passive line)
					(alternate "LCD_SEG28" passive line)
					(alternate "LCD_SEG40" passive line)
					(alternate "USART3_TX" passive line)
				)
				(pin bidirectional line
					(at 38.1 -71.12 180)
					(length 2.54)
					(name "PC11")
					(number "52")
					(alternate "LCD_COM5" passive line)
					(alternate "LCD_SEG29" passive line)
					(alternate "LCD_SEG41" passive line)
					(alternate "USART3_RX" passive line)
				)
				(pin bidirectional line
					(at 38.1 -73.66 180)
					(length 2.54)
					(name "PC12")
					(number "53")
					(alternate "LCD_COM6" passive line)
					(alternate "LCD_SEG30" passive line)
					(alternate "LCD_SEG42" passive line)
					(alternate "USART3_CK" passive line)
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 2.54)
					(name "PD2")
					(number "54")
					(alternate "LCD_COM7" passive line)
					(alternate "LCD_SEG30" passive line)
					(alternate "LCD_SEG43" passive line)
					(alternate "TIM3_ETR" passive line)
				)
				(pin bidirectional line
					(at 38.1 -7.62 180)
					(length 2.54)
					(name "PB3")
					(number "55")
					(alternate "COMP2_INM" passive line)
					(alternate "JTDO" passive line)
					(alternate "LCD_SEG7" passive line)
					(alternate "PB3" passive line)
					(alternate "SPI1_SCK" passive line)
					(alternate "TIM2_CH2" passive line)
				)
				(pin bidirectional line
					(at 38.1 -10.16 180)
					(length 2.54)
					(name "PB4")
					(number "56")
					(alternate "COMP2_INP" passive line)
					(alternate "LCD_SEG8" passive line)
					(alternate "NJTRST" passive line)
					(alternate "PB4" passive line)
					(alternate "SPI1_MISO" passive line)
					(alternate "TIM3_CH1" passive line)
				)
				(pin bidirectional line
					(at 38.1 -12.7 180)
					(length 2.54)
					(name "PB5")
					(number "57")
					(alternate "COMP2_INP" passive line)
					(alternate "I2C1_SMBA" passive line)
					(alternate "LCD_SEG9" passive line)
					(alternate "SPI1_MOSI" passive line)
					(alternate "TIM3_CH2" passive line)
				)
				(pin bidirectional line
					(at 38.1 -15.24 180)
					(length 2.54)
					(name "PB6")
					(number "58")
					(alternate "I2C1_SCL" passive line)
					(alternate "TIM4_CH1" passive line)
					(alternate "USART1_TX" passive line)
				)
				(pin bidirectional line
					(at 38.1 -17.78 180)
					(length 2.54)
					(name "PB7")
					(number "59")
					(alternate "I2C1_SDA" passive line)
					(alternate "PVD_IN" passive line)
					(alternate "TIM4_CH2" passive line)
					(alternate "USART1_RX" passive line)
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "BOOT0")
					(number "60")
				)
				(pin bidirectional line
					(at 38.1 -20.32 180)
					(length 2.54)
					(name "PB8")
					(number "61")
					(alternate "I2C1_SCL" passive line)
					(alternate "LCD_SEG16" passive line)
					(alternate "TIM10_CH1" passive line)
					(alternate "TIM4_CH3" passive line)
				)
				(pin bidirectional line
					(at 38.1 -22.86 180)
					(length 2.54)
					(name "PB9")
					(number "62")
					(alternate "I2C1_SDA" passive line)
					(alternate "LCD_COM3" passive line)
					(alternate "TIM11_CH1" passive line)
					(alternate "TIM4_CH4" passive line)
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "63")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "64")
				)
			)
			(embedded_fonts no)
		)
)
