(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "STM32L552CCT6"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "STM32L552CCT6"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "STM32L552CCT6"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552cc.pdf"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM Microcontrollers - MCU Ultra-low-power FPU Arm Cortex-M33 Trust Zone, MCU 110 MHz 512 kbytes of Flash"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "STM32L552CCT6"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MICROCONTROLLER, IC, ARM, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "STM32L552CCT6_0_1")
			(symbol "STM32L552CCT6_1_1"
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VBAT")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 2.54)
					(name "PC13")
					(number "2")
					(alternate "PWR_WKUP2" bidirectional line)
					(alternate "RTC_OUT1" bidirectional line)
					(alternate "RTC_TS" bidirectional line)
					(alternate "TAMP_IN1" bidirectional line)
					(alternate "TAMP_OUT2" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 2.54)
					(name "PC14")
					(number "3")
					(alternate "RCC_OSC32_IN" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 2.54)
					(name "PC15")
					(number "4")
					(alternate "ADC1_EXTI15" bidirectional line)
					(alternate "ADC2_EXTI15" bidirectional line)
					(alternate "RCC_OSC32_OUT" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 2.54)
					(name "PH0")
					(number "5")
					(alternate "RCC_OSC_IN" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 2.54)
					(name "PH1")
					(number "6")
					(alternate "RCC_OSC_OUT" bidirectional line)
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "NRST")
					(number "7")
				)
				(pin power_in line
					(at 30.48 -74.93 180)
					(length 2.54)
					(name "VSSA")
					(number "8")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDA")
					(number "9")
				)
				(pin bidirectional line
					(at 30.48 0 180)
					(length 2.54)
					(name "PA0")
					(number "10")
					(alternate "ADC1_IN5" bidirectional line)
					(alternate "ADC2_IN5" bidirectional line)
					(alternate "OPAMP1_VINP" bidirectional line)
					(alternate "PWR_WKUP1" bidirectional line)
					(alternate "SAI1_EXTCLK" bidirectional line)
					(alternate "TAMP_IN2" bidirectional line)
					(alternate "TAMP_OUT1" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "TIM5_CH1" bidirectional line)
					(alternate "TIM8_ETR" bidirectional line)
					(alternate "UART4_TX" bidirectional line)
					(alternate "USART2_CTS" bidirectional line)
					(alternate "USART2_NSS" bidirectional line)
				)
				(pin bidirectional line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "PA1")
					(number "11")
					(alternate "ADC1_IN6" bidirectional line)
					(alternate "ADC2_IN6" bidirectional line)
					(alternate "I2C1_SMBA" bidirectional line)
					(alternate "OCTOSPI1_DQS" bidirectional line)
					(alternate "OPAMP1_VINM" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "TAMP_IN5" bidirectional line)
					(alternate "TAMP_OUT4" bidirectional line)
					(alternate "TIM15_CH1N" bidirectional line)
					(alternate "TIM2_CH2" bidirectional line)
					(alternate "TIM5_CH2" bidirectional line)
					(alternate "UART4_RX" bidirectional line)
					(alternate "USART2_DE" bidirectional line)
					(alternate "USART2_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "PA2")
					(number "12")
					(alternate "ADC1_IN7" bidirectional line)
					(alternate "ADC2_IN7" bidirectional line)
					(alternate "COMP1_INP" bidirectional line)
					(alternate "LPUART1_TX" bidirectional line)
					(alternate "OCTOSPI1_NCS" bidirectional line)
					(alternate "PWR_WKUP4" bidirectional line)
					(alternate "RCC_LSCO" bidirectional line)
					(alternate "SAI2_EXTCLK" bidirectional line)
					(alternate "TIM15_CH1" bidirectional line)
					(alternate "TIM2_CH3" bidirectional line)
					(alternate "TIM5_CH3" bidirectional line)
					(alternate "UCPD1_FRSTX1" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "PA3")
					(number "13")
					(alternate "ADC1_IN8" bidirectional line)
					(alternate "ADC2_IN8" bidirectional line)
					(alternate "LPUART1_RX" bidirectional line)
					(alternate "OCTOSPI1_CLK" bidirectional line)
					(alternate "OPAMP1_VOUT" bidirectional line)
					(alternate "SAI1_CK1" bidirectional line)
					(alternate "SAI1_MCLK_A" bidirectional line)
					(alternate "TIM15_CH2" bidirectional line)
					(alternate "TIM2_CH4" bidirectional line)
					(alternate "TIM5_CH4" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 30.48 -10.16 180)
					(length 2.54)
					(name "PA4")
					(number "14")
					(alternate "ADC1_IN9" bidirectional line)
					(alternate "ADC2_IN9" bidirectional line)
					(alternate "DAC1_OUT1" bidirectional line)
					(alternate "LPTIM2_OUT" bidirectional line)
					(alternate "OCTOSPI1_NCS" bidirectional line)
					(alternate "SAI1_FS_B" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "SPI3_NSS" bidirectional line)
					(alternate "USART2_CK" bidirectional line)
				)
				(pin bidirectional line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "PA5")
					(number "15")
					(alternate "ADC1_IN10" bidirectional line)
					(alternate "ADC2_IN10" bidirectional line)
					(alternate "DAC1_OUT2" bidirectional line)
					(alternate "LPTIM2_ETR" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "TIM8_CH1N" bidirectional line)
				)
				(pin bidirectional line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "PA6")
					(number "16")
					(alternate "ADC1_IN11" bidirectional line)
					(alternate "ADC2_IN11" bidirectional line)
					(alternate "LPUART1_CTS" bidirectional line)
					(alternate "OCTOSPI1_IO3" bidirectional line)
					(alternate "OPAMP2_VINP" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "TIM16_CH1" bidirectional line)
					(alternate "TIM1_BKIN" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
					(alternate "TIM8_BKIN" bidirectional line)
					(alternate "USART3_CTS" bidirectional line)
					(alternate "USART3_NSS" bidirectional line)
				)
				(pin bidirectional line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "PA7")
					(number "17")
					(alternate "ADC1_IN12" bidirectional line)
					(alternate "ADC2_IN12" bidirectional line)
					(alternate "I2C3_SCL" bidirectional line)
					(alternate "OCTOSPI1_IO2" bidirectional line)
					(alternate "OPAMP2_VINM" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "TIM17_CH1" bidirectional line)
					(alternate "TIM1_CH1N" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "TIM8_CH1N" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 2.54)
					(name "PB0")
					(number "18")
					(alternate "ADC1_IN15" bidirectional line)
					(alternate "ADC2_IN15" bidirectional line)
					(alternate "COMP1_OUT" bidirectional line)
					(alternate "OCTOSPI1_IO1" bidirectional line)
					(alternate "OPAMP2_VOUT" bidirectional line)
					(alternate "SAI1_EXTCLK" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
					(alternate "TIM8_CH2N" bidirectional line)
					(alternate "USART3_CK" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 2.54)
					(name "PB1")
					(number "19")
					(alternate "ADC1_IN16" bidirectional line)
					(alternate "ADC2_IN16" bidirectional line)
					(alternate "COMP1_INM" bidirectional line)
					(alternate "DFSDM1_DATIN0" bidirectional line)
					(alternate "LPTIM2_IN1" bidirectional line)
					(alternate "LPUART1_DE" bidirectional line)
					(alternate "LPUART1_RTS" bidirectional line)
					(alternate "OCTOSPI1_IO0" bidirectional line)
					(alternate "TIM1_CH3N" bidirectional line)
					(alternate "TIM3_CH4" bidirectional line)
					(alternate "TIM8_CH3N" bidirectional line)
					(alternate "USART3_DE" bidirectional line)
					(alternate "USART3_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 2.54)
					(name "PB2")
					(number "20")
					(alternate "COMP1_INP" bidirectional line)
					(alternate "DFSDM1_CKIN0" bidirectional line)
					(alternate "I2C3_SMBA" bidirectional line)
					(alternate "LPTIM1_OUT" bidirectional line)
					(alternate "OCTOSPI1_DQS" bidirectional line)
					(alternate "RTC_OUT2" bidirectional line)
					(alternate "UCPD1_FRSTX1" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 2.54)
					(name "PB10")
					(number "21")
					(alternate "COMP1_OUT" bidirectional line)
					(alternate "I2C2_SCL" bidirectional line)
					(alternate "I2C4_SCL" bidirectional line)
					(alternate "LPTIM3_OUT" bidirectional line)
					(alternate "LPUART1_RX" bidirectional line)
					(alternate "OCTOSPI1_CLK" bidirectional line)
					(alternate "SAI1_SCK_A" bidirectional line)
					(alternate "SPI2_SCK" bidirectional line)
					(alternate "TIM2_CH3" bidirectional line)
					(alternate "TSC_SYNC" bidirectional line)
					(alternate "USART3_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 2.54)
					(name "PB11")
					(number "22")
					(alternate "ADC1_EXTI11" bidirectional line)
					(alternate "ADC2_EXTI11" bidirectional line)
					(alternate "COMP2_OUT" bidirectional line)
					(alternate "I2C2_SDA" bidirectional line)
					(alternate "I2C4_SDA" bidirectional line)
					(alternate "LPUART1_TX" bidirectional line)
					(alternate "OCTOSPI1_NCS" bidirectional line)
					(alternate "TIM2_CH4" bidirectional line)
					(alternate "USART3_RX" bidirectional line)
				)
				(pin power_in line
					(at 30.48 -77.47 180)
					(length 2.54)
					(name "VSS")
					(number "23")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDD")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 2.54)
					(name "PB12")
					(number "25")
					(alternate "DFSDM1_DATIN1" bidirectional line)
					(alternate "I2C2_SMBA" bidirectional line)
					(alternate "LPUART1_DE" bidirectional line)
					(alternate "LPUART1_RTS" bidirectional line)
					(alternate "OCTOSPI1_NCLK" bidirectional line)
					(alternate "SAI2_FS_A" bidirectional line)
					(alternate "SPI2_NSS" bidirectional line)
					(alternate "TIM15_BKIN" bidirectional line)
					(alternate "TIM1_BKIN" bidirectional line)
					(alternate "TSC_G1_IO1" bidirectional line)
					(alternate "USART3_CK" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 2.54)
					(name "PB13")
					(number "26")
					(alternate "DFSDM1_CKIN1" bidirectional line)
					(alternate "I2C2_SCL" bidirectional line)
					(alternate "LPTIM3_IN1" bidirectional line)
					(alternate "LPUART1_CTS" bidirectional line)
					(alternate "SAI2_SCK_A" bidirectional line)
					(alternate "SPI2_SCK" bidirectional line)
					(alternate "TIM15_CH1N" bidirectional line)
					(alternate "TIM1_CH1N" bidirectional line)
					(alternate "TSC_G1_IO2" bidirectional line)
					(alternate "UCPD1_FRSTX2" bidirectional line)
					(alternate "USART3_CTS" bidirectional line)
					(alternate "USART3_NSS" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 2.54)
					(name "PB14")
					(number "27")
					(alternate "DFSDM1_DATIN2" bidirectional line)
					(alternate "I2C2_SDA" bidirectional line)
					(alternate "LPTIM3_ETR" bidirectional line)
					(alternate "SAI2_MCLK_A" bidirectional line)
					(alternate "SPI2_MISO" bidirectional line)
					(alternate "TIM15_CH1" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "TIM8_CH2N" bidirectional line)
					(alternate "TSC_G1_IO3" bidirectional line)
					(alternate "UCPD1_DBCC2" bidirectional line)
					(alternate "USART3_DE" bidirectional line)
					(alternate "USART3_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 2.54)
					(name "PB15")
					(number "28")
					(alternate "ADC1_EXTI15" bidirectional line)
					(alternate "ADC2_EXTI15" bidirectional line)
					(alternate "DFSDM1_CKIN2" bidirectional line)
					(alternate "RTC_REFIN" bidirectional line)
					(alternate "SAI2_SD_A" bidirectional line)
					(alternate "SPI2_MOSI" bidirectional line)
					(alternate "TIM15_CH2" bidirectional line)
					(alternate "TIM1_CH3N" bidirectional line)
					(alternate "TIM8_CH3N" bidirectional line)
					(alternate "UCPD1_CC2" bidirectional line)
				)
				(pin bidirectional line
					(at 30.48 -20.32 180)
					(length 2.54)
					(name "PA8")
					(number "29")
					(alternate "LPTIM2_OUT" bidirectional line)
					(alternate "RCC_MCO" bidirectional line)
					(alternate "SAI1_CK2" bidirectional line)
					(alternate "SAI1_SCK_A" bidirectional line)
					(alternate "TIM1_CH1" bidirectional line)
					(alternate "USART1_CK" bidirectional line)
				)
				(pin bidirectional line
					(at 30.48 -22.86 180)
					(length 2.54)
					(name "PA9")
					(number "30")
					(alternate "DAC1_EXTI9" bidirectional line)
					(alternate "SAI1_FS_A" bidirectional line)
					(alternate "SPI2_SCK" bidirectional line)
					(alternate "TIM15_BKIN" bidirectional line)
					(alternate "TIM1_CH2" bidirectional line)
					(alternate "USART1_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 30.48 -25.4 180)
					(length 2.54)
					(name "PA10")
					(number "31")
					(alternate "CRS_SYNC" bidirectional line)
					(alternate "SAI1_D1" bidirectional line)
					(alternate "SAI1_SD_A" bidirectional line)
					(alternate "TIM17_BKIN" bidirectional line)
					(alternate "TIM1_CH3" bidirectional line)
					(alternate "USART1_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 30.48 -27.94 180)
					(length 2.54)
					(name "PA11")
					(number "32")
					(alternate "ADC1_EXTI11" bidirectional line)
					(alternate "ADC2_EXTI11" bidirectional line)
					(alternate "FDCAN1_RX" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "TIM1_BKIN2" bidirectional line)
					(alternate "TIM1_CH4" bidirectional line)
					(alternate "USART1_CTS" bidirectional line)
					(alternate "USART1_NSS" bidirectional line)
					(alternate "USB_DM" bidirectional line)
				)
				(pin bidirectional line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "PA12")
					(number "33")
					(alternate "FDCAN1_TX" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "TIM1_ETR" bidirectional line)
					(alternate "USART1_DE" bidirectional line)
					(alternate "USART1_RTS" bidirectional line)
					(alternate "USB_DP" bidirectional line)
				)
				(pin bidirectional line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "PA13")
					(number "34")
					(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
					(alternate "IR_OUT" bidirectional line)
					(alternate "SAI1_SD_B" bidirectional line)
					(alternate "USB_NOE" bidirectional line)
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "35")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDD")
					(number "36")
				)
				(pin bidirectional line
					(at 30.48 -35.56 180)
					(length 2.54)
					(name "PA14")
					(number "37")
					(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
					(alternate "I2C1_SMBA" bidirectional line)
					(alternate "I2C4_SMBA" bidirectional line)
					(alternate "LPTIM1_OUT" bidirectional line)
					(alternate "SAI1_FS_B" bidirectional line)
				)
				(pin bidirectional line
					(at 30.48 -38.1 180)
					(length 2.54)
					(name "PA15")
					(number "38")
					(alternate "ADC1_EXTI15" bidirectional line)
					(alternate "ADC2_EXTI15" bidirectional line)
					(alternate "DEBUG_JTDI" bidirectional line)
					(alternate "SAI2_FS_B" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "SPI3_NSS" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "UART4_DE" bidirectional line)
					(alternate "UART4_RTS" bidirectional line)
					(alternate "UCPD1_CC1" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
					(alternate "USART3_DE" bidirectional line)
					(alternate "USART3_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 2.54)
					(name "PB3")
					(number "39")
					(alternate "COMP2_INM" bidirectional line)
					(alternate "CRS_SYNC" bidirectional line)
					(alternate "DEBUG_JTDO-SWO" bidirectional line)
					(alternate "SAI1_SCK_B" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "SPI3_SCK" bidirectional line)
					(alternate "TIM2_CH2" bidirectional line)
					(alternate "USART1_DE" bidirectional line)
					(alternate "USART1_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 2.54)
					(name "PB4")
					(number "40")
					(alternate "COMP2_INP" bidirectional line)
					(alternate "DEBUG_JTRST" bidirectional line)
					(alternate "I2C3_SDA" bidirectional line)
					(alternate "SAI1_MCLK_B" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "SPI3_MISO" bidirectional line)
					(alternate "TIM17_BKIN" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
					(alternate "TSC_G2_IO1" bidirectional line)
					(alternate "USART1_CTS" bidirectional line)
					(alternate "USART1_NSS" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 2.54)
					(name "PB5")
					(number "41")
					(alternate "COMP2_OUT" bidirectional line)
					(alternate "I2C1_SMBA" bidirectional line)
					(alternate "LPTIM1_IN1" bidirectional line)
					(alternate "OCTOSPI1_NCLK" bidirectional line)
					(alternate "SAI1_SD_B" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "SPI3_MOSI" bidirectional line)
					(alternate "TIM16_BKIN" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "TSC_G2_IO2" bidirectional line)
					(alternate "UCPD1_DBCC1" bidirectional line)
					(alternate "USART1_CK" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 2.54)
					(name "PB6")
					(number "42")
					(alternate "COMP2_INP" bidirectional line)
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "I2C4_SCL" bidirectional line)
					(alternate "LPTIM1_ETR" bidirectional line)
					(alternate "SAI1_FS_B" bidirectional line)
					(alternate "TIM16_CH1N" bidirectional line)
					(alternate "TIM4_CH1" bidirectional line)
					(alternate "TIM8_BKIN2" bidirectional line)
					(alternate "TSC_G2_IO3" bidirectional line)
					(alternate "USART1_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 2.54)
					(name "PB7")
					(number "43")
					(alternate "COMP2_INM" bidirectional line)
					(alternate "I2C1_SDA" bidirectional line)
					(alternate "I2C4_SDA" bidirectional line)
					(alternate "LPTIM1_IN2" bidirectional line)
					(alternate "PWR_PVD_IN" bidirectional line)
					(alternate "TIM17_CH1N" bidirectional line)
					(alternate "TIM4_CH2" bidirectional line)
					(alternate "TIM8_BKIN" bidirectional line)
					(alternate "TSC_G2_IO4" bidirectional line)
					(alternate "UART4_CTS" bidirectional line)
					(alternate "USART1_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 2.54)
					(name "PH3")
					(number "44")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 2.54)
					(name "PB8")
					(number "45")
					(alternate "DFSDM1_CKOUT" bidirectional line)
					(alternate "FDCAN1_RX" bidirectional line)
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "SAI1_CK1" bidirectional line)
					(alternate "SAI1_MCLK_A" bidirectional line)
					(alternate "TIM16_CH1" bidirectional line)
					(alternate "TIM4_CH3" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 2.54)
					(name "PB9")
					(number "46")
					(alternate "DAC1_EXTI9" bidirectional line)
					(alternate "FDCAN1_TX" bidirectional line)
					(alternate "I2C1_SDA" bidirectional line)
					(alternate "IR_OUT" bidirectional line)
					(alternate "SAI1_D2" bidirectional line)
					(alternate "SAI1_FS_A" bidirectional line)
					(alternate "SPI2_NSS" bidirectional line)
					(alternate "TIM17_CH1" bidirectional line)
					(alternate "TIM4_CH4" bidirectional line)
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "47")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "48")
				)
			)
			(embedded_fonts no)
		)
)
