(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "STM32MP157C"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.8 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "STM32MP157C"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "STM32MP157C"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32mp157c.pdf"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM Cortex-A7 processor, 2x209MHz, 1.71-3.6V, 176 GPIO, TFBGA-361"
				(at 50.8 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "STM32MP157CAC3"
				(at 50.8 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 50.8 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "BGA, IC, ARM, MICROPROCESSOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "STM32MP157C_1_1"
				(pin power_in line
					(at 0 -25.4 0)
					(length 5.08)
					(name "VDD_CORE")
					(number "1A2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1A4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1A6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VDDQ_DDR")
					(number "1A8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1B1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1B3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1B5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_DDR")
					(number "1B7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_DDR")
					(number "1B9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1C2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1C4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1C6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_DDR")
					(number "1C8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1D1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1D3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1D5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1D7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_DDR")
					(number "1D9")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1E2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1E4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1E6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_DDR")
					(number "1E8")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "VBAT")
					(number "1F1")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 5.08)
					(name "VDD")
					(number "1F3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1F5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1F7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_DDR")
					(number "1F9")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VDD_ANA")
					(number "1G2")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "1G4")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1G6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_DDR")
					(number "1G8")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 5.08)
					(name "VDDA")
					(number "1H1")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "1H3")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "1H5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CORE")
					(number "1H7")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_DDR")
					(number "1H9")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "1J2")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "1J4")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "1J6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_DDR")
					(number "1J8")
				)
				(pin power_in line
					(at 0 -45.72 0)
					(length 5.08)
					(name "VSS")
					(number "A1")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A23")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA5")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA8")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA12")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 5.08)
					(name "VDD3V3_USBHS")
					(number "AA15")
				)
				(pin power_in line
					(at 0 -50.8 0)
					(length 5.08)
					(name "VSS_USBHS")
					(number "AA16")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 5.08)
					(name "VDD3V3_USBFS")
					(number "AA17")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA21")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 5.08)
					(name "VDDA1V8_REG")
					(number "AB14")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 5.08)
					(name "VDDA1V1_REG")
					(number "AB15")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC1")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC23")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C7")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C12")
				)
				(pin power_in line
					(at 0 -53.34 0)
					(length 5.08)
					(name "VSS_DSI")
					(number "C16")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C21")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D4")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F21")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H3")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K21")
				)
				(pin bidirectional line
					(at 35.56 -11.43 180)
					(length 5.08)
					(name "BOOT2")
					(number "M2")
				)
				(pin bidirectional line
					(at 35.56 -29.21 180)
					(length 5.08)
					(name "NRST")
					(number "M3")
				)
				(pin input line
					(at 35.56 -31.75 180)
					(length 5.08)
					(name "NRST_CORE")
					(number "M4")
				)
				(pin bidirectional line
					(at 35.56 -6.35 180)
					(length 5.08)
					(name "BOOT0")
					(number "N1")
				)
				(pin output line
					(at 35.56 -19.05 180)
					(length 5.08)
					(name "PWR_LP")
					(number "N3")
				)
				(pin bidirectional line
					(at 35.56 -8.89 180)
					(length 5.08)
					(name "BOOT1")
					(number "N4")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P3")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P21")
				)
				(pin output line
					(at 35.56 -16.51 180)
					(length 5.08)
					(name "PWR_ON")
					(number "R2")
				)
				(pin input line
					(at 35.56 -21.59 180)
					(length 5.08)
					(name "PDR_ON")
					(number "R3")
				)
				(pin bidirectional line
					(at 35.56 0 180)
					(length 5.08)
					(name "VREF+")
					(number "R4")
				)
				(pin input line
					(at 35.56 -24.13 180)
					(length 5.08)
					(name "PDR_ON_CORE")
					(number "T3")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V21")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W3")
				)
			)
			(symbol "STM32MP157C_2_1"
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "PC14-OSC32_IN")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "PC15-OSC32_OUT")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PA9")
					(number "A8")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PB3")
					(number "A11")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PA8")
					(number "A13")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PA1")
					(number "AA4")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "PC1")
					(number "AA6")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PB1")
					(number "AA7")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PB13")
					(number "AA10")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PA11")
					(number "AA18")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PB11")
					(number "AB1")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "PA0")
					(number "AB3")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "PC0")
					(number "AB5")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PB0")
					(number "AB6")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "PC5")
					(number "AB7")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PA7")
					(number "AB8")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PB8")
					(number "AB10")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PA12")
					(number "AB19")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PA2")
					(number "AC3")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "PB12")
					(number "AC5")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "PC4")
					(number "AC7")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PA6")
					(number "AC8")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "PB9")
					(number "B10")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "PC7")
					(number "B11")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "PB15")
					(number "B12")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PB4")
					(number "B13")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "PC6")
					(number "B14")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PB14")
					(number "C13")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PA15")
					(number "C19")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PB7")
					(number "D11")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "PC12")
					(number "D13")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "PC10")
					(number "D15")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "PC11")
					(number "D16")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "PC9")
					(number "D17")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "PC8")
					(number "D18")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "PC13")
					(number "K2")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PA13")
					(number "N2")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PA14")
					(number "T2")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PA3")
					(number "U2")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "PA5")
					(number "V3")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PA4")
					(number "V4")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "PC3")
					(number "W2")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "PC2")
					(number "Y2")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PB10")
					(number "Y3")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PB5")
					(number "Y8")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PB6")
					(number "Y14")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PB2")
					(number "Y16")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PA10")
					(number "Y17")
				)
			)
			(symbol "STM32MP157C_3_1"
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PE13")
					(number "A3")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PE11")
					(number "A4")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "PF1")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "PD5")
					(number "A7")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "PF2")
					(number "A14")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "PE9")
					(number "AA9")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PE7")
					(number "AA11")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "PF6")
					(number "AA13")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "PF9")
					(number "AA14")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PD13")
					(number "AA19")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "PF7")
					(number "AB12")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "PF14")
					(number "AC4")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PD11")
					(number "AC10")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "PF8")
					(number "AC11")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PE8")
					(number "AC13")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "PE12")
					(number "B4")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PD10")
					(number "B5")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PD4")
					(number "B6")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "PD0")
					(number "B8")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PD1")
					(number "B9")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PE14")
					(number "C6")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PE1")
					(number "C8")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PE3")
					(number "C9")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PE6")
					(number "C10")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PE5")
					(number "C11")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PD6")
					(number "D2")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "PE15")
					(number "D3")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PE0")
					(number "D6")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "PF5")
					(number "D7")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "PF0")
					(number "D8")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "PF4")
					(number "D9")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PD7")
					(number "D10")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PD2")
					(number "D12")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PD3")
					(number "D14")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PE4")
					(number "D19")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PD15")
					(number "J2")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PD9")
					(number "K1")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PD8")
					(number "K3")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PD14")
					(number "L3")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "PF3")
					(number "U1")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PE2")
					(number "Y1")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "PF15")
					(number "Y4")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "PF13")
					(number "Y5")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "PF12")
					(number "Y9")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "PF11")
					(number "Y10")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "PF10")
					(number "Y12")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PE10")
					(number "Y15")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PD12")
					(number "Y18")
				)
			)
			(symbol "STM32MP157C_4_1"
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PH5")
					(number "A2")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PG6")
					(number "A10")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PG14")
					(number "AA1")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PG13")
					(number "AA2")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PH3")
					(number "AA3")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PG4")
					(number "AB2")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PH2")
					(number "AB4")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PG8")
					(number "AB9")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PG10")
					(number "AB11")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "PG0")
					(number "AC2")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PG7")
					(number "AC14")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "PH15")
					(number "B1")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "PH12")
					(number "B2")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PH4")
					(number "B3")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PG15")
					(number "B7")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "PI0")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PH10")
					(number "C2")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PH14")
					(number "C3")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PH11")
					(number "C4")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "PH9")
					(number "C5")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PH13")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PH8")
					(number "D5")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "PI3")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "PI2")
					(number "E2")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "PI1")
					(number "E3")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "PI4")
					(number "E4")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "PI7")
					(number "F2")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "PI5")
					(number "F3")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "PI6")
					(number "F4")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "PZ1")
					(number "G1")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "PZ4")
					(number "G2")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "PZ0")
					(number "G3")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "PZ3")
					(number "G4")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "PZ6")
					(number "H1")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "PI12")
					(number "H2")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "PZ5")
					(number "H2")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "PI9")
					(number "H4")
				)
				(pin bidirectional line
					(at 0 -139.7 0)
					(length 5.08)
					(name "PZ7")
					(number "J3")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "PZ2")
					(number "J4")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PG12")
					(number "K4")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "PI8")
					(number "L4")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PH0-OSC_IN")
					(number "P1")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PH1-OSC_OUT")
					(number "P2")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "PI11")
					(number "P4")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "PI10")
					(number "T1")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PG3")
					(number "T4")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PG2")
					(number "V2")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PG1")
					(number "W1")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PH7")
					(number "W4")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "PG5")
					(number "Y6")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PG11")
					(number "Y7")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PH6")
					(number "Y11")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PG9")
					(number "Y13")
				)
			)
			(symbol "STM32MP157C_5_1"
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "DSI_CKN")
					(number "A16")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "DSI_D1N")
					(number "A17")
				)
				(pin output line
					(at 0 -45.72 0)
					(length 5.08)
					(name "JTDO-TRACESWO")
					(number "A19")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "JTDI")
					(number "A20")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "BYPASS_REG1V8")
					(number "AB13")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "USB_DM2")
					(number "AB16")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "USB_DM1")
					(number "AB17")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "USB_RREF")
					(number "AB18")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "USB_DP2")
					(number "AC16")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "USB_DP1")
					(number "AC17")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "OTG_VBUS")
					(number "AC19")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "DSI_D0N")
					(number "B15")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "DSI_CKP")
					(number "B16")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "DSI_D1P")
					(number "B17")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 5.08)
					(name "NJTRST")
					(number "B19")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 5.08)
					(name "JTCK-SWCLK")
					(number "B20")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "DSI_D0P")
					(number "C15")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "JTMS-SWDIO")
					(number "C20")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "ANA0")
					(number "U3")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "ANA1")
					(number "U4")
				)
			)
			(symbol "STM32MP157C_6_1"
				(pin output line
					(at 0 -58.42 0)
					(length 5.08)
					(name "DDR_BA0")
					(number "11")
				)
				(pin bidirectional line
					(at 35.56 -71.12 180)
					(length 5.08)
					(name "DDR_DQ20")
					(number "A21")
				)
				(pin bidirectional line
					(at 35.56 -78.74 180)
					(length 5.08)
					(name "DDR_DQ23")
					(number "A22")
				)
				(pin output line
					(at 35.56 -119.38 180)
					(length 5.08)
					(name "DDR_DQM3")
					(number "AA20")
				)
				(pin bidirectional line
					(at 35.56 -106.68 180)
					(length 5.08)
					(name "DDR_DQ31")
					(number "AA22")
				)
				(pin bidirectional line
					(at 35.56 -104.14 180)
					(length 5.08)
					(name "DDR_DQ30")
					(number "AA23")
				)
				(pin bidirectional line
					(at 35.56 -91.44 180)
					(length 5.08)
					(name "DDR_DQ27")
					(number "AB20")
				)
				(pin bidirectional line
					(at 35.56 -88.9 180)
					(length 5.08)
					(name "DDR_DQ26")
					(number "AB21")
				)
				(pin bidirectional line
					(at 35.56 -93.98 180)
					(length 5.08)
					(name "DDR_DQS3P")
					(number "AB22")
				)
				(pin bidirectional line
					(at 35.56 -96.52 180)
					(length 5.08)
					(name "DDR_DQS3N")
					(number "AB23")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "DDR_VREF")
					(number "AC20")
				)
				(pin bidirectional line
					(at 35.56 -101.6 180)
					(length 5.08)
					(name "DDR_DQ29")
					(number "AC21")
				)
				(pin bidirectional line
					(at 35.56 -99.06 180)
					(length 5.08)
					(name "DDR_DQ28")
					(number "AC22")
				)
				(pin bidirectional line
					(at 35.56 -63.5 180)
					(length 5.08)
					(name "DDR_DQ19")
					(number "B21")
				)
				(pin bidirectional line
					(at 35.56 -55.88 180)
					(length 5.08)
					(name "DDR_DQ16")
					(number "B22")
				)
				(pin bidirectional line
					(at 35.56 -68.58 180)
					(length 5.08)
					(name "DDR_DQS2N")
					(number "B23")
				)
				(pin bidirectional line
					(at 35.56 -66.04 180)
					(length 5.08)
					(name "DDR_DQS2P")
					(number "C22")
				)
				(pin output line
					(at 35.56 -116.84 180)
					(length 5.08)
					(name "DDR_DQM2")
					(number "C23")
				)
				(pin output line
					(at 0 -68.58 0)
					(length 5.08)
					(name "DDR_RESETN")
					(number "D20")
				)
				(pin bidirectional line
					(at 35.56 -76.2 180)
					(length 5.08)
					(name "DDR_DQ22")
					(number "D21")
				)
				(pin bidirectional line
					(at 35.56 -58.42 180)
					(length 5.08)
					(name "DDR_DQ17")
					(number "D22")
				)
				(pin bidirectional line
					(at 35.56 -60.96 180)
					(length 5.08)
					(name "DDR_DQ18")
					(number "D23")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 5.08)
					(name "DDR_A7")
					(number "E20")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "DDR_DQ3")
					(number "E21")
				)
				(pin bidirectional line
					(at 35.56 0 180)
					(length 5.08)
					(name "DDR_DQ0")
					(number "E22")
				)
				(pin bidirectional line
					(at 35.56 -73.66 180)
					(length 5.08)
					(name "DDR_DQ21")
					(number "E23")
				)
				(pin output line
					(at 0 -48.26 0)
					(length 5.08)
					(name "DDR_A13")
					(number "F20")
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "DDR_DQ1")
					(number "F22")
				)
				(pin output line
					(at 0 -38.1 0)
					(length 5.08)
					(name "DDR_A9")
					(number "G20")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "DDR_DQ7")
					(number "G21")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "DDR_DQS0P")
					(number "G22")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "DDR_DQS0N")
					(number "G23")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 5.08)
					(name "DDR_A5")
					(number "H20")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "DDR_DQ2")
					(number "H21")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "DDR_DQ6")
					(number "H22")
				)
				(pin output line
					(at 35.56 -111.76 180)
					(length 5.08)
					(name "DDR_DQM0")
					(number "H23")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 5.08)
					(name "DDR_A2")
					(number "J20")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "DDR_DQ4")
					(number "J21")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "DDR_DQ5")
					(number "J22")
				)
				(pin output line
					(at 0 -78.74 0)
					(length 5.08)
					(name "DDR_DTO0")
					(number "K20")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 5.08)
					(name "DDR_A3")
					(number "K22")
				)
				(pin bidirectional line
					(at 35.56 -124.46 180)
					(length 5.08)
					(name "DDR_ZQ")
					(number "K23")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 5.08)
					(name "DDR_A0")
					(number "L20")
				)
				(pin output line
					(at 0 -81.28 0)
					(length 5.08)
					(name "DDR_DTO1")
					(number "L21")
				)
				(pin output line
					(at 0 -71.12 0)
					(length 5.08)
					(name "DDR_ODT")
					(number "L22")
				)
				(pin output line
					(at 0 -91.44 0)
					(length 5.08)
					(name "DDR_WEN")
					(number "M20")
				)
				(pin output line
					(at 0 -63.5 0)
					(length 5.08)
					(name "DDR_BA2")
					(number "M21")
				)
				(pin output line
					(at 0 -88.9 0)
					(length 5.08)
					(name "DDR_CSN")
					(number "M22")
				)
				(pin output line
					(at 0 -73.66 0)
					(length 5.08)
					(name "DDR_RASN")
					(number "N20")
				)
				(pin output line
					(at 0 -76.2 0)
					(length 5.08)
					(name "DDR_CASN")
					(number "N20")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 5.08)
					(name "DDR_CLKP")
					(number "N22")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 5.08)
					(name "DDR_CLKN")
					(number "N23")
				)
				(pin output line
					(at 0 -53.34 0)
					(length 5.08)
					(name "DDR_A15")
					(number "P20")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 5.08)
					(name "DDR_A1")
					(number "P22")
				)
				(pin output line
					(at 0 -45.72 0)
					(length 5.08)
					(name "DDR_A12")
					(number "P23")
				)
				(pin output line
					(at 0 -43.18 0)
					(length 5.08)
					(name "DDR_A11")
					(number "R20")
				)
				(pin output line
					(at 0 -50.8 0)
					(length 5.08)
					(name "DDR_A14")
					(number "R21")
				)
				(pin output line
					(at 0 -40.64 0)
					(length 5.08)
					(name "DDR_A10")
					(number "R22")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 5.08)
					(name "DDR_CKE")
					(number "T20")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "DDR_DQ8")
					(number "T21")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "DDR_DQ10")
					(number "T22")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 5.08)
					(name "DDR_DQ13")
					(number "T23")
				)
				(pin output line
					(at 0 -60.96 0)
					(length 5.08)
					(name "DDR_BA1")
					(number "U20")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "DDR_DQ9")
					(number "U21")
				)
				(pin passive line
					(at 35.56 -63.5 180)
					(length 5.08)
					(hide yes)
					(name "DDR_DQ19")
					(number "U21")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "DDR_DQS1P")
					(number "U22")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 5.08)
					(name "DDR_DQS1N")
					(number "U23")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 5.08)
					(name "DDR_A4")
					(number "V20")
				)
				(pin output line
					(at 35.56 -114.3 180)
					(length 5.08)
					(name "DDR_DQM1")
					(number "V22")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 5.08)
					(name "DDR_A6")
					(number "W20")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "DDR_DQ11")
					(number "W21")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 5.08)
					(name "DDR_DQ14")
					(number "W22")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 5.08)
					(name "DDR_DQ12")
					(number "W23")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "DDR_ATO")
					(number "Y19")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 5.08)
					(name "DDR_A8")
					(number "Y20")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 5.08)
					(name "DDR_DQ15")
					(number "Y21")
				)
				(pin bidirectional line
					(at 35.56 -86.36 180)
					(length 5.08)
					(name "DDR_DQ25")
					(number "Y22")
				)
				(pin bidirectional line
					(at 35.56 -83.82 180)
					(length 5.08)
					(name "DDR_DQ24")
					(number "Y23")
				)
			)
			(embedded_fonts no)
		)
)
