(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "STP08CP05_HTSSOP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "STP08CP05_HTSSOP"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "STP08CP05_HTSSOP"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/stp08cp05.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Low voltage, low current power 8-bit shift register"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "STP08CP05XTTR"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, INTERFACE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "STP08CP05_HTSSOP_1_1"
				(pin power_in line
					(at 21.59 -24.13 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SDI")
					(number "2")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "CLK")
					(number "3")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "LE")
					(number "4")
				)
				(pin output line
					(at 21.59 0 180)
					(length 2.54)
					(name "OUT_0")
					(number "5")
				)
				(pin output line
					(at 21.59 -2.54 180)
					(length 2.54)
					(name "OUT_1")
					(number "6")
				)
				(pin output line
					(at 21.59 -5.08 180)
					(length 2.54)
					(name "OUT_2")
					(number "7")
				)
				(pin output line
					(at 21.59 -7.62 180)
					(length 2.54)
					(name "OUT_3")
					(number "8")
				)
				(pin output line
					(at 21.59 -10.16 180)
					(length 2.54)
					(name "OUT_4")
					(number "9")
				)
				(pin output line
					(at 21.59 -12.7 180)
					(length 2.54)
					(name "OUT_5")
					(number "10")
				)
				(pin output line
					(at 21.59 -15.24 180)
					(length 2.54)
					(name "OUT_6")
					(number "11")
				)
				(pin output line
					(at 21.59 -17.78 180)
					(length 2.54)
					(name "OUT_7")
					(number "12")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "~{OE}")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "SDO")
					(number "14")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "R-EXT")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "16")
				)
				(pin passive line
					(at 21.59 -21.59 180)
					(length 2.54)
					(name "EP")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
)
