(footprint "QFN-28_6x6mm_P0.65mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "QFN, 28 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf (Page 289)), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
	(tags "QFN DFN_QFN")
	(property "Reference" "REF**"
		(at 0 -4.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-28_6x6mm_P0.65mm"
		(at 0 4.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.95 6.3 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at 0.05 5.5 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at 0.05 6.7 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -1.42 -1.42)
		(size 1.14 1.14)
		(layers "F.Paste")
		(roundrect_rratio 0.219298)
	)
	(pad "" smd roundrect
		(at -1.42 0)
		(size 1.14 1.14)
		(layers "F.Paste")
		(roundrect_rratio 0.219298)
	)
	(pad "" smd roundrect
		(at -1.42 1.42)
		(size 1.14 1.14)
		(layers "F.Paste")
		(roundrect_rratio 0.219298)
	)
	(pad "" smd roundrect
		(at 0 -1.42)
		(size 1.14 1.14)
		(layers "F.Paste")
		(roundrect_rratio 0.219298)
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 1.14 1.14)
		(layers "F.Paste")
		(roundrect_rratio 0.219298)
	)
	(pad "" smd roundrect
		(at 0 1.42)
		(size 1.14 1.14)
		(layers "F.Paste")
		(roundrect_rratio 0.219298)
	)
	(pad "" smd roundrect
		(at 1.42 -1.42)
		(size 1.14 1.14)
		(layers "F.Paste")
		(roundrect_rratio 0.219298)
	)
	(pad "" smd roundrect
		(at 1.42 0)
		(size 1.14 1.14)
		(layers "F.Paste")
		(roundrect_rratio 0.219298)
	)
	(pad "" smd roundrect
		(at 1.42 1.42)
		(size 1.14 1.14)
		(layers "F.Paste")
		(roundrect_rratio 0.219298)
	)
	(pad "1" smd roundrect
		(at -2.84 -1.95)
		(size 1.025 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.84 -1.3)
		(size 1.025 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.84 -0.65)
		(size 1.025 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.84 0)
		(size 1.025 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.84 0.65)
		(size 1.025 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -2.84 1.3)
		(size 1.025 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -2.84 1.95)
		(size 1.025 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -1.95 2.84)
		(size 0.3 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -1.3 2.84)
		(size 0.3 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -0.65 2.84)
		(size 0.3 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0 2.84)
		(size 0.3 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 0.65 2.84)
		(size 0.3 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1.3 2.84)
		(size 0.3 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.95 2.84)
		(size 0.3 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 2.84 1.95)
		(size 1.025 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 2.84 1.3)
		(size 1.025 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 2.84 0.65)
		(size 1.025 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 2.84 0)
		(size 1.025 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 2.84 -0.65)
		(size 1.025 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 2.84 -1.3)
		(size 1.025 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 2.84 -1.95)
		(size 1.025 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 1.95 -2.84)
		(size 0.3 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 1.3 -2.84)
		(size 0.3 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 0.65 -2.84)
		(size 0.3 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 0 -2.84)
		(size 0.3 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at -0.65 -2.84)
		(size 0.3 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at -1.3 -2.84)
		(size 0.3 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at -1.95 -2.84)
		(size 0.3 1.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 0 0)
		(size 4.25 4.25)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.058824)
	)
	(embedded_fonts no)
	(model "antmicro_sx1272imltrt.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
