(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SX1276IMLTRT"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SX1276IMLTRT"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SX1276IMLTRT"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://semtech.my.salesforce.com/sfc/p/#E0000000JelG/a/2R0000001Rbr/6EfVZUorrpoKFfvaF_Fkpgp5kzjiNyiAbqcpqh9qSjE"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "LoRa 137 MHz to 1020 MHz Low Power Long Range Transceiver"
				(at 50.8 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Semtech"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SX1276IMLTRT"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 50.8 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SX1276IMLTRT_1_1"
				(pin input line
					(at 30.48 -20.32 180)
					(length 2.54)
					(name "RFI_LF")
					(number "1")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VR_ANA")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VBAT_ANA")
					(number "3")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VR_DIG")
					(number "4")
				)
				(pin bidirectional line
					(at 30.48 -35.56 180)
					(length 2.54)
					(name "XTA")
					(number "5")
				)
				(pin bidirectional line
					(at 30.48 -43.18 180)
					(length 2.54)
					(name "XTB")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "NRESET")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "DIO0")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "DIO1/DCLK")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "DIO2/DATA")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "DIO3")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "DIO4")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DIO5")
					(number "13")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VBAT_DIG")
					(number "14")
				)
				(pin power_in line
					(at 30.48 -48.26 180)
					(length 2.54)
					(name "GND")
					(number "15")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "SCK")
					(number "16")
				)
				(pin output line
					(at 0 -43.18 0)
					(length 2.54)
					(name "MISO")
					(number "17")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "MOSI")
					(number "18")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 2.54)
					(name "NSS")
					(number "19")
				)
				(pin output line
					(at 30.48 -25.4 180)
					(length 2.54)
					(name "RXTX/RF_MOD")
					(number "20")
				)
				(pin input line
					(at 30.48 0 180)
					(length 2.54)
					(name "RFI_HF(GND)")
					(number "21")
				)
				(pin output line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "RFO_HF(GND)")
					(number "22")
				)
				(pin passive line
					(at 30.48 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "23")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VBAT_RF")
					(number "24")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VR_PA")
					(number "25")
				)
				(pin passive line
					(at 30.48 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "26")
				)
				(pin output line
					(at 30.48 -10.16 180)
					(length 2.54)
					(name "PA_BOOST")
					(number "27")
				)
				(pin output line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "RFO_LF")
					(number "28")
				)
				(pin passive line
					(at 30.48 -48.26 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "29")
				)
			)
			(embedded_fonts no)
		)
)
