(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SY75602BTWL-TR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SY75602BTWL-TR"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SY75602BTWL-TR"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/TCG/ProductDocuments/DataSheets/SY75602A-02B-03A-03B-04A-04B-2-4-Outputs-Ultra-Low-Additive-Jitter-PCIe-1-2-3-4-5-6-Clock-Buffer-DS20006508.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "PCIe CLK BUFFER 1:2 250MHZ, small package 8VDFN"
				(at 33.02 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SY75602BTWL-TR"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, CLOCK, SMT, No-RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "VDFN8_NNC_MCH VDFN8_NNC_MCH-M VDFN8_NNC_MCH-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SY75602BTWL-TR_1_1"
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "IN_P")
					(number "1")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "IN_N")
					(number "2")
				)
				(pin output line
					(at 19.05 -1.27 180)
					(length 2.54)
					(name "OUT0_P")
					(number "3")
				)
				(pin output line
					(at 19.05 -3.81 180)
					(length 2.54)
					(name "OUT0_N")
					(number "4")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin output line
					(at 19.05 -8.89 180)
					(length 2.54)
					(name "OUT1_P")
					(number "6")
				)
				(pin output line
					(at 19.05 -11.43 180)
					(length 2.54)
					(name "OUT1_N")
					(number "7")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
