(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SY75604BTWL-TR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SY75604BTWL-TR"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SY75604BTWL-TR"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/TCG/ProductDocuments/DataSheets/SY75602A-02B-03A-03B-04A-04B-2-4-Outputs-Ultra-Low-Additive-Jitter-PCIe-1-2-3-4-5-6-Clock-Buffer-DS20006508.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "PCIe CLK BUFFER 1:4 250MHz, small package VQFN-16"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SY75604BTWL-TR"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, CLOCK, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "VDFN8_NNC_MCH VDFN8_NNC_MCH-M VDFN8_NNC_MCH-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SY75604BTWL-TR_1_1"
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "IN_P")
					(number "1")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "IN_N")
					(number "2")
				)
				(pin input line
					(at 20.32 0 180)
					(length 2.54)
					(name "OE0b")
					(number "3")
				)
				(pin output line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "OUT0_P")
					(number "4")
				)
				(pin output line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "OUT0_N")
					(number "5")
				)
				(pin input line
					(at 20.32 -8.89 180)
					(length 2.54)
					(name "OE1b")
					(number "6")
				)
				(pin output line
					(at 20.32 -11.43 180)
					(length 2.54)
					(name "OUT1_P")
					(number "7")
				)
				(pin output line
					(at 20.32 -13.97 180)
					(length 2.54)
					(name "OUT1_N")
					(number "8")
				)
				(pin power_in line
					(at 0 -31.75 0)
					(length 2.54)
					(name "GND")
					(number "9")
				)
				(pin output line
					(at 20.32 -20.32 180)
					(length 2.54)
					(name "OUT2_P")
					(number "10")
				)
				(pin output line
					(at 20.32 -22.86 180)
					(length 2.54)
					(name "OUT2_N")
					(number "11")
				)
				(pin input line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "OE2b")
					(number "12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "13")
				)
				(pin output line
					(at 20.32 -29.21 180)
					(length 2.54)
					(name "OUT3_P")
					(number "14")
				)
				(pin output line
					(at 20.32 -31.75 180)
					(length 2.54)
					(name "OUT3_N")
					(number "15")
				)
				(pin input line
					(at 20.32 -26.67 180)
					(length 2.54)
					(name "OE3b")
					(number "16")
				)
				(pin power_in line
					(at 0 -29.21 0)
					(length 2.54)
					(name "EP")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
)
