(footprint "QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "QFN, 24 Pin (https://www.ti.com/lit/ds/symlink/tas2505.pdf?ts=1735823429657&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FTAS2505%252Fpart-details%252FTAS2505IRGER)")
	(tags "QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -2.66 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
		(at 0 3.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -0.002 -0.002 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -0.002 -0.002 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -2.81 4.45 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.81 5.65 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.81 6.85 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.655 -0.655)
		(size 1.188 1.188)
		(layers "F.Paste")
		(roundrect_rratio 0.238095)
	)
	(pad "" smd roundrect
		(at -0.655 0.65)
		(size 1.188 1.188)
		(layers "F.Paste")
		(roundrect_rratio 0.238095)
	)
	(pad "" smd roundrect
		(at 0.65 -0.655)
		(size 1.188 1.188)
		(layers "F.Paste")
		(roundrect_rratio 0.238095)
	)
	(pad "" smd roundrect
		(at 0.65 0.65)
		(size 1.188 1.188)
		(layers "F.Paste")
		(roundrect_rratio 0.238095)
	)
	(pad "1" smd roundrect
		(at -1.915 -1.25)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.915 -0.75)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.915 -0.25)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.915 0.25)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.915 0.75)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1.915 1.25)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -1.25 1.91)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -0.75 1.91)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -0.25 1.91)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 0.25 1.91)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0.75 1.91)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 1.25 1.91)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1.91 1.25)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.91 0.75)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 1.91 0.25)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 1.91 -0.25)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 1.91 -0.75)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 1.91 -1.25)
		(size 0.58 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 1.25 -1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 0.75 -1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 0.25 -1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at -0.25 -1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at -0.75 -1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at -1.25 -1.915)
		(size 0.24 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd rect
		(at 0 0)
		(size 2.7 2.7)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "antmicro_tas2505irger.glb"
		(offset
			(xyz -0.002 0.002 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 -90)
		)
	)
)
