(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TAS2505IRGER"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TAS2505IRGER"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TAS2505IRGER"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tas2505.pdf?ts=1735823429657&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FTAS2505%252Fpart-details%252FTAS2505IRGER"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "2.6-W Digital/Analog Input Class-D Speaker Amplifier With Audio Processing, VQFN-24"
				(at 43.18 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TAS2505IRGER"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, POWER, AMP, AUDIO"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TAS2505IRGER_1_0"
				(pin passive line
					(at 27.94 -48.26 180)
					(length 2.54)
					(name "EP")
					(number "25")
				)
			)
			(symbol "TAS2505IRGER_1_1"
				(pin input line
					(at 0 -53.34 0)
					(length 2.54)
					(name "SPI_SEL")
					(number "1")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{RST}")
					(number "2")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "AINL")
					(number "3")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "AINR")
					(number "4")
				)
				(pin output line
					(at 27.94 -35.56 180)
					(length 2.54)
					(name "HPOUT")
					(number "5")
				)
				(pin power_in line
					(at 27.94 -53.34 180)
					(length 2.54)
					(name "AVSS")
					(number "6")
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 2.54)
					(name "AVDD")
					(number "7")
				)
				(pin input line
					(at 27.94 -45.72 180)
					(length 2.54)
					(name "LDO_SEL")
					(number "8")
				)
				(pin output line
					(at 27.94 -25.4 180)
					(length 2.54)
					(name "SPKM")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "SPKVDD")
					(number "10")
				)
				(pin power_in line
					(at 27.94 -50.8 180)
					(length 2.54)
					(name "SPKVSS")
					(number "11")
				)
				(pin output line
					(at 27.94 -22.86 180)
					(length 2.54)
					(name "SPKP")
					(number "12")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "DIN")
					(number "13")
				)
				(pin bidirectional clock
					(at 0 -40.64 0)
					(length 2.54)
					(name "WCLK")
					(number "14")
				)
				(pin bidirectional clock
					(at 0 -45.72 0)
					(length 2.54)
					(name "BCLK")
					(number "15")
				)
				(pin input clock
					(at 0 -35.56 0)
					(length 2.54)
					(name "MCLK")
					(number "16")
				)
				(pin output line
					(at 0 -50.8 0)
					(length 2.54)
					(name "MISO")
					(number "17")
				)
				(pin tri_state line
					(at 0 -30.48 0)
					(length 2.54)
					(name "GPIO")
					(number "18")
					(alternate "DOUT" passive line)
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "SCL")
					(number "19")
					(alternate "SSZ" passive line)
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "SDA")
					(number "20")
					(alternate "MOSI" passive line)
				)
				(pin input clock
					(at 0 -55.88 0)
					(length 2.54)
					(name "SCLK")
					(number "21")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "IOVDD")
					(number "22")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DVDD")
					(number "23")
				)
				(pin power_in line
					(at 27.94 -55.88 180)
					(length 2.54)
					(name "DVSS")
					(number "24")
				)
			)
			(embedded_fonts no)
		)
)
