(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TC358743XBG"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TC358743XBG"
				(at 40.64 7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TC358743XBG"
				(at 40.64 5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://toshiba.semicon-storage.com/info/TC358743XBG_datasheet_en_20171026.pdf?did=35655&prodName=TC358743XBG"
				(at 40.64 2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "HDMI to MIPI CSI-2 bridge. Supports HDMI 1.4. MIPI CSI-2 compliant. 80-Pin VFBGA"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TC358743XBG"
				(at 40.64 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Toshiba"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, CONTROLLER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TC358743XBG_1_1"
				(pin output line
					(at 30.48 -22.86 180)
					(length 2.54)
					(name "CSID3_N")
					(number "A7")
				)
				(pin output line
					(at 30.48 -20.32 180)
					(length 2.54)
					(name "CSID3_P")
					(number "A8")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "IR")
					(number "B4")
				)
				(pin output line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "CSID2_N")
					(number "B7")
				)
				(pin output line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "CSID2_P")
					(number "B8")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "HDMIC_P")
					(number "C1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "HDMIC_N")
					(number "C2")
				)
				(pin output line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "CSIC_N")
					(number "C7")
				)
				(pin output line
					(at 30.48 0 180)
					(length 2.54)
					(name "CSIC_P")
					(number "C8")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "HDMID0_P")
					(number "D1")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "HDMID0_N")
					(number "D2")
				)
				(pin output line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "CSID1_N")
					(number "D7")
				)
				(pin output line
					(at 30.48 -10.16 180)
					(length 2.54)
					(name "CSID1_P")
					(number "D8")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "HDMID1_P")
					(number "E1")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "HDMID1_N")
					(number "E2")
				)
				(pin output line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "CSID0_N")
					(number "E7")
				)
				(pin output line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "CSID0_P")
					(number "E8")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "HDMID2_P")
					(number "F1")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "HDMID2_N")
					(number "F2")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "CEC")
					(number "G1")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "DDC_SDA")
					(number "G3")
				)
				(pin bidirectional line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "I2C_SDA")
					(number "G4")
				)
				(pin bidirectional line
					(at 30.48 -43.18 180)
					(length 2.54)
					(name "EDID_SDA")
					(number "G6")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 2.54)
					(name "HPDO")
					(number "H1")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "HPDI")
					(number "H2")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "DDC_SCL")
					(number "H3")
				)
				(pin bidirectional line
					(at 30.48 -35.56 180)
					(length 2.54)
					(name "I2C_SCL")
					(number "H4")
				)
				(pin bidirectional line
					(at 30.48 -45.72 180)
					(length 2.54)
					(name "EDID_SCL")
					(number "H6")
				)
			)
			(symbol "TC358743XBG_2_1"
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "REXT")
					(number "A1")
				)
				(pin power_in line
					(at 0 -43.18 0)
					(length 2.54)
					(name "GND")
					(number "A2")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "VPGM")
					(number "A3")
				)
				(pin power_in line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "AVDD33")
					(number "B1")
				)
				(pin power_in line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "AVDD12")
					(number "B2")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "INT")
					(number "B3")
				)
				(pin power_in line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "AVDD25")
					(number "B5")
				)
				(pin power_in line
					(at 25.4 -43.18 180)
					(length 2.54)
					(name "VDDC2")
					(number "C3")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "C4")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "C5")
				)
				(pin power_in line
					(at 25.4 -30.48 180)
					(length 2.54)
					(name "VDD_MIPI")
					(number "C6")
				)
				(pin passive line
					(at 25.4 -22.86 180)
					(length 2.54)
					(hide yes)
					(name "AVDD12")
					(number "D3")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "D4")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "D5")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "D6")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "E3")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "E4")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "TEST")
					(number "E5")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "E6")
				)
				(pin passive line
					(at 25.4 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "AVDD33")
					(number "F3")
				)
				(pin power_in line
					(at 25.4 0 180)
					(length 2.54)
					(name "VDDIO1")
					(number "F4")
				)
				(pin passive line
					(at 25.4 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "VDDC2")
					(number "F5")
				)
				(pin passive line
					(at 25.4 -30.48 180)
					(length 2.54)
					(hide yes)
					(name "VDD_MIPI")
					(number "F6")
				)
				(pin power_in line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "VDDC1")
					(number "G2")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{RESET}")
					(number "G5")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "REFCLK")
					(number "H5")
				)
				(pin power_in line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "VDDIO2")
					(number "H7")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "H8")
				)
			)
			(symbol "TC358743XBG_3_1"
				(pin output line
					(at 0 -20.32 0)
					(length 2.54)
					(name "BIASDA")
					(number "A4")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 2.54)
					(name "DAOUT")
					(number "A5")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 2.54)
					(name "PFIL")
					(number "A6")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "PCKIN")
					(number "B6")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "A_SCK")
					(number "F7")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 2.54)
					(name "A_SD")
					(number "F8")
				)
				(pin output line
					(at 0 0 0)
					(length 2.54)
					(name "A_WFS")
					(number "G7")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 2.54)
					(name "A_OSCK")
					(number "G8")
				)
			)
			(embedded_fonts no)
		)
)
