(footprint "BGA-80_7x7mm_Layout10x10_P0.65mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -1.901 -4.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-80_7x7mm_Layout10x10_P0.65mm"
		(at 0 4.65 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -3.75 6.65 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -3.75 7.85 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.75 9.05 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -2.925 -2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "A2" smd circle
		(at -2.275 -2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "A3" smd circle
		(at -1.625 -2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "A4" smd circle
		(at -0.975 -2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "A5" smd circle
		(at -0.325 -2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "A6" smd circle
		(at 0.325 -2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "A7" smd circle
		(at 0.975 -2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "A8" smd circle
		(at 1.625 -2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "A9" smd circle
		(at 2.275 -2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "A10" smd circle
		(at 2.925 -2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "B1" smd circle
		(at -2.925 -2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "B2" smd circle
		(at -2.275 -2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "B3" smd circle
		(at -1.625 -2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "B4" smd circle
		(at -0.975 -2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "B5" smd circle
		(at -0.325 -2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "B6" smd circle
		(at 0.325 -2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "B7" smd circle
		(at 0.975 -2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "B8" smd circle
		(at 1.625 -2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "B9" smd circle
		(at 2.275 -2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "B10" smd circle
		(at 2.925 -2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "C1" smd circle
		(at -2.925 -1.625)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "C2" smd circle
		(at -2.275 -1.625)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "C9" smd circle
		(at 2.275 -1.625)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "C10" smd circle
		(at 2.925 -1.625)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "D1" smd circle
		(at -2.925 -0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "D2" smd circle
		(at -2.275 -0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "D4" smd circle
		(at -0.975 -0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "D5" smd circle
		(at -0.325 -0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "D6" smd circle
		(at 0.325 -0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "D7" smd circle
		(at 0.975 -0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "D9" smd circle
		(at 2.275 -0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "D10" smd circle
		(at 2.925 -0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "E1" smd circle
		(at -2.925 -0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "E2" smd circle
		(at -2.275 -0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "E4" smd circle
		(at -0.975 -0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "E5" smd circle
		(at -0.325 -0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "E6" smd circle
		(at 0.325 -0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "E7" smd circle
		(at 0.975 -0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "E9" smd circle
		(at 2.275 -0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "E10" smd circle
		(at 2.925 -0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "F1" smd circle
		(at -2.925 0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "F2" smd circle
		(at -2.275 0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "F4" smd circle
		(at -0.975 0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "F5" smd circle
		(at -0.325 0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "F6" smd circle
		(at 0.325 0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "F7" smd circle
		(at 0.975 0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "F9" smd circle
		(at 2.275 0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "F10" smd circle
		(at 2.925 0.325)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "G1" smd circle
		(at -2.925 0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "G2" smd circle
		(at -2.275 0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "G4" smd circle
		(at -0.975 0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "G5" smd circle
		(at -0.325 0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "G6" smd circle
		(at 0.325 0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "G7" smd circle
		(at 0.975 0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "G9" smd circle
		(at 2.275 0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "G10" smd circle
		(at 2.925 0.975)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "H1" smd circle
		(at -2.925 1.625)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "H2" smd circle
		(at -2.275 1.625)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "H9" smd circle
		(at 2.275 1.625)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "H10" smd circle
		(at 2.925 1.625)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "J1" smd circle
		(at -2.925 2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "J2" smd circle
		(at -2.275 2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "J3" smd circle
		(at -1.625 2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "J4" smd circle
		(at -0.975 2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "J5" smd circle
		(at -0.325 2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "J6" smd circle
		(at 0.325 2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "J7" smd circle
		(at 0.975 2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "J8" smd circle
		(at 1.625 2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "J9" smd circle
		(at 2.275 2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "J10" smd circle
		(at 2.925 2.275)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "K1" smd circle
		(at -2.925 2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "K2" smd circle
		(at -2.275 2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "K3" smd circle
		(at -1.625 2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "K4" smd circle
		(at -0.975 2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "K5" smd circle
		(at -0.325 2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "K6" smd circle
		(at 0.325 2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "K7" smd circle
		(at 0.975 2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "K8" smd circle
		(at 1.625 2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "K9" smd circle
		(at 2.275 2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(pad "K10" smd circle
		(at 2.925 2.925)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin -0.025)
		(solder_paste_margin -0.025)
	)
	(embedded_fonts no)
	(model "antmicro_tc358840xbg.glb"
		(offset
			(xyz 0 0 -0.03)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
