(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TC358840XBG"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 59.69 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TC358840XBG"
				(at 59.69 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TC358840XBG"
				(at 59.69 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://toshiba.semicon-storage.com/info/TC358840XBG_datasheet_en_20171024.pdf?did=28738&prodName=TC358840XBG"
				(at 59.69 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "CMOS Ultra HD to MIPI  CSI-2 80-Pin VFBGA"
				(at 59.69 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TC358840XBG"
				(at 59.69 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Toshiba"
				(at 59.69 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 59.69 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 59.69 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, CONTROLLER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TC358840XBG_1_1"
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "CEC")
					(number "A2")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "DDC_SCL")
					(number "A3")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "HPDI")
					(number "A4")
				)
				(pin passive line
					(at 40.64 -48.26 180)
					(length 3.81)
					(name "CDSI1D3P")
					(number "A5")
				)
				(pin passive line
					(at 40.64 -43.18 180)
					(length 3.81)
					(name "CDSI1D2P")
					(number "A6")
				)
				(pin passive line
					(at 40.64 -27.94 180)
					(length 3.81)
					(name "CDSI1CP")
					(number "A7")
				)
				(pin passive line
					(at 40.64 -38.1 180)
					(length 3.81)
					(name "CDSI1D1P")
					(number "A8")
				)
				(pin passive line
					(at 40.64 -33.02 180)
					(length 3.81)
					(name "CDSI1D0P")
					(number "A9")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "DDC_SDA")
					(number "B3")
				)
				(pin passive line
					(at 40.64 -55.88 180)
					(length 3.81)
					(name "HPDO")
					(number "B4")
				)
				(pin passive line
					(at 40.64 -50.8 180)
					(length 3.81)
					(name "CDSI1D3N")
					(number "B5")
				)
				(pin passive line
					(at 40.64 -45.72 180)
					(length 3.81)
					(name "CDSI1D2N")
					(number "B6")
				)
				(pin passive line
					(at 40.64 -30.48 180)
					(length 3.81)
					(name "CDSI1CN")
					(number "B7")
				)
				(pin passive line
					(at 40.64 -40.64 180)
					(length 3.81)
					(name "CDSI1D1N")
					(number "B8")
				)
				(pin passive line
					(at 40.64 -35.56 180)
					(length 3.81)
					(name "CDSI1D0N")
					(number "B9")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "HDMICP")
					(number "C1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "HDMICN")
					(number "C2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "HDMID0P")
					(number "D1")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "HDMID0N")
					(number "D2")
				)
				(pin passive line
					(at 40.64 -22.86 180)
					(length 3.81)
					(name "CDSI0D3N")
					(number "D9")
				)
				(pin passive line
					(at 40.64 -20.32 180)
					(length 3.81)
					(name "CDSI0D3P")
					(number "D10")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "HDMID1P")
					(number "E1")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "HDMID1N")
					(number "E2")
				)
				(pin passive line
					(at 40.64 -17.78 180)
					(length 3.81)
					(name "CDSI0D2N")
					(number "E9")
				)
				(pin passive line
					(at 40.64 -15.24 180)
					(length 3.81)
					(name "CDSI0D2P")
					(number "E10")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "HDMID2P")
					(number "F1")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "HDMID2N")
					(number "F2")
				)
				(pin passive line
					(at 40.64 -2.54 180)
					(length 3.81)
					(name "CDSI0CN")
					(number "F9")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 3.81)
					(name "CDSI0CP")
					(number "F10")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "IR")
					(number "G6")
				)
				(pin passive line
					(at 40.64 -12.7 180)
					(length 3.81)
					(name "CDSI0D1N")
					(number "G9")
				)
				(pin passive line
					(at 40.64 -10.16 180)
					(length 3.81)
					(name "CDSI0D1P")
					(number "G10")
				)
				(pin passive line
					(at 40.64 -7.62 180)
					(length 3.81)
					(name "CDSI0D0N")
					(number "H9")
				)
				(pin passive line
					(at 40.64 -5.08 180)
					(length 3.81)
					(name "CDSI0D0P")
					(number "H10")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "I2C_SDA")
					(number "K3")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "I2C_SCL")
					(number "K4")
				)
			)
			(symbol "TC358840XBG_2_1"
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "REXT")
					(number "A1")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 3.81)
					(name "GND")
					(number "A10")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDD33_HDMI")
					(number "B1")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDD11_HDMI")
					(number "B2")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 3.81)
					(name "VDD12_MIPI1")
					(number "B10")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C9")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 3.81)
					(name "VDDC11")
					(number "C10")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D4")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D5")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D6")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D7")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E4")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E6")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E7")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F4")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F5")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F6")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F7")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD33_HDMI")
					(number "G1")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "VDD11_HDMI")
					(number "G2")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G4")
				)
				(pin passive line
					(at 30.48 -2.54 180)
					(length 3.81)
					(name "TEST")
					(number "G5")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G7")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H1")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 3.81)
					(name "VDDIO33")
					(number "H2")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(name "INT")
					(number "J3")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 3.81)
					(name "VDDIO18")
					(number "J7")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 3.81)
					(name "VDD12_MIPI0")
					(number "J10")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "VDDC11")
					(number "K6")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "RESETN")
					(number "K8")
				)
				(pin passive line
					(at 30.48 -7.62 180)
					(length 3.81)
					(name "REFCLK")
					(number "K9")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K10")
				)
			)
			(symbol "TC358840XBG_3_1"
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "BIASDA")
					(number "J1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "DAOUT")
					(number "J2")
				)
				(pin passive line
					(at 33.02 -15.24 180)
					(length 3.81)
					(name "A_OSCK")
					(number "J4")
				)
				(pin passive line
					(at 33.02 -5.08 180)
					(length 3.81)
					(name "A_SD3")
					(number "J5")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(name "A_SD2")
					(number "J6")
				)
				(pin passive line
					(at 33.02 -10.16 180)
					(length 3.81)
					(name "A_SD1")
					(number "J8")
				)
				(pin passive line
					(at 33.02 -12.7 180)
					(length 3.81)
					(name "A_SD0")
					(number "J9")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PCKIN")
					(number "K1")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PFIL")
					(number "K2")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 3.81)
					(name "A_WFS")
					(number "K5")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(name "A_SCK")
					(number "K7")
				)
			)
			(embedded_fonts no)
		)
)
