(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TCA9534PWR_TSSOP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TCA9534PWR_TSSOP"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TCA9534PWR_TSSOP"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9534.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Low Voltage 8-Bit I2C and SMBUS Low-Power I/O Expander with Interrupt Output and Configuration Registers"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TCA9534PWR"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, I2C"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm* SOIC*7.5x10.3mm*P1.27mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TCA9534PWR_TSSOP_1_1"
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "A0")
					(number "1")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "A1")
					(number "2")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "A2")
					(number "3")
				)
				(pin bidirectional line
					(at 17.78 0 180)
					(length 2.54)
					(name "P0")
					(number "4")
				)
				(pin bidirectional line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "P1")
					(number "5")
				)
				(pin bidirectional line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "P2")
					(number "6")
				)
				(pin bidirectional line
					(at 17.78 -7.62 180)
					(length 2.54)
					(name "P3")
					(number "7")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin bidirectional line
					(at 17.78 -10.16 180)
					(length 2.54)
					(name "P4")
					(number "9")
				)
				(pin bidirectional line
					(at 17.78 -12.7 180)
					(length 2.54)
					(name "P5")
					(number "10")
				)
				(pin bidirectional line
					(at 17.78 -15.24 180)
					(length 2.54)
					(name "P6")
					(number "11")
				)
				(pin bidirectional line
					(at 17.78 -17.78 180)
					(length 2.54)
					(name "P7")
					(number "12")
				)
				(pin open_collector line
					(at 0 -8.89 0)
					(length 2.54)
					(name "~{INT}")
					(number "13")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SCL")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 2.54)
					(name "SDA")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
