(footprint "BGA-392-169_12x16mm_Layout14x28_P0.5mm_H1.1mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -8.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-392-169_12x16mm_Layout14x28_P0.5mm_H1.1mm"
		(at -6.45 9.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -6.4 10.55 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -6.4 11.75 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -6.4 12.85 0)
		(layer "F.Fab")
	)
	(pad "A4" smd circle
		(at -1.75 -6.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at -0.75 -6.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at 0.75 -6.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd circle
		(at 1.75 -6.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA1" smd circle
		(at -3.25 3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA2" smd circle
		(at -2.75 3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA3" smd circle
		(at -2.25 3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA4" smd circle
		(at -1.75 3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA5" smd circle
		(at -1.25 3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA6" smd circle
		(at -0.75 3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA7" smd circle
		(at -0.25 3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA8" smd circle
		(at 0.25 3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA9" smd circle
		(at 0.75 3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA10" smd circle
		(at 1.25 3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA11" smd circle
		(at 1.75 3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA12" smd circle
		(at 2.25 3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA13" smd circle
		(at 2.75 3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA14" smd circle
		(at 3.25 3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE1" smd circle
		(at -3.25 5.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE14" smd circle
		(at 3.25 5.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG2" smd circle
		(at -2.75 6.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG13" smd circle
		(at 2.75 6.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH4" smd circle
		(at -1.75 6.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH6" smd circle
		(at -0.75 6.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH9" smd circle
		(at 0.75 6.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH11" smd circle
		(at 1.75 6.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -2.75 -6.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B13" smd circle
		(at 2.75 -6.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -3.25 -5.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D14" smd circle
		(at 3.25 -5.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -3.25 -3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -2.75 -3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -2.25 -3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -1.75 -3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H5" smd circle
		(at -1.25 -3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H6" smd circle
		(at -0.75 -3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H7" smd circle
		(at -0.25 -3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H8" smd circle
		(at 0.25 -3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at 0.75 -3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H10" smd circle
		(at 1.25 -3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H11" smd circle
		(at 1.75 -3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H12" smd circle
		(at 2.25 -3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H13" smd circle
		(at 2.75 -3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H14" smd circle
		(at 3.25 -3.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -3.25 -2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -2.75 -2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at -2.25 -2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at -1.75 -2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J5" smd circle
		(at -1.25 -2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J6" smd circle
		(at -0.75 -2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J7" smd circle
		(at -0.25 -2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J8" smd circle
		(at 0.25 -2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J9" smd circle
		(at 0.75 -2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J10" smd circle
		(at 1.25 -2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J11" smd circle
		(at 1.75 -2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J12" smd circle
		(at 2.25 -2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J13" smd circle
		(at 2.75 -2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J14" smd circle
		(at 3.25 -2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K1" smd circle
		(at -3.25 -2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -2.75 -2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at -2.25 -2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K4" smd circle
		(at -1.75 -2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K5" smd circle
		(at -1.25 -2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K6" smd circle
		(at -0.75 -2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K7" smd circle
		(at -0.25 -2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K8" smd circle
		(at 0.25 -2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K9" smd circle
		(at 0.75 -2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K10" smd circle
		(at 1.25 -2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K11" smd circle
		(at 1.75 -2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K12" smd circle
		(at 2.25 -2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K13" smd circle
		(at 2.75 -2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K14" smd circle
		(at 3.25 -2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L1" smd circle
		(at -3.25 -1.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L2" smd circle
		(at -2.75 -1.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L3" smd circle
		(at -2.25 -1.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L4" smd circle
		(at -1.75 -1.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L12" smd circle
		(at 2.25 -1.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L13" smd circle
		(at 2.75 -1.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L14" smd circle
		(at 3.25 -1.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M1" smd circle
		(at -3.25 -1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M2" smd circle
		(at -2.75 -1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M3" smd circle
		(at -2.25 -1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M5" smd circle
		(at -1.25 -1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M6" smd circle
		(at -0.75 -1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M7" smd circle
		(at -0.25 -1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M8" smd circle
		(at 0.25 -1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M9" smd circle
		(at 0.75 -1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M10" smd circle
		(at 1.25 -1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M12" smd circle
		(at 2.25 -1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M13" smd circle
		(at 2.75 -1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M14" smd circle
		(at 3.25 -1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N1" smd circle
		(at -3.25 -0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N2" smd circle
		(at -2.75 -0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N3" smd circle
		(at -2.25 -0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N5" smd circle
		(at -1.25 -0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N10" smd circle
		(at 1.25 -0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N12" smd circle
		(at 2.25 -0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N13" smd circle
		(at 2.75 -0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N14" smd circle
		(at 3.25 -0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P1" smd circle
		(at -3.25 -0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P2" smd circle
		(at -2.75 -0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P3" smd circle
		(at -2.25 -0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P5" smd circle
		(at -1.25 -0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P10" smd circle
		(at 1.25 -0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P12" smd circle
		(at 2.25 -0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P13" smd circle
		(at 2.75 -0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P14" smd circle
		(at 3.25 -0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R1" smd circle
		(at -3.25 0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R2" smd circle
		(at -2.75 0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R3" smd circle
		(at -2.25 0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R5" smd circle
		(at -1.25 0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R10" smd circle
		(at 1.25 0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R12" smd circle
		(at 2.25 0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R13" smd circle
		(at 2.75 0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R14" smd circle
		(at 3.25 0.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T1" smd circle
		(at -3.25 0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T2" smd circle
		(at -2.75 0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T3" smd circle
		(at -2.25 0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T5" smd circle
		(at -1.25 0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T10" smd circle
		(at 1.25 0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T12" smd circle
		(at 2.25 0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T13" smd circle
		(at 2.75 0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T14" smd circle
		(at 3.25 0.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U1" smd circle
		(at -3.25 1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U2" smd circle
		(at -2.75 1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U3" smd circle
		(at -2.25 1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U5" smd circle
		(at -1.25 1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U6" smd circle
		(at -0.75 1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U7" smd circle
		(at -0.25 1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U8" smd circle
		(at 0.25 1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U9" smd circle
		(at 0.75 1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U10" smd circle
		(at 1.25 1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U12" smd circle
		(at 2.25 1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U13" smd circle
		(at 2.75 1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U14" smd circle
		(at 3.25 1.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V1" smd circle
		(at -3.25 1.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V2" smd circle
		(at -2.75 1.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V3" smd circle
		(at -2.25 1.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V12" smd circle
		(at 2.25 1.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V13" smd circle
		(at 2.75 1.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V14" smd circle
		(at 3.25 1.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W1" smd circle
		(at -3.25 2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W2" smd circle
		(at -2.75 2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W3" smd circle
		(at -2.25 2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W4" smd circle
		(at -1.75 2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W5" smd circle
		(at -1.25 2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W6" smd circle
		(at -0.75 2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W7" smd circle
		(at -0.25 2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W8" smd circle
		(at 0.25 2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W9" smd circle
		(at 0.75 2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W10" smd circle
		(at 1.25 2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W11" smd circle
		(at 1.75 2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W12" smd circle
		(at 2.25 2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W13" smd circle
		(at 2.75 2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W14" smd circle
		(at 3.25 2.25)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y1" smd circle
		(at -3.25 2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y2" smd circle
		(at -2.75 2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y3" smd circle
		(at -2.25 2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y4" smd circle
		(at -1.75 2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y5" smd circle
		(at -1.25 2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y6" smd circle
		(at -0.75 2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y7" smd circle
		(at -0.25 2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y8" smd circle
		(at 0.25 2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y9" smd circle
		(at 0.75 2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y10" smd circle
		(at 1.25 2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y11" smd circle
		(at 1.75 2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y12" smd circle
		(at 2.25 2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y13" smd circle
		(at 2.75 2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y14" smd circle
		(at 3.25 2.75)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_thgbm2g6d2fbai9.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
