(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "THGBM2G6D2FBAI9"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "THGBM2G6D2FBAI9"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "THGBM2G6D2FBAI9"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://datasheet.ciiva.com/9276/5975e-9276317.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "eMMC 8GB 15nm"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "THGBM2G6D2FBAI9"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Toshiba Memory"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MEMORY, BGA"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "THGBM2G6D2FBAI9_1_1"
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A4")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A6")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A9")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A11")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AA1")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AA2")
				)
				(pin power_in line
					(at 24.13 -2.54 180)
					(length 3.81)
					(name "VCCQ")
					(number "AA3")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 3.81)
					(name "VSSQ")
					(number "AA4")
				)
				(pin passive line
					(at 24.13 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "VCCQ")
					(number "AA5")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "VSSQ")
					(number "AA6")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "AA7")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AA8")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AA9")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "AA10")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AA11")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AA12")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AA13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AA14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AE1")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AE14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AG2")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AG13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AH4")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AH6")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AH9")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "AH11")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B2")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "D1")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "D14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H1")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H2")
				)
				(pin bidirectional line
					(at 24.13 -10.16 180)
					(length 3.81)
					(name "DAT0")
					(number "H3")
				)
				(pin bidirectional line
					(at 24.13 -12.7 180)
					(length 3.81)
					(name "DAT1")
					(number "H4")
				)
				(pin bidirectional line
					(at 24.13 -15.24 180)
					(length 3.81)
					(name "DAT2")
					(number "H5")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "H6")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "H7")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H8")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H9")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H10")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H11")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H12")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J1")
				)
				(pin bidirectional line
					(at 24.13 -17.78 180)
					(length 3.81)
					(name "DAT3")
					(number "J2")
				)
				(pin bidirectional line
					(at 24.13 -20.32 180)
					(length 3.81)
					(name "DAT4")
					(number "J3")
				)
				(pin bidirectional line
					(at 24.13 -22.86 180)
					(length 3.81)
					(name "DAT5")
					(number "J4")
				)
				(pin bidirectional line
					(at 24.13 -25.4 180)
					(length 3.81)
					(name "DAT6")
					(number "J5")
				)
				(pin bidirectional line
					(at 24.13 -27.94 180)
					(length 3.81)
					(name "DAT7")
					(number "J6")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J7")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J8")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J9")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J10")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J11")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J12")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K1")
				)
				(pin power_in line
					(at 24.13 -5.08 180)
					(length 3.81)
					(name "VDDI")
					(number "K2")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K3")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "VSSQ")
					(number "K4")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "K5")
				)
				(pin passive line
					(at 24.13 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "VCCQ")
					(number "K6")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K7")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K8")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K9")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K10")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K11")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K12")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L1")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L2")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L3")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L4")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L12")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M1")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M2")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M3")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "M5")
				)
				(pin power_in line
					(at 24.13 0 180)
					(length 3.81)
					(name "VCC")
					(number "M6")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 3.81)
					(name "VSS")
					(number "M7")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "M8")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "M9")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "M10")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M12")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N1")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N2")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N3")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "N5")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "N10")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N12")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "P1")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "P2")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "P3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "P5")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "P10")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "P12")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "P13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "P14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R1")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R2")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R3")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "R5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "R10")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R12")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "R14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T1")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T2")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T3")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "T5")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "T10")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T12")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "T14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "U1")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "U2")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "U3")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "~{RST}")
					(number "U5")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "U6")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "U7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "U8")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "U9")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "U10")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "U12")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "U13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "U14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "V1")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "V2")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "V3")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "V12")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "V13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "V14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "W1")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "W2")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "W3")
				)
				(pin passive line
					(at 24.13 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "VCCQ")
					(number "W4")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "CMD")
					(number "W5")
				)
				(pin input clock
					(at 0 -2.54 0)
					(length 3.81)
					(name "CLK")
					(number "W6")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "W7")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "W8")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "W9")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "W10")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "W11")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "W12")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "W13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "W14")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "Y1")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "VSSQ")
					(number "Y2")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "Y3")
				)
				(pin passive line
					(at 24.13 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "VCCQ")
					(number "Y4")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "VSSQ")
					(number "Y5")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "Y6")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "Y7")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "Y8")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "Y9")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "Y10")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "Y11")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "Y12")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "Y13")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "Y14")
				)
			)
			(embedded_fonts no)
		)
)
