(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "THVD2452VDREP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "THVD2452VDREP"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "THVD2452VDREP"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/thvd2452v-ep.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Enhanced RS-485 transceiver, 20Mbps and 50Mbps Differential, 3.3V to 5V, 14-Pin SOIC"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "THVD2452VDREP"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, DRIVER, TRANSCEIVER, No-RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "THVD2452VDREP_1_1"
				(pin output line
					(at 0 -3.81 0)
					(length 2.54)
					(name "R")
					(number "2")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "~{RE}")
					(number "3")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DE")
					(number "4")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "D")
					(number "5")
				)
				(pin power_in line
					(at 0 -16.51 0)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin no_connect line
					(at 17.78 0 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "SLR")
					(number "8")
				)
				(pin output line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "Y")
					(number "9")
				)
				(pin output line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "Z")
					(number "10")
				)
				(pin input line
					(at 20.32 -3.81 180)
					(length 2.54)
					(name "B")
					(number "11")
				)
				(pin input line
					(at 20.32 -6.35 180)
					(length 2.54)
					(name "A")
					(number "12")
				)
				(pin no_connect line
					(at 17.78 0 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{CC}")
					(number "14")
				)
			)
			(embedded_fonts no)
		)
)
