(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS2372-3RGWR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS2372-3RGWR"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS2372-3RGWR"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2372.pdf?ts=1679042478513&ref_url=https%253A%252F%252Fwww.google.com%252F"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "PoE interface"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS2372-3RGWR"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, POE, IC, INTERFACE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS2372-3RGWR_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "DEN")
					(number "2")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "CLSA")
					(number "3")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VSSA")
					(number "4")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VSSB")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "CLSB")
					(number "6")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "REF")
					(number "7")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "AMPS_CTL")
					(number "8")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "MPS_DUTY")
					(number "9")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "~{AUTCLS}")
					(number "10")
				)
				(pin power_out line
					(at 21.59 -30.48 180)
					(length 2.54)
					(name "RTNA")
					(number "11")
				)
				(pin power_out line
					(at 21.59 -33.02 180)
					(length 2.54)
					(name "RTNB")
					(number "12")
				)
				(pin output line
					(at 21.59 -20.32 180)
					(length 2.54)
					(name "PG")
					(number "13")
				)
				(pin no_connect line
					(at 19.05 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "14")
				)
				(pin no_connect line
					(at 19.05 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "15")
				)
				(pin output line
					(at 21.59 -25.4 180)
					(length 2.54)
					(name "IRSHDL_EN")
					(number "16")
				)
				(pin output line
					(at 21.59 -2.54 180)
					(length 2.54)
					(name "TPL")
					(number "17")
				)
				(pin output line
					(at 21.59 0 180)
					(length 2.54)
					(name "TPH")
					(number "18")
				)
				(pin output line
					(at 21.59 -5.08 180)
					(length 2.54)
					(name "~{BT}")
					(number "19")
				)
				(pin no_connect line
					(at 19.05 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "20")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "PAD_VSSC")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
