(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS2378DDA"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS2378DDA"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS2378DDA"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2378.pdf"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Power Over Ethernet (POE) Controller, 57 V/ 500 µA, 40 V UVLO Threshold, SOIC-8"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS2378DDA"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, POE, IC, INTERFACE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS2378DDA_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "DEN")
					(number "2")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(name "CLS")
					(number "3")
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 2.54)
					(name "VSS")
					(number "4")
				)
				(pin passive line
					(at 20.32 -13.97 180)
					(length 2.54)
					(name "RTN")
					(number "5")
				)
				(pin passive line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "CDB")
					(number "6")
				)
				(pin passive line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "T2P")
					(number "7")
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(name "APD")
					(number "8")
				)
				(pin power_in line
					(at 0 -13.97 0)
					(length 2.54)
					(name "EP")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
