(footprint "WSON-10-1EP_2.5x2.5mm_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "https://www.ti.com/lit/ds/symlink/tps38-q1.pdf?ts=1768310866404")
	(property "Reference" "REF**"
		(at -1.55 -1.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "WSON-10-1EP_2.5x2.5mm_P0.5mm"
		(at -1.55 2.45 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -1.55 3.65 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -1.55 4.85 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.55 6.05 0)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.5")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.9")
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 1 1.79)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(zone_connect 0)
	)
	(pad "1" smd rect
		(at -1.15 -1)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.15 -0.5)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.15 0)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.15 0.495)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.15 0.995)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.15 0.995)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.15 0.495)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.15 0)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.15 -0.5)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.15 -1)
		(size 0.6 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0 0)
		(size 1.2 2)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
	)
	(embedded_fonts no)
	(model "antmicro_tps38j010155dskrq1.glb"
		(offset
			(xyz -0 -0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
