(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TRSF3232EIDR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TRSF3232EIDR"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TRSF3232EIDR"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/trsf3232e.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RS-232 Interface IC 3V-5.5V 2Ch RS-232 1 Mbit Line Drvr/Rcvr"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TRSF3232EIDR"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, DRIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TRSF3232EIDR_1_1"
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "C1+")
					(number "1")
				)
				(pin output line
					(at 21.59 -20.32 180)
					(length 2.54)
					(name "V+")
					(number "2")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "C1-")
					(number "3")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "C2+")
					(number "4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "C2-")
					(number "5")
				)
				(pin output line
					(at 21.59 -22.86 180)
					(length 2.54)
					(name "V-")
					(number "6")
				)
				(pin output line
					(at 21.59 -7.62 180)
					(length 2.54)
					(name "DOUT2")
					(number "7")
				)
				(pin input line
					(at 21.59 -15.24 180)
					(length 2.54)
					(name "RIN2")
					(number "8")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 2.54)
					(name "ROUT2")
					(number "9")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DIN2")
					(number "10")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DIN1")
					(number "11")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 2.54)
					(name "ROUT1")
					(number "12")
				)
				(pin input line
					(at 21.59 -12.7 180)
					(length 2.54)
					(name "RIN1")
					(number "13")
				)
				(pin output line
					(at 21.59 -5.08 180)
					(length 2.54)
					(name "DOUT1")
					(number "14")
				)
				(pin power_in line
					(at 21.59 -30.48 180)
					(length 2.54)
					(name "GND")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
