(footprint "UQFN-12_2x1.7mm_P0.4mm_Texas_RUT"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Texas_R_PUQFN-N12")
	(tags "Texas_R_PUQFN-N12")
	(property "Reference" "REF**"
		(at 0 -1.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "UQFN-12_2x1.7mm_P0.4mm_Texas_RUT"
		(at 0 2.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -1.1 4.35 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -1.1 5.55 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.1 6.75 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.653 -0.803 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at -0.425 -0.975)
		(size 0.15 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.653 -0.403 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.653 0 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.653 0.4 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -0.653 0.8 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0 0.8 270)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0.65 0.8 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.65 0.4 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0.65 0 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 0.65 -0.403 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0.65 -0.803 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 0 -0.803 270)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_txb0104rutr.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
