(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TXS02612RTWR_QFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TXS02612RTWR_QFN"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TXS02612RTWR_QFN"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/txs02612.pdf?HQS=dis-mous-null-mousermode-dsf-pf-null-wwe&ts=1651653695097&ref_url=https%253A%252F%252Fwww.mouser.com%252F"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "SDIO port expander with voltage-level translation, WQFN-24"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TXS02612RTWR"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TXS02612RTWR_QFN_1_1"
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DAT2A")
					(number "1")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "DAT3A")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "CMDA")
					(number "4")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCCA")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DAT0A")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DAT1A")
					(number "7")
				)
				(pin bidirectional line
					(at 30.48 -35.56 180)
					(length 2.54)
					(name "DAT2B1")
					(number "8")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "CLKA")
					(number "9")
				)
				(pin bidirectional line
					(at 30.48 -38.1 180)
					(length 2.54)
					(name "DAT3B1")
					(number "10")
				)
				(pin power_in line
					(at 0 -45.72 0)
					(length 2.54)
					(name "GND")
					(number "11")
				)
				(pin bidirectional line
					(at 30.48 -43.18 180)
					(length 2.54)
					(name "CMDB1")
					(number "12")
				)
				(pin output line
					(at 30.48 -45.72 180)
					(length 2.54)
					(name "CLKB1")
					(number "13")
				)
				(pin bidirectional line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "DAT0B1")
					(number "14")
				)
				(pin bidirectional line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "DAT1B1")
					(number "15")
				)
				(pin bidirectional line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "DAT1B0")
					(number "16")
				)
				(pin power_in line
					(at 30.48 -25.4 180)
					(length 2.54)
					(name "VCCB1")
					(number "17")
				)
				(pin bidirectional line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "DAT0B0")
					(number "18")
				)
				(pin output line
					(at 30.48 -20.32 180)
					(length 2.54)
					(name "CLKB0")
					(number "19")
				)
				(pin bidirectional line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "CMDB0")
					(number "20")
				)
				(pin power_in line
					(at 30.48 0 180)
					(length 2.54)
					(name "VCCB0")
					(number "21")
				)
				(pin bidirectional line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "DAT3B0")
					(number "22")
				)
				(pin bidirectional line
					(at 30.48 -10.16 180)
					(length 2.54)
					(name "DAT2B0")
					(number "23")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "SEL")
					(number "24")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "EP")
					(number "25")
				)
			)
			(embedded_fonts no)
		)
)
